DB_ENV->rep_stat()
Prev | Chapter 10. Replication Methods | Next

## DB_ENV->rep_stat()

    #include <db.h>

    int
    DB_ENV->rep_stat(DB_ENV *env, DB_REP_STAT **statp, u_int32_t flags);

The `DB_ENV->rep_stat()` method returns the replication subsystem statistics.

The `DB_ENV->rep_stat()` method creates a statistical structure of type `DB_REP_STAT` and copies a pointer to it into a user-specified memory location.

Statistical structures are stored in allocated memory. If application-specific allocation routines have been declared (see DB_ENV->set_alloc() for more information), they are used to allocate the memory; otherwise, the standard C library malloc(3) is used. The caller is responsible for deallocating the memory. To deallocate the memory, free the memory reference; references inside the returned memory need not be individually freed.

The following `DB_REP_STAT` fields will be filled in:

- uintmax_t st_bulk_fills;

  The number of times the bulk buffer filled up, forcing the buffer content to be sent.

- uintmax_t st_bulk_overflows;

  The number of times a record was bigger than the entire bulk buffer, and therefore had to be sent as a singleton.

- uintmax_t st_bulk_records;

  The number of records added to a bulk buffer.

- uintmax_t st_bulk_transfers;

  The number of bulk buffers transferred (via a call to the application's send function).

- uintmax_t st_client_rerequests;

  The number of times this client site received a "re-request" message, indicating that a request it previously sent to another client could not be serviced by that client. (Compare to st_client_svc_miss.)

- uintmax_t st_client_svc_miss;

  The number of "request" type messages received by this client that could not be processed, forcing the originating requester to try sending the request to the master (or another client).

- uintmax_t st_client_svc_req;

  The number of "request" type messages received by this client. ("Request" messages are usually sent from a client to the master, but a message marked with the DB_REP_ANYWHERE flag in the invocation of the application's send function may be sent to another client instead.)

- u_int32_t st_dupmasters;

  The number of duplicate master conditions originally detected at this site.

- u_int32_t st_egen;

  The election generation number for the current or next election.

- int st_election_cur_winner;

  The environment ID of the winner of the current or last election.

- u_int32_t st_election_gen;

  The master generation number of the winner of the current or last election.

- DB_LSN st_election_lsn;

  The maximum LSN of the winner of the current or last election.

- u_int32_t st_election_nsites;

  The number of sites responding to this site during the current election.

- u_int32_t st_election_nvotes;

  The number of votes required in the current or last election.

- u_int32_t st_election_priority;

  The priority of the winner of the current or last election.

- u_int32_t st_election_sec;

  The number of seconds the last election took (the total election time is st_election_sec plus st_election_usec).

- int st_election_status;

  The current election phase (0 if no election is in progress).

- u_int32_t st_election_tiebreaker;

  The tiebreaker value of the winner of the current or last election.

- u_int32_t st_election_usec;

  The number of microseconds the last election took (the total election time is st_election_sec plus st_election_usec).

- u_int32_t st_election_votes;

  The number of votes received during the current election.

- uintmax_t st_elections;

  The number of elections held.

- uintmax_t st_elections_won;

  The number of elections won.

- int st_env_id;

  The current environment ID.

- u_int32_t st_env_priority;

  The current environment priority.

- u_int32_t st_gen;

  The current master generation number.

- uintmax_t st_log_duplicated;

  The number of duplicate log records received.

- uintmax_t st_log_queued;

  The number of log records currently queued.

- uintmax_t st_log_queued_max;

  The maximum number of log records ever queued at once.

- uintmax_t st_log_queued_total;

  The total number of log records queued.

- uintmax_t st_log_records;

  The number of log records received and appended to the log.

- uintmax_t st_log_requested;

  The number of times log records were missed and requested.

- int st_master;

  The current master environment ID.

- uintmax_t st_master_changes;

  The number of times the master has changed.

- u_int32_t st_max_lease_sec;

  The number of seconds of the longest lease (the total lease time is st_max_lease_sec plus st_max_lease_usec).

- u_int32_t st_max_lease_usec;

  The number of microseconds of the longest lease (the total lease time is st_max_lease_sec plus st_max_lease_usec).

- DB_LSN st_max_perm_lsn;

  The LSN of the maximum permanent log record, or 0 if there are no permanent log records.

- uintmax_t st_msgs_badgen;

  The number of messages received with a bad generation number.

- uintmax_t st_msgs_processed;

  The number of messages received and processed.

- uintmax_t st_msgs_recover;

  The number of messages ignored due to pending recovery.

- uintmax_t st_msgs_send_failures;

  The number of failed message sends.

- uintmax_t st_msgs_sent;

  The number of messages sent.

- uintmax_t st_newsites;

  The number of new site messages received.

- DB_LSN st_next_lsn;

  In replication environments configured as masters, the next LSN to be used. In replication environments configured as clients, the next LSN expected.

- u_int32_t st_next_pg;

  The next page number we expect to receive.

- u_int32_t st_nsites;

  The number of sites used in the last election.

- uintmax_t st_nthrottles;

  Transmission limited. This indicates the number of times that data transmission was stopped to limit the amount of data sent in response to a single call to DB_ENV->rep_process_message().

- uintmax_t st_outdated;

  The number of outdated conditions detected.

- uintmax_t st_pg_duplicated;

  The number of duplicate pages received.

- uintmax_t st_pg_records;

  The number of pages received and stored.

- uintmax_t st_pg_requested;

  The number of pages missed and requested from the master.

- uintmax_t st_startsync_delayed;

  The number of times the client had to delay the start of a cache flush operation (initiated by the master for an impending checkpoint) because it was missing some previous log record(s).

- u_int32_t st_startup_complete;

  The client site has completed its startup procedures and is now handling live records from the master.

- u_int32_t st_status;

  The current replication mode. Set to DB_REP_MASTER if the environment is a replication master, DB_REP_CLIENT if the environment is a replication client, or 0 if replication is not configured.

- uintmax_t st_txns_applied;

  The number of transactions applied.

- DB_LSN st_waiting_lsn;

  The LSN of the first log record we have after missing log records being waited for, or 0 if no log records are currently missing.

- u_int32_t st_waiting_pg;

  The page number of the first page we have after missing pages being waited for, or 0 if no pages are currently missing.

The `DB_ENV->rep_stat()` method may not be called before the DB_ENV->open() method is called.

The `DB_ENV->rep_stat()` method returns a non-zero error value on failure and 0 on success.

### Parameters

#### flags

The flags parameter must be set to 0 or the following value:

- `DB_STAT_CLEAR`

  Reset statistics after returning their values.

#### statp

The statp parameter references memory into which a pointer to the allocated statistics structure is copied.

### Errors

The `DB_ENV->rep_stat()` method may fail and return one of the following non-zero errors:

#### EINVAL

If the database environment was not already opened; or if an invalid flag value or parameter was specified.

### Class

DB_ENV

### See Also

Replication and Related Methods

Prev | Up | Next
DB_ENV->rep_start() | Home | DB_ENV->rep_stat_print()