Oracle8 Error Messages Release 8.0.4 A58312-01 |
Library | Product | Contents | Index

## Video Pump Messages

##### OVS-00506: [str] read not complete in time

Cause: Disk reads may not complete in time when your volume is overloaded or a stream is in ff/rw mode some disk is dead.

Action: Verify all disks in your volume are healthy and make sure you have configured a volume that is big enough to support all your concurrent streams.

##### OVS-00511: [str] bad end position=str, start position=str, movie length=str

Cause: The stream service asked the pump to play from past the end of a file.

Action: Verify the file being played and its tag file are valid and up to date.

##### OVS-00512: [str] Downstream device str was never opened

Cause: The pump was asked to write to a downstream device that was not previously opened. The device can either be opened at initialization time via command line arguments or at run time via an RPC call from the upstream manager.

Action: Verify that either your DSM specifier command line argument is correct or that that upstream manager has been configured with network provisioning turned on.

##### OVS-00516: hostname 'str' is unknown

Cause: The hostname given in the DSM specifier on the vpump command line is unknown by the system.

Action: Check that the hostname is listed in /etc/hosts or use the IP address directly in the DSM specifier.

##### OVS-00517: cannot create socket: str

Cause: An error occurred in the operating system UDP/IP library.

Action: Verify UDP is alive and working on your server.

##### OVS-00518: cannot set socket options: str

Cause: An error occurred in the operating system UDP/IP library.

Action: Verify UDP is alive and working on your server.

##### OVS-00520: [str] cannot open DSM device str: str

Cause: The video pump can not open the downstream device.

Action: Verify the down stream device is functioning properly.

##### OVS-00521: ATM device str error: str

Cause: The video pump can not open the downstream device.

Action: Verify the down stream device is functioning properly.

##### OVS-00523: [str] cannot send data to DSM device str: str: [hex]

Cause: The video pump can not send data to the downstream device.

Action: Verify the down stream device is functioning properly.

##### OVS-00524: cannot send data to DSM device str: str - str: [hex]

Cause: The video pump can not send data to the downstream device.

Action: Verify the down stream device is functioning properly.

##### OVS-00525: cannot create RPC server handle: str

Cause: Media net was unable to create an RPC service.

Action: This is an internal error. Contact customer support.

##### OVS-00526: cannot register video pump as RPC server: str

Cause: Media net was unable to register an RPC service.

Action: Verify media net and, in particular, the name service are ok.

##### OVS-00538: cannot create dump file 'str'

Cause: MDS was unable to create the raw dump file.

Action: Verify the raw dump file name specified on the command line is a valid MDS file name. Make sure MDS is up and running.

##### OVS-00543: cannot add DSM to connection service: str

Cause: Communication with the connection service failed.

Action: Verify the connection service is up.

##### OVS-00545: [str] unrecognized stream service RPC call num

Cause: The stream service issued an unrecognized command to the pump.

Action: This is an internal error. Contact customer support.

##### OVS-00546: cannot find connection service: str

Cause: The lookup operation on the connection service failed.

Action: Verify the connection service is up.

##### OVS-00548: [str] cannot connect to DSM device str: str

Cause: The video pump can not connect to the downstream device.

Action: Verify the down stream device is functioning properly.

##### OVS-00549: [str] cannot close DSM device str: str

Cause: The video pump can not close the downstream device.

Action: Verify the down stream device is functioning properly.

##### OVS-00556: [str] open of 'str' not complete on time

Cause: A file could not be opened in a reasonable amount of time.

Action: Make sure MDS is up and functioning properly.

##### OVS-00557: [str] priming of 'str' not complete on time

Cause: The initial reads of a file to prime the internal cache did not complete in a reasonable amount of time.

Action: Make sure MDS is up and functioning properly.

##### OVS-00558: [str] dsm open not complete on time

Cause: The video pump can not open the downstream device.

Action: Verify the down stream device is functioning properly.

##### OVS-00561: mds failed to initialize

Cause: The video pump can not initialize MDS.

Action: Make sure MDS is up and functioning properly.

##### OVS-00562: [str] stop RPC called when not initialized

Cause: A spurious stop RPC was received.

Action: This is somewhat unusual but not harmful, no action needed.

##### OVS-00563: [str] initialize RPC called twice in a row

Cause: A spurious initialize RPC was received.

Action: This is somewhat unusual but not harmful, no action needed.

##### OVS-00564: [str] initialize RPC failed

Cause: Media net was unable process the RPC call.

Action: This is an internal error. Contact customer support.

##### OVS-00565: [str] bad file data at position str: no mpeg2 header found

Cause: The video pump could not make sense out of data in the file.

Action: Verify the file in question is valid.

##### OVS-00569: [str] mpeg misaligned in str at str out of str

Cause: During ff/rw, invalid file data was seen.

Action: Verify that the playing file is valid.

##### OVS-00570: [str] bad ff/rw vectors, invalid start position

Cause: During ff/rw, invalid file data was seen.

Action: Verify that the playing file is valid.

##### OVS-00571: [str] bad ff/rw vectors, I/O buffers misaligned

Cause: During ff/rw, invalid file data was seen.

Action: Verify that the playing file is valid.

##### OVS-00572: [str] stream service play RPC received before initialized

Cause: The stream service is issuing invalid RPC calls to the video pump.

Action: This is an internal error. Contact customer support.

##### OVS-00573: no output buffer size specified via -n

Cause: The video pump was not started with a valid buffer size argument.

Action: Examine the video pump's usage statement and add the correct argument to the command line.

##### OVS-00574: DSM buffer size=num not a multiple of packet size=num

Cause: The video pump was not started with a valid buffer size argument.

Action: The output buffer size must be a multiple of the format packet size.

##### OVS-00577: [str] bad file data at position str: no mpeg2 header found while muxing

Cause: The video pump could not make sense out of data in the file.

Action: Verify the file in question is valid.

##### OVS-00601: comm buffer memory exhausted: message dropped

Cause: The video pump ran out of communication buffer space.

Action: Verify you have enough memory to run all your streams.

Prev | Top | Next
| Copyright © 1997 Oracle Corporation. All Rights Reserved. |
Library | Product | Contents | Index