Corporate Info | News | Solutions | Products | Partners | Services | Events | Download | How To Buy
eLink Adapter for R/3 ALE Doc Home | eLink Adapter for R/3 ALE User's Guide | Previous Topic | Next Topic | Contents | Index

TUXEDO Initialization File

BEA eLink Adapter for R/3 ALE requires some configuration of the TUXEDO initialization file. For configuration instructions, see the BEA TUXEDO Administrator's Guide for your platform.

BEA eLink Adapter for R/3 ALE provides a semi-configured TUXEDO initialization file, cr3_ale.ubb , in the config sub-directory of the BEA eLink Adapter for R/3 ALE installation directory. This cr3_ale.ubb file is configured for the BEA eLink Adapter for R/3 ALE servers and it requires further configuration for integration into the global TUXEDO environment. For example, in the GROUPS section of your UBB file, you must define the server group to which the ALE eLink to R/3 belongs, such as CR3. See Appendix A, "Sample cr3_ale.ubb File," for a listing of this file.

Note: ALE eLink to R/3 and ALE R/3 to eLink use TUXEDO transactions. For these components, you need to create a transaction log (TLOG) using TUXEDO administrative tools. See the BEA TUXEDO Administrator's Guide for your platform.

Copyright © 2000 BEA Systems, Inc. All rights reserved. Required browser: Netscape 4.0 or higher, or Microsoft Internet Explorer 4.0 or higher.