## Machine Properties (Network)

You get the Network Machine Properties dialog window when you select your machine in the left panel on the main window and choose Edit->Properties, then select the Networks tab.

> Figure 7-6 Network Machine Properties

#### Fields

The following table explains the options available on this window.

> Table 7-6 Network Machine Properties

Field | Description
--- | ---
`BRIDGE` Listener Port | TCP/IP port number to be used by the `BRIDGE` process.
`Tlisten` Listener Port | TCP/IP port number to be used by the `tlisten` process.
USER ID | Specific USER ID of the BEA TUXEDO administrator on that machine (UNIX only). The corresponding BEA TUXEDO machine parameter is `UID`.
GROUP ID | Specific GROUP ID of the BEA TUXEDO administrator on that machine (UNIX only). The corresponding BEA TUXEDO machine parameter is `GID`.

#### Description

This is where you define port numbers, and `USER` and `GROUP` ID's.

#### Buttons

When you have filled in the fields, click OK to close the window and save your changes. (Or click Cancel to close the window without saving your changes.)

#### See Also

Configuring Machines (Step1), Modifying Machine Properties