Corporate Info | News | Solutions | Products | Partners | Services | Events | Download | How To Buy
eLink Adapter for R/3 ALE Doc Home | BEA eLink Adapter for R/3 ALE User Guide | Previous Topic | Next Topic | Contents | Index

Sample Configuration Files

This topic describes the two preconfigured sample cr3_ale.ubb files and the setenv files ("cr3_ale.ubb for UNIX" and "cr3_ale.ubb for Windows NT") that come with BEA eLink Adapter for R/3 ALE. It includes the following main sections:

- cr3_ale.ubb for UNIX

- cr3_ale.ubb for Windows NT

- setenv_ale.sh (UNIX)

- setenv_ale.bat (Windows NT)

cr3_ale.ubb for UNIX

>     ##############################################################
>     *RESOURCES
>     ##############################################################

>     IPCKEY		40000
>     DOMAINID		CR3
>     MASTER		SITE1
>     MAXACCESSERS		30
>     MAXSERVERS		20
>     MAXSERVICES		30
>     SCANUNIT		10
>     SANITYSCAN		12
>     BLOCKTIME		30
>     MAXGTT		200
>     MODEL		SHM
>     LDBAL		Y

>     ##############################################################
>     *MACHINES
>     ##############################################################

>     <system name>
>     	LMID=SITE1
>     	TYPE="HP-UX"
>     	TUXDIR="<your Tuxedo install directory>"
>     	TUXCONFIG="<your eLink app directory>/tuxconfig"
>     	TLOGDEVICE ="<your eLink app directory>/TLOG"
>     	TLOGSIZE=10
>     	APPDIR="<your eLink app directory>"
>     	ULOGPFX="<your eLink app directory>/ULOG"
>     	MAXWSCLIENTS=2
>     	UID=278

>     ##############################################################
>     *GROUPS
>     ##############################################################

>     QUE
>     	LMID=SITE1  GRPNO=1
>     	TMSNAME=TMS_QM TMSCOUNT=2
>     	OPENINFO="TUXEDO/QM:<your eLink app directory>/QUE:QSPACE"

>     CR3
>     	LMID=SITE1  GRPNO=2
>     	TMSNAME=TMS TMSCOUNT=2

>     ##############################################################
>     *SERVERS
>     ##############################################################

>     DEFAULT:
>     	CLOPT="-A"

>     TMQUEUE
>     	SRVGRP=QUE SRVID=1
>     	GRACE=0  RESTART=Y CONV=N  MAXGEN=10
>     	CLOPT="-s QSPACE:TMQUEUE --  "

>     TMQFORWARD
>     	SRVGRP=QUE SRVID=2
>     	GRACE=0  RESTART=Y  CONV=N  MAXGEN=10
>     	CLOPT=" -- -i 10 -q CR3_IDOC_IN,CR3_SUBMIT"

>     cr3alein
>         SRVGRP=CR3 SRVID=3
>     	CLOPT="-A -- -i cr3alein -e cr3alein.env"

>     cr3aleout
>         SRVGRP=CR3 SRVID=4
>     	CLOPT="-A -- -i cr3aleout -e cr3aleout.env"

>     ##############################################################
>     *SERVICES
>     ##############################################################

>     CR3_SUBMIT
>     CR3_IDOC_IN
>     CR3_ALE_OUT

1. Replace <your Tuxedo install directory> with the path to the location where you installed the eLink Platform.

2. Replace <your eLink app directory> with the path to the location containing the edited versions of the BEA eLink Adapter for R/3 ALE configuration files. The directory containing these files is named bin. For more information, see Step 1 of "Configuration Quick Reference for UNIX" in Configuration Quick Reference.

3. This value (278) that is set for the UID parameter is not always correct depending on the machine upon which the Adapter for R/3 ALE is running. Having this parameter incorrectly set causes an error while running the tmloadcf command. This parameter setting should be changed to a valid UID for your environment. See the Tuxedo Administration Guide for more information.

4. The value set for the Type variable should correspond to the system used. The value presently set in the sample version of cr3_ale.ubb (HP-UX) is appropriate only for HP systems. If you are using other UNIX systems, the appropriate value for your particular system should be used. For example, if you are using Solaris, this value should be SUNOS. If you don't know what the value is for your particular system, you can determine it with the following command:

   >     > uname

   The system will return a string that should be set as the Type value.

cr3_ale.ubb for Windows NT

>     ##############################################################
>     *RESOURCES
>     ##############################################################

>     IPCKEY		40000
>     DOMAINID		CR3
>     MASTER		SITE1
>     MAXACCESSERS		30
>     MAXSERVERS		20
>     MAXSERVICES		30
>     SCANUNIT		10
>     SANITYSCAN		12
>     BLOCKTIME		30
>     MAXGTT		200
>     MODEL		SHM
>     LDBAL		Y

>     ##############################################################
>     *MACHINES
>     ##############################################################

>     <system name>
>     	LMID=SITE1
>     	TYPE="Win32"
>     	TUXDIR="<your Tuxedo install directory>"
>     	TUXCONFIG="<your eLink app directory>\tuxconfig"
>     	TLOGDEVICE ="<your eLink app directory>\TLOG"
>     	TLOGSIZE=10
>     	APPDIR="<your eLink app directory>"
>     	ULOGPFX="<your eLink app directory>\ULOG"
>     	MAXWSCLIENTS=2

>     ##############################################################
>     *GROUPS
>     ##############################################################

>     QUE
>     	LMID=SITE1  GRPNO=1
>     	TMSNAME=TMS_QM TMSCOUNT=2
>     	OPENINFO="TUXEDO/QM:<your eLink app directory>\QUE;QSPACE"

>     CR3
>     	LMID=SITE1  GRPNO=2
>     	TMSNAME=TMS TMSCOUNT=2

>     ##############################################################
>     *SERVERS
>     ##############################################################

>     DEFAULT:
>     	CLOPT="-A"

>     TMQUEUE
>     	SRVGRP=QUE SRVID=1
>     	GRACE=0  RESTART=Y CONV=N  MAXGEN=10
>     	CLOPT="-s QSPACE:TMQUEUE --  "

>     TMQFORWARD
>     	SRVGRP=QUE SRVID=2
>     	GRACE=0  RESTART=Y  CONV=N  MAXGEN=10
>     	CLOPT=" -- -i 10 -q CR3_IDOC_IN,CR3_SUBMIT"

>     cr3alein
>         SRVGRP=CR3 SRVID=3
>     	CLOPT="-A -- -i cr3alein -e cr3alein.env"

>     cr3aleout
>         SRVGRP=CR3 SRVID=4
>     	CLOPT="-A -- -i cr3aleout -e cr3aleout.env"

>     ##############################################################
>     *SERVICES
>     ##############################################################

>     CR3_SUBMIT
>     CR3_IDOC_IN
>     CR3_ALE_OUT

1. Replace <your Tuxedo install directory> with the path to the location where you installed the eLink Platform.

2. Replace <your eLink app directory> with the path to the location containing the edited versions of the BEA eLink Adapter for R/3 ALE configuration files. The directory containing these files is named bin. For more information, see Step 1 of "Configuration Quick Reference for Windows NT" in Configuration Quick Reference.

setenv_ale.sh (UNIX)

This section provides a code listing corresponding to the template that is placed in <installation directory>/adapters/sapr3_ale/config during installation of the BEA eLink Adapter for R/3 ALE. <installation directory> is whatever path that you specified during installation. (Of course, this and other configuration files are copied to the bin directory during configuration, and this bin directory is <your eLink app directory> .)

>     #!/bin/sh
>     TUXDIR=<your Tuxedo directory> ;          export TUXDIR
>     APPDIR=<your eLink app directory> ;       export APPDIR
>     TUXCONFIG=$APPDIR/tuxconfig ;             export TUXCONFIG
>     QMCONFIG=$APPDIR/QUE ;                    export QMCONFIG
>     FLDTBLDIR32=$APPDIR:$TUXDIR/udataobj ;    export FLDTBLDIR32
>     FIELDTBLS32=cr3_ale.fml ;                export FIELDTBLS32

1. Replace <your Tuxedo directory> with the path to the location where you installed the eLink Platform.

2. Replace <your eLink app directory> with the path to the location containing the edited versions of the BEA eLink Adapter for R/3 ALE configuration files. The directory containing these files is named bin. For more information, see Step 1 of "Configuration Quick Reference for UNIX" in Configuration Quick Reference.

setenv_ale.bat (Windows NT)

This section provides a code listing corresponding to the template that is placed in <installation directory>\adapters\sapr3_ale\config during installation of the BEA eLink Adapter for R/3 ALE. <installation directory> is whatever path that you specified during installation. (Of course, this and other configuration files are copied to the bin directory during configuration, and this bin directory is <your eLink app directory> .)

>     rem
>     set TUXDIR=<your Tuxedo directory>
>     set APPDIR=<your eLink app directory>
>     set TUXCONFIG=%APPDIR%\tuxconfig
>     set QMCONFIG=%APPDIR%\QUE
>     set FLDTBLDIR32=%APPDIR%:%TUXDIR%\udataobj
>     set FIELDTBLS32=cr3_ale.fml,Usysfl32

Note: The value Usysf132 set as a FIELDTBLS32 value is optional and is only used if you intend to use the ud32 application.

1. Replace <your Tuxedo directory> with the path to the location where you installed the eLink Platform.

2. Replace <your eLink app directory> with the path to the location containing the edited versions of the BEA eLink Adapter for R/3 ALE configuration files. The directory containing these files is named bin. For more information, see Step 1 of "Configuration Quick Reference for Windows NT" in Configuration Quick Reference.

Copyright © 2000 BEA Systems, Inc. All rights reserved. Required browser: Netscape 4.0 or higher, or Microsoft Internet Explorer 4.0 or higher.