Corporate Info | News | Solutions | Products | Partners | Services | Events | Download | How To Buy
eLink Adapter for Kenan Arbor/BP Doc Home | BEA eLink Adapter for Kenan Arbor/BP User Guide | Previous Topic | Next Topic | Contents |

Installing eLink Adapter for Kenan Arbor/BP

This chapter contains the following topics:

- Pre-Installation Considerations

- Installing on Unix Platforms

- Distribution Libraries and Executables

Pre-Installation Considerations

The eLink Adapter for Kenan Arbor/BP runs on the HP-UX platform. Complete the following tasks prior to installing eLink Adapter for Kenan Arbor/BP:

- Read the BEA eLink Adapter for Kenan Arbor/BP Release Notes.

- Install and verify the operation of the BEA eLink Platform product.

Installing on Unix Platforms

To install the eLink Adapter for Kenan Arbor/BP on Unix platforms, you run the install.sh script. This script installs all the necessary software components. Perform the following steps to install the eLink Adapter for Kenan Arbor/BP on a supported UNIX platform.

1. Log on as root.

   >     $ su -
   >     Password:

2. Access the CD-ROM device.

   >     # ls -1 /dev/cdrom
   >     total 0
   >     brw-rw-rw-   1 root   sys    27,   0 January 27  10:55 c1b0t010

3. Mount the CD-ROM.

   >     # mount -r -F cdfs /dev/cdrom/c1b0t010 /mnt

4. Change the directory to your CD-ROM device.

   >     # cd /mnt

5. List the CD-ROM contents.

   >     # ls

   >     install.sh  hp

6. Execute the installation script.

   >     # sh ./install.sh

7. The installation script runs and prompts you for responses. Listing 2-1 is an example of the installation script. The entries in bold represent user responses.

   Listing 2-1 Install.sh Example

   >     cmadm@dalsun4:/cmhome/dist/bat-1 ls
   >     hp          install.sh  sun5x
   >     cmadm@dalsun4:/cmhome/dist/bat-1 sh install.sh

   >     01) hp/hpux1020      02) sun5x/sol26

   >     Install which platform's files? [01-       2, q to quit, l for list]: 2

   >     ** You have chosen to install from sun5x/sol26 **

   >     BEA eLink Adapter for Kenan Arbor/BP Release 1.1

   >     This directory contains the BEA eLink Adapter for Kenan Arbor/BP System for
   >     SunOS 5.6 (Solaris 2.6) on SPARC.

   >     Is this correct? [y,n,q]: y

   >     To terminate the installation at any time
   >     press the interrupt key,
   >     typically <del>, <break>, or <ctrl+c>.

   >     The following packages are available:

   >       1     eken            BEA eLink Adapter for Kenan Arbor/BP

   >     Select the package(s) you wish to install (or 'all' to install
   >     all packages) (default: all) [?,??,q]:

   >     BEA eLink Adapter for Kenan Arbor/BP
   >     (sparc) Release 1.1
   >     Copyright (c) 2000 BEA Systems, Inc.
   >     All Rights Reserved.
   >     Distributed under license by BEA Systems, Inc.
   >     BEA eLink is a trademark of BEA Systems, Inc.

   >     Directory where Kenan Arbor/BP Adapter files are to be installed
   >     (Enter your eLink Platform directory path) [?,q]: /work/cmadm/tux65

   >     Using /work/cmadm/tux65 as the Kenan Arbor/BP Adapter base directory

   >     Determining if sufficient space is available ...
   >     9406 blocks are required
   >     626198 blocks are available to /work/cmadm/tux65

   >     Unloading /cmhome/dist/bat-1/sun5x/sol26/eken/EKENT65.Z ...
   >     bin/ELINKABPO
   >     bin/lic.sh
   >     eLink/kenan_abp/elabp_env.cfg
   >     eLink/kenan_abp/setenv.sh
   >     eLink/kenan_abp/ubbelabp
   >     udataobj/fml_fields
   >     9380 blocks
   >     ... finished

   >     Changing file permissions...
   >     ... finished

   >     If your license file is accessible, you may install it now.
   >     Install license file? [y/n]: n

   >     Please don't forget to use lic.sh located in your product bin directory
   >     to install the license file from the enclosed floppy.
   >     Refer to your product Release Notes for details on how to do this.

   >     Installation of BEA eLink Adapter for Kenan Arbor/BP was successful

   >     Please don't forget to fill out and send in your registration card
   >     cmadm@dalsun4:/cmhome/dist/bat-1

8. Change the directory to your root directory.

   >     # cd /

9. Unmount the CD-ROM device.

Distribution Libraries and Executables

The eLink Adapter for Kenan Arbor/BP CD-ROM contains the following libraries and executable programs. After installing the eLink Adapter for Kenan Arbor/BP software, verify that these libraries and programs are installed on your system. Verify that the following files are installed by the eLink Adapter for Kenan Arbor/BP software.

####

Table 2-1 Distribution Libraries and Executables

Directory | Files
--- | ---
/bin | ELINKABPO
/elink/kenan_abp | elabp_env.cfg
/elink/kenan_abp | ubbelabp
/elink/kenan_abp | setenv.sh
/udataobj | fml_fields

Copyright © 2000 BEA Systems, Inc. All rights reserved. Required browser: Netscape 4.0 or higher, or Microsoft Internet Explorer 4.0 or higher.