Corporate Info | News | Solutions | Products | Partners | Services | Events | Download | How To Buy
eLink Adapter for R/3 BAPI/RFC Doc Home | eLink Adapter for R/3 BAPI/RFC User's Guide | Previous Topic | Next Topic | Contents | Index

TUXEDO Initialization File

BEA eLink Adapter for R/3 BAPI/RFC requires some configuration of the TUXEDO initialization file. For configuration instructions, see the BEA TUXEDO Administrator's Guide for your platform.

BEA eLink Adapter for R/3 BAPI/RFC provides a semi-configured TUXEDO initialization file, cr3_bapi.ubb , in the config sub-directory of the BEA eLink Adapter for R/3 BAPI/RFC installation directory. This cr3_bapi.ubb file is configured for the BEA eLink Adapter for R/3 BAPI/RFC servers and it requires further configuration for integration into the global TUXEDO environment. For example, in the GROUPS section of your UBB file, you must define the server group to which the BAPI/RFC eLink to R/3 belongs, such as CR3. See Sample cr3_bapi.ubb File, for a listing of this file.

Note: BAPI/RFC eLink to R/3 and RFC R/3 to eLink use TUXEDO transactions. For these components, you need to create a transaction log (TLOG) using TUXEDO administrative tools. See the BEA TUXEDO Administrator's Guide for your platform.

Copyright © 2000 BEA Systems, Inc. All rights reserved. Required browser: Netscape 4.0 or higher, or Microsoft Internet Explorer 4.0 or higher.