[Table of Contents] [Index] [Previous] [Next] Managing Your Installation

# Managing Your Installation

This chapter describes how to manage your BEA eLink Adapter for R/3 installation. It includes the following sections:

- Managing ALE Inbound and RFC Inbound

- Managing ALE Outbound

## Managing ALE Inbound and RFC Inbound

The ALE Inbound and RFC Inbound servers can be started and managed as normal TUXEDO application servers.

## Managing ALE Outbound

The ALE Outbound client is a TUXEDO client that is started by executing its startup script.

[Table of Contents] [Index] [Previous] [Next]