|  | BEA eLink for Mainframe SNA 3.2 Information Center
HOME | SEARCH | CONTACT | PDF FILES | WHAT'S NEW
| TABLE OF CONTENTS | PREVIOUS TOPIC | NEXT TOPIC

# Appendix D. Error Messages

The following messages are logged to the USERLOG file from an SNA Domains Instance (GWSNAX) and/or the SNA Communications Resource Manager (SNACRM).

1118:INFO | A BLOCKING timeout has occurred on an outbound request
| DESCRIPTION | A blocking time out has occurred on a request to the host.
| ACTION | Examine the ULOG for more information concerning the reason for the failure. Check configuration and increase the BLOCKTIME value, if needed.
1121:ERROR | Bad action state
| DESCRIPTION | An internal error has been detected processing the action.
| ACTION | Contact BEA Customer Support.
1122:ERROR | Invalid action index
| DESCRIPTION | An internal error has been detected, `gw_nw_acall` has returned a failure.
| ACTION | Contact BEA Customer Support.
1600:ERROR | Invalid action index
| DESCRIPTION | An internal error has been detected, `gw_nw_connect` has returned a failure.
| ACTION | Contact BEA Customer Support.
1602:ERROR | Cannot open SNA connection
| DESCRIPTION | Unable to allocate a network context. `gw_nw_AllocNwCtx` failed.
| ACTION | See previously printed ULOG message for cause.
1604:ERROR | Initialization of environment failed
| DESCRIPTION | Unable to initialize the conversation environment.
| ACTION | See previously printed ULOG message for cause.
1621:ERROR | Bad action state
| DESCRIPTION | An internal error has been detected processing the action.
| ACTION | Contact BEA Customer Support.
1622:ERROR | Invalid action index
| DESCRIPTION | An internal error has been detected, `gw_nw_convsend` has returned a failure.
| ACTION | Contact BEA Customer Support.
1625:ERROR | Invalid action index
| DESCRIPTION | An internal error has been detected, gw_nw_disconnect has returned a failure.
| ACTION | Contact BEA Customer Support.
1630:ERROR | Unable to send data on sna_conv_idx %d
| DESCRIPTION | A network error has occurred while while processing a send to the SNACRM. gw_nw_convsend failed.
| ACTION | Determine if SNACRM is still active. Look for other ULOG messages that specify a reason for this failure.
1989:ERROR | External encode/decode service returned error: \n\tTUXEDO code (%d) %s
| DESCRIPTION | A TUXEDO error has occurred in the Data Integration portion of the product.
| ACTION | Use the TUXEDO error to resolve the Data Integration problem. If unable to resolve the problem, contact BEA Customer Support.
1990:ERROR | Cannot create external decode action!
| DESCRIPTION | An internal error has occurred in the Data Integration portion of the product.
| ACTION | Contact BEA Customer Support.
1991:ERROR | Cannot create external encode action!
| DESCRIPTION | An internal error has occurred in the Data Integration portion of the product.
| ACTION | Contact BEA Customer Support.
1992:ERROR | Invalid action index
| DESCRIPTION | An internal error has been detected, `gw_nw_decode` has returned a failure.
| ACTION | Contact BEA Customer Support.
1993:ERROR | Invalid action index
| DESCRIPTION | An internal error has been detected, `gw_nw_encode` has returned a failure.
| ACTION | Contact BEA Customer Support.
1994:ERROR | Context data incorrect - null context index
| DESCRIPTION | An internal error has been detected, `gw_nw_decode` has returned a failure.
| ACTION | Contact BEA Customer Support.
1995:ERROR | Context data incorrect - null context index
| DESCRIPTION | An internal error has been detected, `gw_nw_encode` has returned a failure.
| ACTION | Contact BEA Customer Support.
2200:ERROR | Cannot malloc sna structures
| DESCRIPTION | An internal error has been detected, `gw_nw_init` was unable to allocate memory needed.
| ACTION | Contact BEA Customer Support.
2203:ERROR | Cannot malloc remote domain structure
| DESCRIPTION | An internal error has been detected, `gw_nw_init` was unable to allocate memory needed.
| ACTION | Contact BEA Customer Support.
2204:ERROR | Cannot malloc local SNA structure
| DESCRIPTION | An internal error has been detected, `gw_nw_init` was unable to allocate memory needed.
| ACTION | Contact BEA Customer Support.
2205:ERROR | Unable to obtain local snadom information from shmem
| DESCRIPTION | An internal error has been detected, `gw_nw_init` was unable to get needed information from shared memory.
| ACTION | Contact BEA Customer Support.
2206:ERROR | Cannot malloc remote service structure
| DESCRIPTION | An internal error has been detected, `gw_nw_init` was unable to allocate memory needed.
| ACTION | Contact BEA Customer Support.
2207:ERROR | Cannot malloc remote SNA structure
| DESCRIPTION | An internal error has been detected, `gw_nw_init` was unable to allocate memory needed.
| ACTION | Contact BEA Customer Support.
2210:ERROR | Can't create listener for this GATEWAY
| DESCRIPTION | An internal error has been detected, `gw_nw_init` was unable to create a listener.
| ACTION | Contact BEA Customer Support.
2211:WARNING | NO SNA conversations waiting for startup
| DESCRIPTION | No conversations are waiting at startup.
| ACTION | No action needs to be taken.
2214:ERROR | Unable to set APPC_GATEWAY environment variable
| DESCRIPTION | An internal error has been detected, `_gp_get_nodename` failed.
| ACTION | Contact BEA Customer Support.
2220:ERROR | Memory Allocation Failure
| DESCRIPTION | An internal error has been detected, `gw_nw_init` was unable to allocate memory needed.
| ACTION | Contact BEA Customer Support.
2221:ERROR | Memory Allocation Failure
| DESCRIPTION | An internal error has been detected, `gw_nw_init` was unable to allocate memory needed.
| ACTION | Contact BEA Customer Support.
2222:ERROR | Memory Allocation Failure for RDOM table
| DESCRIPTION | An internal error has been detected, `gw_nw_init` was unable to allocate memory needed.
| ACTION | Contact BEA Customer Support.
2223:ERROR | Memory Allocation Failure for SNALINK table
| DESCRIPTION | An internal error has been detected, `gw_nw_init` was unable to allocate memory needed.
| ACTION | Contact BEA Customer Support.
2224:ERROR | Memory Allocation Failure for SNACRM table
| DESCRIPTION | An internal error has been detected, `gw_nw_init` was unable to allocate memory needed.
| ACTION | Contact BEA Customer Support.
2225:ERROR | Memory Allocation Failure for SNASTACK table
| DESCRIPTION | An internal error has been detected, `gw_nw_init` was unable to allocate memory needed.
| ACTION | Contact BEA Customer Support.
2226:ERROR | Unable to access SNALINK information from memory
| DESCRIPTION | An internal error has been detected, `gw_nw_init` was unable to get needed information from shared memory.
| ACTION | Contact BEA Customer Support.
2227:ERROR | Unable to access SNACRM information from memory
| DESCRIPTION | An internal error has been detected, `gw_nw_init` was unable to get needed information from shared memory.
| ACTION | Contact BEA Customer Support.
2228:ERROR | Unable to convert SNACRM network address for %s
| DESCRIPTION | An error has occurred while trying to contact the SNACRM during startup.
| ACTION | Examine the ULOG for more information concerning the reason for the failure. Probably due to a configuration problem.
2229:ERROR | Unable to access SNASTACK information from memory
| DESCRIPTION | An internal error has been detected, `gw_nw_init` was unable to get needed information from shared memory.
| ACTION | Contact BEA Customer Support.
2230:ERROR | Unable to build internal network tables
| DESCRIPTION | An internal error has been detected, gw_nw_build_nwtbls failed.
| ACTION | Examine the ULOG for more information concerning the reason for the failure. Probably due to a configuration problem.
2231:ERROR | Unable to connect to SNACRM %s
| DESCRIPTION | An error has occurred while trying to contact the SNACRM during startup.
| ACTION | Examine the ULOG for more information concerning the reason for the failure. Possible reasons are: The SNACRM server was not configured in the UBBCONFIG. The `//host:port` parameters as specified in the DMCONFIG and the SNACRM command line parameters in the UBBCONFIG do not agree

2232:ERROR

Unable to SIGNON to SNACRM %s

DESCRIPTION

An error has occurred while signing on to the SNACRM.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

2233:ERROR

Unable to send STACK %s configuration to SNACRM %s

DESCRIPTION

An error has occurred while sending the stack configuration to the SNACRM.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

2234:ERROR

Unable to send SNALINK %s configuration to SNACRM %s

DESCRIPTION

An error has occurred while sending the link configuration to the SNACRM.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

2235:ERROR

Unable to send START message to SNACRM %s

DESCRIPTION

An error has occurred while sending the START command to the SNACRM.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

2236:ERROR

Unable to send SHUTDOWN message to SNACRM %s

DESCRIPTION

An error has occurred while sending the SHUTDOWN command to the SNACRM.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

2237:ERROR

STATE ERROR occurred during initialization, SHUTTING DOWN

DESCRIPTION

An internal state error has occurred start up.

ACTION

Contact BEA Customer Support.

2238:ERROR

Unknown message type received from SNACRM during initialization

DESCRIPTION

An unknown message has been received from SNACRM.

ACTION

Contact BEA Customer Support.

2239:ERROR

GATEWAY FAILS to complete connection to the SNACRM during initialization

DESCRIPTION

Connection to SNACRM is incomplete.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

2240:ERROR

Unable to send SHUTDOWN message to SNACRM %s

DESCRIPTION

GWSNAX is unable to send the SHUTDOWN command to SNACRM.

ACTION

Examine the ULOG for more information concerning the reason for the failure. The SNACRM process has probably already terminated.

2241:ERROR

Unable to access codepage table [%s], reason=%s (%d)

DESCRIPTION

GWSNAX is unable to find the file for the listed codepage for the reason specified. If reason is "Error 0", the (%d) value is the return code from the codepage read routine.

2 - Can't read from file

3 - Can't allocate memory

4 - Null/invalid pointer

5 - Invalid parameter

10 - Syntax error

11 - Unsupported format version

12 - Unsupported item

ACTION

Examine the DMCONFIG to determine if the CODEPAGE for a remote domain is specified incorrectly. Correct and retry.

2302:ERROR

Unable to complete initialization with SNACRM

DESCRIPTION

Connection to SNACRM is incomplete.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

2509:ERROR

Unable to obtain new convid id for this request

DESCRIPTION

An internal error has been detected, `gw_nw_getnxt_cd` has returned a failure.

ACTION

Contact BEA Customer Support.

2561:ERROR

Action data incorrect - null action index

DESCRIPTION

An internal error has been detected in `gw_nw_recv`.

ACTION

Contact BEA Customer Support.

2601:ERROR

Unable to send data on sna_conv_idx %d

DESCRIPTION

An error has occurred while sending reply data (`gw_nw_reply`) to the SNACRM.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

2800:ERROR

Invalid action index

DESCRIPTION

An internal error has been detected in `gw_nw_clr_convid`.

ACTION

Contact BEA Customer Support.

2801:ERROR

Invalid conversation id

DESCRIPTION

An internal error has been detected in `gw_nw_clr_convid`.

ACTION

Contact BEA Customer Support.

2802:ERROR

Invalid action index

DESCRIPTION

An internal error has been detected in `gw_nw_getnxt_cd`.

ACTION

Contact BEA Customer Support.

2805:ERROR

Unable to obtain remote domain info from shared memory

DESCRIPTION

An internal error has been detected, `gw_nw_init_env` was unable to get needed information from shared memory.

ACTION

Contact BEA Customer Support.

2806:ERROR

Unable to obtain snadom info from rdom

DESCRIPTION

An internal error has been detected, `gw_nw_init_env` was unable to get needed information from shared memory.

ACTION

Contact BEA Customer Support.

2808:ERROR

Cannot realloc sna structures

DESCRIPTION

An internal error has been detected, `gw_nw_AllocNwCtx` was unable to allocate memory needed.

ACTION

Contact BEA Customer Support.

2816:ERROR

Memory allocation failure

DESCRIPTION

An internal error has been detected, `gw_nw_empty_sndbuf` was unable to allocate memory needed.

ACTION

Contact BEA Customer Support.

2847:ERROR

SECURITY: Unable to get remote username from shared memory using local principal name %s

DESCRIPTION

A security error has occurred, the user is not authorized to access the remote host.

ACTION

Contact your local security administrator.

2848:ERROR

SECURITY: Unable to get local principal name from shared memory using appkey

DESCRIPTION

A security error has occurred, the user is not authorized to access the remote host.

ACTION

Contact your local security administrator.

2849:ERROR

SECURITY: Unable to extract password from shared memory

DESCRIPTION

A security error has occurred, the user is not authorized to access the remote host.

ACTION

Contact your local security administrator.

2850:ERROR

SECURITY: Unable to get security schedule

DESCRIPTION

A security error has occurred, the user is not authorized to access the remote host.

ACTION

Contact your local security administrator.

2853:ERROR

Invalid action index

DESCRIPTION

An internal error has been detected in `gw_nw_mk_error`.

ACTION

Contact BEA Customer Support.

2854:ERROR

Context data incorrect - null context index for action %d

DESCRIPTION

An internal error has been detected in `gw_nw_mk_error`.

ACTION

Contact BEA Customer Support.

2860:ERROR

SECURITY: Unable to get remote user from shared memory

DESCRIPTION

A security error has occurred, the remote user is not authorized to access the local TUXEDO host.

ACTION

Contact your local security administrator.

2935:ERROR

Too many unrecoverable errors occurred - deleting action

DESCRIPTION

An error has occurred in `gw_nw_mk_error`.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

2938:ERROR

SECURITY: Unable to get appkey for this outbound request

DESCRIPTION

A security error has occurred, the user is not authorized to access the remote host.

ACTION

Contact your local security administrator.

2939:ERROR

Deleting the action with the invalid context, %d

DESCRIPTION

An internal error has been detected in `gw_nw_snd` failure.

ACTION

Contact BEA Customer Support.

3028:ERROR

Can't find transaction node for Network TMS event!

DESCRIPTION

An internal error has been detected in `gw_nw_TranCommon`.

ACTION

Contact BEA Customer Support.

3029:WARNING

Shutting down GWSNAX!

DESCRIPTION

A severe error such as a protocol error or memory corruption has occurred and has already been logged. The GWSNAX process will shutdown.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

3030:ERROR

Unknown input transactional event(%d)!

DESCRIPTION

An internal error has been detected in `gw_nw_TranCvtMsgEvt2TranEvt`.

ACTION

Contact BEA Customer Support.

3031:ERROR

Invalid input object pointer!

DESCRIPTION

An internal error has been detected in `gw_nw_BindStateObject`.

ACTION

Contact BEA Customer Support.

3032:ERROR

Invalid input object initial state!

DESCRIPTION

An internal error has been detected in `gw_nw_BindStateObject`.

ACTION

Contact BEA Customer Support.

3033:ERROR

Invalid input object type!

DESCRIPTION

An internal error has been detected in `gw_nw_BindStateObject`.

ACTION

Contact BEA Customer Support.

3034:ERROR

Invalid input state object event(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_StateObjectTestEvent`.

ACTION

Contact BEA Customer Support.

3035:ERROR

Event %s is not allowed for state %s!

DESCRIPTION

An internal error has been detected in `gw_nw_StateObjectTestEvent`.

ACTION

Contact BEA Customer Support.

3036:ERROR

Invalid object event test metric with value %d for %s!

DESCRIPTION

An internal error has been detected in `gw_nw_StateObjectTestEvent`.

ACTION

Contact BEA Customer Support.

3037:ERROR

Invalid input trace object pointer!

DESCRIPTION

An internal error has been detected in `gw_nw_InitEventTrace`.

ACTION

Contact BEA Customer Support.

3038:ERROR

Invalid input trace object pointer!

DESCRIPTION

An internal error has been detected in `gw_nw_AddEventTrace`.

ACTION

Contact BEA Customer Support.

3039:ERROR

Input event %d out of range %d!

DESCRIPTION

An internal error has been detected in `gw_nw_AddEventTrace`.

ACTION

Contact BEA Customer Support.

3040:ERROR

Invalid input trace object pointer!

DESCRIPTION

An internal error has been detected in `gw_nw_QueryEventTrace`.

ACTION

Contact BEA Customer Support.

3041:ERROR

Invalid input trace object pointer!

DESCRIPTION

An internal error has been detected in `gw_nw_PrintEventTrace`.

ACTION

Contact BEA Customer Support.

3042:ERROR

Invalid input event identification(%d)!

DESCRIPTION

An internal error has been detected in `gw_nw_EventToString`.

ACTION

Contact BEA Customer Support.

3043:ERROR

Memory allocation failure

DESCRIPTION

An internal error has been detected in `gw_nw_CreateNodeTable`.

ACTION

Contact BEA Customer Support.

3044:WARNING

Transaction table already exists!

DESCRIPTION

An attempt has been made to create the node table and it already exists.

ACTION

No action needs to be taken.

3045:ERROR

Invalid input parameters!

DESCRIPTION

An internal error has been detected in `gw_nw_AssociateTranByTXID`.

ACTION

Contact BEA Customer Support.

3046:ERROR

Requires SNACRM id to create transaction!

DESCRIPTION

An internal error has been detected in `gw_nw_AssociateTranByTXID`.

ACTION

Contact BEA Customer Support.

3047:ERROR

Cannot associate with network transaction!

DESCRIPTION

An internal error has been detected in `gw_nw_AssociateTranByTXID`.

ACTION

Contact BEA Customer Support.

3048:ERROR

Invalid input transaction context!

DESCRIPTION

An internal error has been detected in `gw_nw_AssociateTranByTCTXT`.

ACTION

Contact BEA Customer Support.

3049:ERROR

Invalid input transaction event(%d)!

DESCRIPTION

An internal error has been detected in `gw_nw_AssociateTranByTCTXT`.

ACTION

Contact BEA Customer Support.

3050:ERROR

Invalid input transaction context pointer!

DESCRIPTION

An internal error has been detected in `gw_nw_TranCreateTCTXT`.

ACTION

Contact BEA Customer Support.

3051:ERROR

Exceeded local transaction limit(%d)!

DESCRIPTION

Number of concurrent transactions using this domain gateway exceeded the configured limit.

ACTION

Examine the DMCONFIG file for the MAXTRAN parameter, this number is the limit. If MAXTRAN is not specified, then examine the ubbconfig file for the MAXGTT parameter. In the later case MAXGTT is the limit. Modify the limit if necessary.

3052:ERROR

Can not create shared memory nettxid!

DESCRIPTION

An internal error has been detected in `gw_nw_TranCreateTCTXT`.

ACTION

Contact BEA Customer Support.

3053:ERROR

Create transaction tree node failed!

DESCRIPTION

`gw_nw_TranCreateTCTXT` failed to create the transaction tree node object. This can be caused by reaching the configured transaction limit or by a memory allocation failure.

ACTION

Examine the ULOG for more information concerning the reason for the failure. If the cause is the limit being reached, update the configuration. If the cause is a memory allocation failure, update the system and/or the system configuration.

3054:ERROR

Invalid input transaction handle!

DESCRIPTION

An internal error has been detected in `gw_nw_TranGetTCTXT`.

ACTION

Contact BEA Customer Support.

3055:ERROR

Invalid input transaction handle!

DESCRIPTION

An internal error has been detected in `gw_nw_TranGetTXID`.

ACTION

Contact BEA Customer Support.

3056:ERROR

Invalid input parameter!

DESCRIPTION

An internal error has been detected in `gw_nw_TranProcessEvent`.

ACTION

Contact BEA Customer Support.

3057:ERROR

Unable to calculate transaction handle!

DESCRIPTION

An internal error has been detected in `gw_nw_TranProcessEvent`.

ACTION

Contact BEA Customer Support.

3058:ERROR

Input Gateway event not transactional!

DESCRIPTION

The service request inbound from a remote host is transactional but the GWSNAX is not configured as a transactional gateway.

ACTION

The MAXSYNCLVL specified in the DMCONFIG must be 2 if transactional requests are to be processed.

3059:ERROR

Transaction does not exist!

DESCRIPTION

An internal error has been detected in `gw_nw_TranProcessEvent`.

ACTION

Contact BEA Customer Support.

3060:ERROR

Invalid input transaction handle!

DESCRIPTION

An internal error has been detected in `gw_nw_TranProcessEvent`.

ACTION

Contact BEA Customer Support.

3061:ERROR

Invalid Gateway action identification!

DESCRIPTION

An internal error has been detected in `gw_nw_TranSetUpExtTmsEvent`.

ACTION

Contact BEA Customer Support.

3062:ERROR

Decoding input transaction message failed!

DESCRIPTION

An internal error has been detected in `gw_nw_TranSetUpExtTmsEvent`.

ACTION

Contact BEA Customer Support.

3063:ERROR

SNACRM verb %d is not for TMS event!

DESCRIPTION

An internal error has been detected in `gw_nw_TranSetUpExtTmsEvent`.

ACTION

Contact BEA Customer Support.

3064:ERROR

Invalid input transaction context!!

DESCRIPTION

An internal error has been detected in `gw_nw_TranRelease`.

ACTION

Contact BEA Customer Support.

3065:ERROR

Transaction for context(%d) not found!

DESCRIPTION

The specified context for the transaction to be released could not be found by `gw_nw_TranRelease`.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

3066:ERROR

Cannot disassociate with network transaction!

DESCRIPTION

An error has been returned by `gw_tx_end`.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

3067:ERROR

Cannot set remote domain for transaction!

DESCRIPTION

An error has been returned by `gw_tx_set_rdom`. Several possibilities exist for this failure.

1. The process is unable to obtain the shared memory lock.

2. The configured limit for the number of remote domains that can be involved in the same transaction has been reached. This limit is specified in the MAXRDTRAN in the DMCONFIG.

ACTION

Examine the DMCONFIG and compare with the number of remote domains which might become involved in the same transaction. Update the DMCONFIG if necessary. Also examine the ULOG for more information concerning possible reasons for the failure.

3068:ERROR

Invalid input transaction handle!

DESCRIPTION

An internal error has been detected in `gw_nw_TranGetNodePtr`.

ACTION

Contact BEA Customer Support.

3069:ERROR

Transaction handle not in use!

DESCRIPTION

An internal error has been detected in `gw_nw_TranGetNodePtr`.

ACTION

Contact BEA Customer Support.

3070:ERROR

Transaction processing not yet initialize!

DESCRIPTION

An internal error has been detected in `gw_nw_TranGetNodePtr`.

ACTION

Contact BEA Customer Support.

3071:ERROR

Defined transaction limit %d reached!

DESCRIPTION

The number of concurrent transactions using this domain gateway has exceeded the limit.

ACTION

Examine the DMCONFIG file for the MAXTRAN parameter, this number is the limit. If MAXTRAN is not specified, then examine the ubbconfig file for the MAXGTT parameter. In the later case MAXGTT is the limit. Modify the limit if necessary.

3072:ERROR

Allocate SNACRM branch structure failed!

DESCRIPTION

An internal error has been detected in `gw_nw__gw_nw_AllocateNode`.

ACTION

Contact BEA Customer Support.

3073:ERROR

Unable to bind outbound node state object!

DESCRIPTION

A failure was returned by `gw_nw_BindStateObject`.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

3074:ERROR

Unable to bind inbound node state object!

DESCRIPTION

A failure was returned by `gw_nw_BindStateObject`.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

3075:ERROR

Unable to bind recover node state object!

DESCRIPTION

A failure was returned by `gw_nw_BindStateObject`.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

3076:ERROR

Invalid event %s to create transaction tree node!

DESCRIPTION

An internal error has been detected in _`gw_nw_AllocateNode`.

ACTION

Contact BEA Customer Support.

3077:ERROR

Memory allocation failure!

DESCRIPTION

An internal error has been detected in `gw_nw_AllocBranch`.

ACTION

Contact BEA Customer Support.

3078:ERROR

Event(%s) is not allowed to create SNACRM branch!

DESCRIPTION

An internal error has been detected in `gw_nw_AllocBranch`.

ACTION

Contact BEA Customer Support.

3079:ERROR

Free more branch than transaction tree node has!

DESCRIPTION

An internal error has been detected in `gw_nw_FreeBranch`.

ACTION

Contact BEA Customer Support.

3080:ERROR

Protocol violation, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_3`.

ACTION

Contact BEA Customer Support.

3081:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_4`.

ACTION

Contact BEA Customer Support.

3082:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_5`.

ACTION

Contact BEA Customer Support.

3083:ERROR

Branch in a bad state(%s) to issue prepare!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_5`.

ACTION

Contact BEA Customer Support.

3084:WARNING

Inconsistent branch state for prepare(%d, %d)!

DESCRIPTION

The transaction branch is in an inconsistent state for issuing a prepare. It will be assumed that they are all prepared.

ACTION

No action needs to be taken.

3085:INFO

Transaction node is deallocated because of ABEND!

DESCRIPTION

Informational message. GWSNAX detected an ABEND condition or received an ABEND event from the SNACRM which caused the node object to be destroyed.

ACTION

No action needs to be taken.

3086:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_7`.

ACTION

Contact BEA Customer Support.

3087:ERROR

Branch in a bad state(%s) to issue prepare!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_7`.

ACTION

Contact BEA Customer Support.

3088:WARNING

Inconsistent branch state for rollback(%d, %d)!

DESCRIPTION

The transaction branch was in an inconsistent state for issuing a rollback. It will be assumed that they are all rolled back.

ACTION

No action needs to be taken.

3089:WARNING

Inconsistent branch accounting for rollback(%d, %d, %d)!

DESCRIPTION

The transaction branch accounting was inconsistent while issuing a rollback.

ACTION

No action needs to be taken.

3090:WARNING

Incorrect branch accounting for rollback(%d)!

DESCRIPTION

The transaction branch accounting was incorrect while issuing a rollback.

ACTION

No action needs to be taken.

3091:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_8`.

ACTION

Contact BEA Customer Support.

3092:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_9`.

ACTION

Contact BEA Customer Support.

3093:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_10`.

ACTION

Contact BEA Customer Support.

3094:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_11`.

ACTION

Contact BEA Customer Support.

3095:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_12`.

ACTION

Contact BEA Customer Support.

3096:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_13`.

ACTION

Contact BEA Customer Support.

3097:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_14`.

ACTION

Contact BEA Customer Support.

3098:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_15`.

ACTION

Contact BEA Customer Support.

3099:ERROR

Retired node method!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_Retired`.

ACTION

Contact BEA Customer Support.

3100:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_16`.

ACTION

Contact BEA Customer Support.

3101:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_17`.

ACTION

Contact BEA Customer Support.

3102:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_18`.

ACTION

Contact BEA Customer Support.

3103:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_19`.

ACTION

Contact BEA Customer Support.

3104:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_20`.

ACTION

Contact BEA Customer Support.

3105:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_21`.

ACTION

Contact BEA Customer Support.

3106:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_22`.

ACTION

Contact BEA Customer Support.

3107:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_23`.

ACTION

Contact BEA Customer Support.

3108:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_24`.

ACTION

Contact BEA Customer Support.

3109:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_25`.

ACTION

Contact BEA Customer Support.

3110:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_26`.

ACTION

Contact BEA Customer Support.

3111:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_27`.

ACTION

Contact BEA Customer Support.

3112:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_28`.

ACTION

Contact BEA Customer Support.

3113:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_29`.

ACTION

Contact BEA Customer Support.

3114:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_30`.

ACTION

Contact BEA Customer Support.

3115:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_31`.

ACTION

Contact BEA Customer Support.

3116:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_32`.

ACTION

Contact BEA Customer Support.

3117:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_33`.

ACTION

Contact BEA Customer Support.

3118:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_39`.

ACTION

Contact BEA Customer Support.

3119:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_40`.

ACTION

Contact BEA Customer Support.

3120:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_42`.

ACTION

Contact BEA Customer Support.

3121:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_43`.

ACTION

Contact BEA Customer Support.

3122:ERROR

Encoding transaction message for verb(%d) failed!

DESCRIPTION

A failure was returned by snacrm_tx_msg.

ACTION

Contact BEA Customer Support.

3123:ERROR

SNACRM(%d) in bad state(%s) to issue verb(%d)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeSendToBranch`.

ACTION

Contact BEA Customer Support.

3124:ERROR

Send verb %d to snacrm failed!

DESCRIPTION

A failure has been detected while sending the specified verb to the SNACRM.

ACTION

Examine the ULOG for more information concerning the reason for the failure. Determine if the SNACRM process is still active.

3125:ERROR

Encoding transactional message for verb(%d) failed!

DESCRIPTION

A failure was returned by snacrm_tx_msg.

ACTION

Contact BEA Customer Support.

3126:ERROR

SNACRM(%d) in bad state(%s) to issue verb(%d)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeSendToSubordinate`.

ACTION

Contact BEA Customer Support.

3127:ERROR

Send verb(%d) to SNACRM failed!

DESCRIPTION

A failure has been detected while sending the specified verb to the SNACRM.

ACTION

Examine the ULOG for more information concerning the reason for the failure. Determine if the SNACRM process is still active.

3128:ERROR

Encoding transactional message for verb(%d) failed!

DESCRIPTION

A failure was returned by snacrm_tx_msg.

ACTION

Contact BEA Customer Support.

3129:ERROR

SNACRM(%d) in bad state(%s) to issue verb(%d)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeSendToSubordinate`.

ACTION

Contact BEA Customer Support.

3130:ERROR

Send verb(%d) to SNACRM failed!

DESCRIPTION

A failure has been detected while sending the specified verb to the SNACRM.

ACTION

Examine the ULOG for more information concerning the reason for the failure. Determine if the SNACRM process is still active.

3131:ERROR

Protocol violation, branch id[%d] at state(%s) receive event(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_BranchMethod_1`.

ACTION

Contact BEA Customer Support.

3132:ERROR

Memory allocation error!

DESCRIPTION

An internal error has been detected in `gw_nw_TranRestart`.

ACTION

Contact BEA Customer Support.

3133:ERROR

Unable to get shared memory semaphore lock!

DESCRIPTION

An internal error has been detected in `gw_nw_TranRestart`.

ACTION

Contact BEA Customer Support.

3134:ERROR

Unable to find transaction on GTT!

DESCRIPTION

An internal error has been detected in `gw_nw_TranRestart`.

ACTION

Contact BEA Customer Support.

3135:ERROR

SNAX group is not participating the transaction!

DESCRIPTION

An internal error has been detected in `gw_nw_TranRestart`.

ACTION

Contact BEA Customer Support.

3136:ERROR

Unable to setup transaction recovery!

DESCRIPTION

A failure was returned by `gw_nw_TranRecover`.

ACTION

Contact BEA Customer Support.

3137:ERROR

Unable to setup transaction recovery!

DESCRIPTION

A failure was returned by `gw_nw_TranRecover`.

ACTION

Contact BEA Customer Support.

3138:ERROR

Unable to create recovery action!

DESCRIPTION

A failure was returned by `gw_new_action`.

ACTION

Contact BEA Customer Support.

3139:ERROR

Unable to create recovery action!

DESCRIPTION

A failure was returned by `gw_chld_action`.

ACTION

Contact BEA Customer Support.

3140:ERROR

Unable to setup transaction recovery!

DESCRIPTION

A failure was returned by `gw_nw_TranRecover`.

ACTION

Contact BEA Customer Support.

3141:ERROR

Unable to create recovery action!

DESCRIPTION

A failure was returned by `gw_new_action`.

ACTION

Contact BEA Customer Support.

3142:ERROR

Unable to create recovery action!

DESCRIPTION

A failure was returned by `gw_chld_action`.

ACTION

Contact BEA Customer Support.

3143:ERROR

Unable to setup transaction recovery!

DESCRIPTION

A failure was returned by `gw_nw_TranRecover`.

ACTION

Contact BEA Customer Support.

3144:ERROR

Unable to setup transaction recovery!

DESCRIPTION

A failure was returned by `gw_nw_TranRecover`.

ACTION

Contact BEA Customer Support.

3145:ERROR

Unable to release shared memory lock!

DESCRIPTION

A failure was returned by _`gw_shmunlock`.

ACTION

Contact BEA Customer Support.

3146:ERROR

Unable to find SNACRM for superior remote domain(%s)!

DESCRIPTION

Failed to find the remote domain definition in the configuration in order to get the SNACRM identification.

ACTION

Examine the DMCONFIG for changes between the boots that would modify or remove the remote definition. If no such change has occurred, contact BEA Customer Support.

3147:ERROR

Could not find Remote Domain(%s) to do recovery!

DESCRIPTION

An internal error has been detected in `gw_nw_TranRecover`.

ACTION

Contact BEA Customer Support.

3148:ERROR

Could not find Remote Domain to do recovery!

DESCRIPTION

An internal error has been detected in `gw_nw_TranRecover`.

ACTION

Contact BEA Customer Support.

3149:ERROR

Could not create transaction tree structure!

DESCRIPTION

Unable to allocate a transaction tree node structure to represent the transaction recovery object.

ACTION

Examine the configuration to determine if there has been a change of MAXTRAN in DMCONFIG and/or a change of MAXGTT in UBBCONFIG. This condition may occur if there is a decrease in the number of transactions allowed between boots while many transactions must be recovered. If no changes have been made, contact BEA Customer Support.

3150:ERROR

Unable to create SNACRM branch structure!

DESCRIPTION

A failure was returned by _`gw_nw_AllocBranch`.

ACTION

Contact BEA Customer Support.

3151:ERROR

Unable to create SNACRM branch structure!

DESCRIPTION

A failure was returned by _`gw_nw_AllocBranch`.

ACTION

Contact BEA Customer Support.

3152:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_44`.

ACTION

Contact BEA Customer Support.

3153:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_45`.

ACTION

Contact BEA Customer Support.

3154:ERROR

Invalid Gateway action, receive event(%s) at state(%s)!

DESCRIPTION

An internal error has been detected in `gw_nw_NodeMethod_46`.

ACTION

Contact BEA Customer Support.

3155:ERROR

Invalid transaction context(%d) from SNACRM!

DESCRIPTION

An internal error has been detected in `gw_nw_TranSetUpExtTmsEvent`.

ACTION

Contact BEA Customer Support.

3156:WARNING

Undefined instrumentation register %d specification, ignored!

DESCRIPTION

An internal error has been detected in `gw_nw_SetUpInstrumentation`.

ACTION

Contact BEA Customer Support.

3157:INFO

CONNECTED TO SNACRM

DESCRIPTION

The GWSNAX process has successfully started the gateway connection to the SNACRM process.

ACTION

No action needs to be taken.

3158:WARNING

SNACRM Link %s Inoperable

DESCRIPTION

The specified link did not start up correctly.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

3159:ERROR

INVALID STARTTYPE (%s) - calling shutdown

DESCRIPTION

The STARTTYPE specified in the DMCONFIG must be AUTO or COLD.

ACTION

Correct the value specified in the DMCONFIG and restart.

3500:ERROR

Unable to find remote service definition link

DESCRIPTION

An internal error has been detected in `gw_nw_decode`.

ACTION

Contact BEA Customer Support.

3501:ERROR

Unable to find local service definition link

DESCRIPTION

An internal error has been detected in `gw_nw_decode`.

ACTION

Contact BEA Customer Support.

3502:ERROR

Buffer type (%s,%s) not defined in the buffer type switch!

DESCRIPTION

The buffer type associated with the inbound message is not specified in the type switch.

ACTION

Examine the application and the configuration to determine which buffer type is being used. GWSNAX only supports standard TUXEDO buffer types over the domain gateway. If the buffer type is VIEW, VIEW32, then also examine the environment variables VIEWDIR, VIEWFILES, VIEW32DIR, or VIEW32FILES.

3503:ERROR

Failed to tpalloc() STRING buffer of size %ld

DESCRIPTION

No buffer of type STRING was returned by tpalloc for the size specified.

ACTION

If the size specified is 1, then a length of zero was received. Check the application to determine if it has an error, otherwise contact BEA Customer Support.

3504:ERROR

Failed to tpalloc() CARRAY/X_OCTET buffer of size %ld

DESCRIPTION

No buffer of type CARRAY or X_OCTET was returned by tpalloc for the size specified.

ACTION

If the size specified is 1, then a length of zero was received. Check the application to determine if it has an error, otherwise contact BEA Customer Support.

3505:ERROR

Input buffer too big(%ld)!

DESCRIPTION

The buffer received of the size specified, exceeded the maximum allowed of 32767.

ACTION

Check the application to determine if it has an error, otherwise contact BEA Customer Support.

3506:ERROR

Missing subtype specification for %s

DESCRIPTION

The buffer type specified of VIEW, VIEW32, X_C_TYPE, or X_COMMON requires that a subtype be specified.

ACTION

Examine the application and the DMCONFIG and correct the problem.

3507:ERROR

Malloc temporary buffer of size(%ld) failed!

DESCRIPTION

An internal error has been detected in gw_nw_decode.

ACTION

Contact BEA Customer Support.

3508:ERROR

Convert buffer type(%s,%s) failed, convert failure!

DESCRIPTION

The conversion of the buffer received from the remote host was unsuccessful.

ACTION

Examine the application to determine if it has an error, examine the DMCONFIG definition for any errors in the buffer type specification. If no errors are found, contact BEA Customer Support.

3509:ERROR

Convert buffer type(%s,%s) failed, length too big!

DESCRIPTION

The conversion of the buffer received from the remote host was unsuccessful due to the resulting size exceeding the maximum of 32767.

ACTION

Examine the application to determine if it has an error, examine the DMCONFIG definition for any errors in the buffer type specification. If no errors are found, contact BEA Customer Support.

3510:ERROR

Failed to tpalloc() buffer (%s,%s) of size %ld

DESCRIPTION

No buffer was returned by tpalloc for the size specified to hold the converted buffer data.

ACTION

Examine the application to determine if it has an error, otherwise contact BEA Customer Support.

3511:ERROR

Missing subtype for FML type buffer!

DESCRIPTION

The buffer type specified of FML requires that a subtype be specified.

ACTION

Examine the application and the configuration to determine which buffer type is being used. GWSNAX only supports standard TUXEDO buffer types over the domain gateway. If the buffer type is VIEW, VIEW32, then also examine the environment variables VIEWDIR, VIEWFILES, VIEW32DIR, or VIEW32FILES.

3512:ERROR

Malloc temporary buffer of size(%ld) failed!

DESCRIPTION

An internal error has been detected in `gw_nw_decode`.

ACTION

Contact BEA Customer Support.

3513:ERROR

Malloc failed, unable to convert!

DESCRIPTION

The conversion of the buffer received from the remote host was unsuccessful.

ACTION

Examine the application to determine if it has an error, examine the DMCONFIG definition for any errors in the buffer type specification. If no errors are found, contact BEA Customer Support.

3514:ERROR

Failed to malloc temporary buffer of size %ld

DESCRIPTION

An internal error has been detected in `gw_nw_decode`.

ACTION

Contact BEA Customer Support.

3515:ERROR

Convert buffer type(%s,%s) failed, convert failure!

DESCRIPTION

The conversion of the buffer received from the remote host was unsuccessful.

ACTION

Examine the application to determine if it has an error, examine the DMCONFIG definition for any mistakes in the buffer type specification. If no errors are found, contact BEA Customer Support.

3516:ERROR

Failed to tpalloc() buffer (%s,%s) of size %ld

DESCRIPTION

No buffer was returned by tpalloc for the size specified to hold the converted buffer data.

ACTION

Check the application to determine if it has an error, otherwise contact BEA Customer Support.

3517:ERROR

Missing subtype definition for FML32 buffer type!

DESCRIPTION

The buffer type specified of FML32 requires that a subtype be specified.

ACTION

Correct the DMCONFIG definition.

3518:ERROR

Malloc temporary of size(%ld) failed!

DESCRIPTION

An internal error has been detected in `gw_nw_decode`.

ACTION

Contact BEA Customer Support.

3519:ERROR

Convert FML32 buffer type(%s,%s) failed, convert failure!

DESCRIPTION

The conversion of the buffer received from the remote host was unsuccessful.

ACTION

Examine the application to determine if it has an error, examine the DMCONFIG definition for any errors in the buffer type specification. If no errors are found, contact BEA Customer Support.

3520:ERROR

Malloc temporary buffer of size(%ld) failed!

DESCRIPTION

An internal error has been detected in `gw_nw_decode`.

ACTION

Contact BEA Customer Support.

3521:ERROR

Convert FML32 buffer with subtype(%s) failed!

DESCRIPTION

The conversion of the buffer received from the remote host was unsuccessful.

ACTION

Examine the application to determine if it has an error, examine the DMCONFIG definition for any errors in the buffer type specification. If no errors are found, contact BEA Customer Support.

3522:ERROR

Failed to tpalloc() FML32 buffer of size %d for %s!

DESCRIPTION

An internal error has been detected in `gw_nw_decode`.

ACTION

Contact BEA Customer Support.

3523:ERROR

Fail to convert for FML buffer(%s), exceeding limit!

DESCRIPTION

Failed to convert the FML buffer; the buffer size required to process the conversion exceeds the limit.

ACTION

Examine the application and the view for this buffer for any errors. If no errors are found, contact BEA Customer Support.

3524:ERROR

Fail to convert for FML32 buffer(%s), exceeding limit!

DESCRIPTION

Failed to convert the FML32 buffer; the buffer size required to process the conversion exceeds the limit.

ACTION

Examine the application and the view for this buffer for any errors. If no errors are found, contact BEA Customer Support.

3525:ERROR

Fail to retrieve remote service definition!

DESCRIPTION

Unable to find the remote service definition in shared memory.

ACTION

Examine the DMCONFIG remote service definitions. Correct any errors found. If no error is found, contact BEA Customer Support.

3526:ERROR

Fail to retrieve local service definition!

DESCRIPTION

Unable to find the local service definition in shared memory.

ACTION

Examine the DMCONFIG local service definitions. Correct any errors found. If no error is found, contact BEA Customer Support.

3527:ERROR

Must specify subtype for %s

DESCRIPTION

The buffer type specified of VIEW, VIEW32, X_C_TYPE, or X_COMMON requires that a subtype be specified.

ACTION

Correct any errors in the DMCONFIG buffer type definitions. If no errors are found, contact BEA Customer Support.

3528:ERROR

Malloc temporary buffer of size(%d) failed!

DESCRIPTION

An internal error has been detected in `gw_nw_encode`.

ACTION

Contact BEA Customer Support.

3529:ERROR

Convert buffer type %s with subtype %s failed(rc=%d)!

DESCRIPTION

The conversion of the buffer received from TUXEDO was unsuccessful.

ACTION

Examine the application to determine if it has an error, examine the DMCONFIG definition for any errors in the buffer type specification. If no errors are found, contact BEA Customer Support.

3530:ERROR

Convert buffer type %s with subtype %s failed(rc=%d)!

DESCRIPTION

The conversion of the buffer received from TUXEDO was unsuccessful due to the resulting size exceeding the maximum of 32767.

ACTION

Examine the application to determine if it has an error, examine the DMCONFIG definition for any errors in the buffer type specification. If no errors are found, contact BEA Customer Support.

3531:ERROR

Malloc temporary buffer of size(%d) failed!

DESCRIPTION

An internal error has been detected in `gw_nw_encode`.

ACTION

Contact BEA Customer Support.

3532:ERROR

FML buffer type requires subtype to be specified!

DESCRIPTION

The buffer type specified of FML requires that a subtype be specified.

ACTION

Correct the DMCONFIG definition.

3533:ERROR

Malloc temporary buffer of size(%d) failed!

DESCRIPTION

An internal error has been detected in `gw_nw_encode`.

ACTION

Contact BEA Customer Support.

3534:ERROR

Convert FML buffer with subtype %s failed(Ferror=%d)!

DESCRIPTION

The conversion of the FML buffer received from TUXEDO was unsuccessful. Ferror is the return code from the FML conversion routine.

ACTION

Examine the application to determine if it has an error, examine the DMCONFIG definition for any errors in the buffer type specification. If no errors are found, contact BEA Customer Support.

3535:ERROR

Malloc temporary buffer of size(%d) failed!

DESCRIPTION

An internal error has been detected in `gw_nw_encode`.

ACTION

Contact BEA Customer Support.

3536:ERROR

Convert FML buffer with subtype %s failed(Ferror=%d)!

DESCRIPTION

The conversion of the FML buffer received from TUXEDO was unsuccessful. Ferror is the return code from the FML conversion routine.

ACTION

Examine the application to determine if it has an error, examine the DMCONFIG definition for any errors in the buffer type specification. If no errors are found, contact BEA Customer Support.

3537:ERROR

Malloc buffer of size(%d) failed!

DESCRIPTION

An internal error has been detected in `gw_nw_encode`.

ACTION

Contact BEA Customer Support.

3538:ERROR

FML32 buffer type requires subtype to be specified!

DESCRIPTION

The buffer type specified of FML32 requires that a subtype be specified.

ACTION

Correct the DMCONFIG definition.

3539:ERROR

Malloc temporary buffer of size(%d) failed!

DESCRIPTION

An internal error has been detected, `gw_nw_Alloc` was unable to allocate memory needed.

ACTION

Contact BEA Customer Support.

3540:ERROR

Convert FML32 buffer with subtype %s failed(Ferror=%d)!

DESCRIPTION

The conversion of the FML32 buffer received from TUXEDO was unsuccessful. Ferror is the return code from the FML conversion routine.

ACTION

Examine the application to determine if it has an error, examine the DMCONFIG definition for any errors in the buffer type specification. If no errors are found, contact BEA Customer Support.

3541:ERROR

Malloc temporary buffer of size(%d) failed!

DESCRIPTION

An internal error has been detected, `gw_nw_Alloc` was unable to allocate memory needed.

ACTION

Contact BEA Customer Support.

3542:ERROR

Convert FML32 buffer with subtype %s failed(Ferror=%d)!

DESCRIPTION

The conversion of the FML32 buffer received from TUXEDO was unsuccessful. Ferror is the return code from the FML conversion routine.

ACTION

Examine the application to determine if it has an error, examine the DMCONFIG definition for any errors in the buffer type specification. If no errors are found, contact BEA Customer Support.

4000:ERROR

GP_SEND flow controlled for GPND %d

DESCRIPTION

An internal error has been detected, `gw_nw_proto_flow` has detected a flow control callback from gp_send.

ACTION

Contact BEA Customer Support.

4100:ERROR

Maximum number of pointers exceeded

DESCRIPTION

An internal error has been detected. The maximum number of pointers has exceeded 500.

ACTION

Contact BEA Customer Support.

4124:ERROR

Unable to format snacrm_acall

DESCRIPTION

An internal error has been detected, snacrm_acall has returned an error.

ACTION

Contact BEA Customer Support.

4125:ERROR

Unable to send data on sna_conv_idx %d, gpnd = %d

DESCRIPTION

An error has occurred while sending acall data (`gw_nw_acall`) to the SNACRM.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

4126:ERROR

Unable to format snacrm_connect

DESCRIPTION

An internal error has been detected, snacrm_connect has returned an error.

ACTION

Contact BEA Customer Support.

4127:ERROR

Unable to send data on sna_conv_idx %d, gpnd = %d

DESCRIPTION

An error has occurred while sending connect data (`gw_nw_connect`) to the SNACRM.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

4128:ERROR

Unable to format snacrm_send_data

DESCRIPTION

An internal error has been detected, snacrm_send has returned an error.

ACTION

Contact BEA Customer Support.

4130:ERROR

Unable to format snacrm_connect

DESCRIPTION

An internal error has been detected, snacrm_connect_rsp has returned an error.

ACTION

Contact BEA Customer Support.

5019:ERROR

Send event for RRCORR(%ld) failed!

DESCRIPTION

An internal error has been detected, `gw_nw_SendEvent` has returned an error.

ACTION

Contact BEA Customer Support.

5020:ERROR

Encode ACALL_RSP failed, RRCORR(%ld)!

DESCRIPTION

An internal error has been detected, snacrm_acall_rsp has returned an error.

ACTION

Contact BEA Customer Support.

5021:ERROR

Encode reply failed!

DESCRIPTION

An error was detected while attempting to encode the reply message data destined for the remote host.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

5022:ERROR

Invalid network descriptor(%d)!

DESCRIPTION

The network descriptor this context is invalid.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

5023:ERROR

Could not get transaction

DESCRIPTION

Failed to associate a transactional ACALL service request to a transaction object. The most likely reasons for this failure are:

1. The locally configured limit has been exceeded, or

2. Memory allocation has failed to create the transaction object.

ACTION

Determine if the application is licensed to do transactions. Examine the DMCONFIG file for the MAXTRAN parameter, this number is the limit. If MAXTRAN is not specified, then examine the ubbconfig file for the MAXGTT parameter. In the later case MAXGTT is the limit. Modify the limit if necessary. Verify that the remote domain MAXSYNCLVL is set to 2.

5024:ERROR

Could not get API

DESCRIPTION

An internal error has been detected. The API information is invalid.

ACTION

Contact BEA Customer Support.

5025:ERROR

Could not get transaction

DESCRIPTION

Failed to associate a transactional CONNECT service request to a transaction object. The most likely reasons for this failure are:

1. The locally configured limit has been exceeded, or

2. Memory allocation has failed to create the transaction object

ACTION

Determine if the application is licensed to do transactions. Examine the DMCONFIG file for the MAXTRAN parameter, this number is the limit. If MAXTRAN is not specified, then examine the ubbconfig file for the MAXGTT parameter. In the later case MAXGTT is the limit. Modify the limit if necessary. Verify that the remote domain MAXSYNCLVL is set to 2.

5026:ERROR

Could not get API

DESCRIPTION

An internal error has been detected. The API information is invalid.

ACTION

Contact BEA Customer Support.

5027:ERROR

Could not get API

DESCRIPTION

An internal error has been detected. The API information is invalid.

ACTION

Contact BEA Customer Support.

5028:ERROR

Protocol violation, shutdown gateway!

DESCRIPTION

An internal error has been detected by `gw_nw_crmrcv`.

ACTION

Contact BEA Customer Support.

5029:ERROR

Link status down for remote domain %s

DESCRIPTION

The link status returned by the SNACRM is LINK_DOWN.

ACTION

Determine if the stack is active and check that the session between the stack provider and the remote host is active.

5030:ERROR

Link status pending for remote domain %s

DESCRIPTION

The link status returned by the SNACRM is LINK_PENDING. Transaction recovery for the link is still in progress following a restart. Only non-transactional requests may be sent to this link.

ACTION

Wait until recovery is complete before requesting transactional services on this link.

5031:ERROR

Transaction not allowed, request rejected!

DESCRIPTION

Failed to send a transactional ACALL request to the remote domain because MAXSYNCLVL is not 2.

ACTION

Determine the following things:

1. GWSNAX is licensed for transactions, and

2. DMCONFIG specifies MAXSYNCLVL=2 for the link.

5032:ERROR

Transaction not allowed, request rejected!

DESCRIPTION

Failed to send a transactional CONNECT request to the remote domain because MAXSYNCLVL is not 2.

ACTION

Determine the following things:

1. GWSNAX is licensed for transactions, and

2. DMCONFIG specifies MAXSYNCLVL=2 for the link.

5033:ERROR

Protocol violation, shutdown gateway!

DESCRIPTION

An internal error has been detected by `gw_nw_crmrcv`.

ACTION

Contact BEA Customer Support.

5034:ERROR

Allocate context failed!

DESCRIPTION

An internal error has been detected. An error was returned by `gw_nw_AllocNwCtx`.

ACTION

Contact BEA Customer Support.

5035:ERROR

Enter shutdown

DESCRIPTION

An internal error has been detected by `gw_nw_crmrcv`.

ACTION

Contact BEA Customer Support.

5036:ERROR

Invalid conversation identification, shutdown gateway!

DESCRIPTION

An internal error has been detected by `gw_nw_convsend`.

ACTION

Contact BEA Customer Support.

5037:ERROR

Unknown message type, shutdown gateway!

DESCRIPTION

An internal error has been detected by `gw_nw_crmrcv`.

ACTION

Contact BEA Customer Support.

5038:ERROR

LINK_STATUS state error, shutdown gateway!

DESCRIPTION

An internal error has been detected by `gw_nw_crmrcv`.

ACTION

Contact BEA Customer Support.

5039:ERROR

Protocol violation, shutdown gateway!

DESCRIPTION

An internal error has been detected by `gw_nw_crmrcv`.

ACTION

Contact BEA Customer Support.

5040:ERROR

Enter shutdown

DESCRIPTION

An internal error has been detected, an error was returned by `gw_nw_getsncrm_idx`.

ACTION

Contact BEA Customer Support.

5041:ERROR

Trans Event Error shutdown

DESCRIPTION

An internal error has been detected, an error was returned by `gw_nw_TranSetUpExtTmsEvent`.

ACTION

Contact BEA Customer Support.

5042:WARNING

SIGNON identify failed, shutdown gateway!

DESCRIPTION

SNACRM returned an error to the SIGNON request by GWSNAX.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

5043:ERROR

Trans Event Error

DESCRIPTION

An internal error has been detected. An error was returned by `gw_nw_AssociateTranBy`.

ACTION

Contact BEA Customer Support.

5044:ERROR

SIGNON state error, shutdown gateway!

DESCRIPTION

An internal error has been detected, an error was returned by _`gw_nw_snacrm_nextop`.

ACTION

Contact BEA Customer Support.

5045:ERROR

STARTUP state error, shutdown gateway!

DESCRIPTION

An internal error has been detected, an error was returned by _`gw_nw_snacrm_nextop`.

ACTION

Contact BEA Customer Support.

5046:WARNING

LINK_STATUS decode error, shutdown gateway!

DESCRIPTION

An internal error has been detected. An error was returned by snacrm_linkstatus_rcv.

ACTION

Contact BEA Customer Support.

5047:WARNING

LINK_STATUS status error, shutdown gateway!

DESCRIPTION

An internal error has been detected by `gw_nw_crmrcv`.

ACTION

Contact BEA Customer Support.

5048:WARNING

LINK_CONFIG state error, shutdown gateway!

DESCRIPTION

An internal error has been detected, an error was returned by _`gw_nw_snacrm_nextop`.

ACTION

Contact BEA Customer Support.

5049:WARNING

STACK_CONFIG state error, shutdown gateway!

DESCRIPTION

An internal error has been detected, an error was returned by _`gw_nw_snacrm_nextop`.

ACTION

Contact BEA Customer Support.

5050:WARNING

SHUTDOWN message received, shutdown gateway!

DESCRIPTION

GWSNAX has received a SHUTDOWN request from the SNACRM and will shut down immediately.

ACTION

Examine the ULOG for more information concerning the reason for the shutdown.

5051:ERROR

LOG_DATA decode error, shutdown gateway!

DESCRIPTION

An internal error has been detected. An error was returned by `snacrm_log_data_rcv`.

ACTION

Contact BEA Customer Support.

5052:ERROR

LOG_DATA state error(%d), shutdown gateway!

DESCRIPTION

An internal error has been detected by `gw_nw_crmrcv`.

ACTION

Contact BEA Customer Support.

5053:ERROR

Protocol violation, shutdown gateway!

DESCRIPTION

An internal error has been detected by `gw_nw_crmrcv`. Inbound ACALL request contained SEND_INVITE for function DPL.

ACTION

Contact BEA Customer Support.

5054:ERROR

Invalid action index

DESCRIPTION

An internal error has been detected by `gw_nw_InBoundConnectRqst`.

ACTION

Contact BEA Customer Support.

5055:ERROR

Invalid action index

DESCRIPTION

An internal error has been detected by `gw_nw_OutBoundConnectRsp`.

ACTION

Contact BEA Customer Support.

5056:ERROR

Protocol violation, shutdown gateway!

DESCRIPTION

An internal error has been detected by `gw_nw_crmrcv`.

ACTION

Contact BEA Customer Support.

5057:ERROR

SEND_DATA decode error, shutdown gateway!

DESCRIPTION

An internal error has been detected by `gw_nw_crmrcv`.

ACTION

Contact BEA Customer Support.

5058:ERROR

Cannot create action to send remote disconnect

DESCRIPTION

An internal error has been detected, an error was returned by `gw_new_action`.

ACTION

Contact BEA Customer Support.

5059:ERROR

ACALL decode error, shutdown gateway!

DESCRIPTION

An internal error has been detected by `gw_nw_crmrcv`.

ACTION

Contact BEA Customer Support.

5060:ERROR

Invalid action index

DESCRIPTION

An internal error has been detected by `gw_nw_InBoundAcallRqst`.

ACTION

Contact BEA Customer Support.

5061:ERROR

Invalid action index

DESCRIPTION

An internal error has been detected by `gw_nw_OutBoundAcallRsp`.

ACTION

Contact BEA Customer Support.

5062:ERROR

Failed to find local service(%s) definition!

DESCRIPTION

Unable to find the local service definition for the inbound request.

ACTION

Examine the DMCONFIG local service definitions. Correct any errors found. If no error is found, contact BEA Customer Support.

5063:ERROR

Invalid link index

DESCRIPTION

An internal error has been detected, an error was returned by `_gw_nw_set_link_idx`.

ACTION

Contact BEA Customer Support.

5064:ERROR

Invalid query_rsp index

DESCRIPTION

An internal error has been detected by `gw_nw_QueryProcess`.

ACTION

Contact BEA Customer Support.

5065:ERROR

Enter shutdown

DESCRIPTION

A failure has been detected while sending the SNACRM_QSVC_RSP verb to the SNACRM.

ACTION

Examine the ULOG for more information concerning the reason for the failure. Determine if the SNACRM process is still active.

5066:ERROR

Encode SEND_DATA failed, RRCORR(%ld)!

DESCRIPTION

An internal error has been detected by `gw_nw_reply`.

ACTION

Contact BEA Customer Support.

5067:ERROR

Decode inbound ACALL request failed!

DESCRIPTION

An error has occurred while decoding an inbound ACALL request in `gw_nw_decode`.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

5068:ERROR

Could not get FUNC

DESCRIPTION

An internal error has been detected by `gw_nw_acall`.

ACTION

Contact BEA Customer Support.

5069:ERROR

Could not get FUNC

DESCRIPTION

An internal error has been detected by `gw_nw_connect`.

ACTION

Contact BEA Customer Support.

5070:ERROR

SECURITY: Failed in security checking for RRCORR(%lx)!

DESCRIPTION

Security checking failed for the inbound ACALL request. An error was returned by `gw_nw_SetSecurity`.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

5071:ERROR

BAD Transaction ID shutdown

DESCRIPTION

An internal error has been detected by `gw_nw_SendData`.

ACTION

Contact BEA Customer Support.

5072:ERROR

BAD Transaction ID shutdown

DESCRIPTION

An internal error has been detected by `gw_nw_OutBoundAcallRsp`.

ACTION

Contact BEA Customer Support.

5073:ERROR

Could not get API

DESCRIPTION

An internal error has been detected by `gw_nw_QueryProcess`.

ACTION

Contact BEA Customer Support.

5074:ERROR

Decode outbound ACALL response failed, RRCORR(%lx)!

DESCRIPTION

An error has occurred while decoding the response from the host application to an outbound ACALL.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

5075:ERROR

Invalid query_rsp index

DESCRIPTION

An internal error has been detected by `gw_nw_QueryProcessError`.

ACTION

Contact BEA Customer Support.

5076:ERROR

Invalid connect_resp index

DESCRIPTION

An internal error has been detected by `gw_nw_ConnectError`.

ACTION

Contact BEA Customer Support.

5077:ERROR

Enter shutdown

DESCRIPTION

A failure has been detected while sending the SNACRM_QSVC_RSP verb to the SNACRM.

ACTION

Examine the ULOG for more information concerning the reason for the failure. Determine if the SNACRM process is still active.

5078:ERROR

Enter shutdown

DESCRIPTION

A failure has been detected while sending the SNACRM_CONNECT_RSP verb to the SNACRM.

ACTION

Examine the ULOG for more information concerning the reason for the failure. Determine if the SNACRM process is still active.

5079:ERROR

BAD Transaction ID shutdown

DESCRIPTION

An internal error has been detected by `gw_nw_InBoundAcallRqst`.

ACTION

Contact BEA Customer Support.

5080:ERROR

Decode inbound connect request failed, RRCORR(%lx)!

DESCRIPTION

An error has occurred while decoding an inbound connect request in `gw_nw_InBoundConnectRqst`.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

5081:ERROR

SECURITY: Inbound connect request security check failed, RRCORR(%lx)!

DESCRIPTION

Security checking failed for the inbound CONNECT request. An error was returned by `gw_nw_SetSecurity`.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

5082:ERROR

Decode SEND_DATA failed, RRCORR(%lx)!

DESCRIPTION

An error has occurred while decoding an outbound send data request in `gw_nw_SendData`.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

5083:ERROR

Invalid buffer type, encode failed!

DESCRIPTION

The buffer type specified for the outbound message was invalid. GWSNAX only supports standard TUXEDO buffer types over the domain gateway.

ACTION

Correct the DMCONFIG definition.

5084:ERROR

Outbound ACALL encode failed!

DESCRIPTION

An error has occurred while encoding an outbound ACALL request in `gw_nw_encode`.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

5085:ERROR

BAD SNACRM_IDX shutdown

DESCRIPTION

An internal error has been detected by `gw_nw_InBoundAcallRqst`.

ACTION

Contact BEA Customer Support.

5086:ERROR

BAD Context shutdown

DESCRIPTION

An internal error has been detected by `gw_nw_InBoundAcallRqst`.

ACTION

Contact BEA Customer Support.

5087:ERROR

Invalid buffer type, decode failed!

DESCRIPTION

The buffer type specified for the inbound message was invalid. GWSNAX only supports standard TUXEDO buffer types over the domain gateway.

ACTION

Correct the DMCONFIG definition.

5088:ERROR

Unable to get RDOM

DESCRIPTION

An internal error has been detected by `gw_nw_init_env`.

ACTION

Contact BEA Customer Support.

5089:ERROR

BAD SNACRM_IDX shutdown

DESCRIPTION

An internal error has been detected by `gw_nw_InBoundConnectRqst`.

ACTION

Contact BEA Customer Support.

5090:ERROR

Outbound CONNECT encode failed!

DESCRIPTION

An error has occurred while encoding an outbound CONNECT request in `gw_nw_encode`.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

5091:ERROR

Outbound CONVSEND encode failed!

DESCRIPTION

An error has occurred while encoding an outbound CONVSEND request in `gw_nw_encode`.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

5093:ERROR

Bad Connect

DESCRIPTION

An internal error has been detected by `gw_nw_crmrcv`.

ACTION

Contact BEA Customer Support.

5094:ERROR

Unable to send data on sna_conv_idx %d, gpnd = %d

DESCRIPTION

An error has occurred while sending a connect response to the SNACRM.

ACTION

Examine the ULOG for more information concerning the reason for the failure.

5095:ERROR

BAD Transaction ID shutdown

DESCRIPTION

An internal error has been detected by `gw_nw_InBoundConnectRqst`.

ACTION

Contact BEA Customer Support.

5096:ERROR

Unable to obtain socket id

DESCRIPTION

An internal error has been detected by `gw_nw_link_gp`.

ACTION

Contact BEA Customer Support.

5097:ERROR

Unable to get RDOM

DESCRIPTION

An internal error has been detected by `gw_nw_link_gp`.

ACTION

Contact BEA Customer Support.

5098:ERROR

Invalid action index

DESCRIPTION

An internal error has been detected by `gw_nw_link_gp`.

ACTION

Contact BEA Customer Support.

5099:ERROR

Allocate context failed!

DESCRIPTION

An internal error has been detected, an error was returned by `gw_nw_AllocNwCtx`.

ACTION

Contact BEA Customer Support.

5100:ERROR

Unable to obtain socket id

DESCRIPTION

An internal error has been detected by `gw_nw_init_env`.

ACTION

Contact BEA Customer Support.

5101:ERROR

Unable to find view file for %s %s

DESCRIPTION

Failed to find the view file for the FML buffer type specified in the INBUFTYPE for an inbound request.

ACTION

Examine the environment variables VIEWDIR, VIEWFILES, VIEW32DIR, and VIEW32FILES to determine if the requested view is present.

5102:ERROR

Invalid action index

DESCRIPTION

An internal error has been detected by `gw_nw_reply`.

ACTION

Contact BEA Customer Support.

5103:ERROR

Invalid action index

DESCRIPTION

An internal error has been detected by `gw_nw_reply`.

ACTION

Contact BEA Customer Support.

5104:ERROR

Invalid action index

DESCRIPTION

An internal error has been detected by `gw_nw_QueryProcess`.

ACTION

Contact BEA Customer Support.

5105:ERROR

Invalid buffer pointer

DESCRIPTION

An internal error has been detected by `gw_nw_encode`.

ACTION

Contact BEA Customer Support.

5106:ERROR

Allocate send buffer failed!

DESCRIPTION

An internal error has been detected, an error was returned by `gw_nw_empty_sndbuf`.

ACTION

Contact BEA Customer Support.

5107:ERROR

Unable to get appkey for this outbound request

DESCRIPTION

An internal error has been detected, `gw_shm_getbylink` returned an error while getting the remote domain entry.

ACTION

Examine the DMCONFIG remote domain definitions and its security setting. Correct any errors found. If no error is found, contact BEA Customer Support.

5108:ERROR

Enter shutdown

DESCRIPTION

An internal error has been detected by `gw_nw_SendEvent`.

ACTION

Contact BEA Customer Support.

5109:ERROR

Unable to find view file for %s %s

DESCRIPTION

Failed to find the view file for encoding outbound FML data as specified in the OUTBUFTYPE.

ACTION

Examine the environment variables VIEWDIR, VIEWFILES, VIEW32DIR, and VIEW32FILES to determine if the requested view is present.

5110:ERROR

Unable to find view file for %s %s

DESCRIPTION

Failed to find the view file for encoding outbound FML32 data as specified in the OUTBUFTYPE.

ACTION

Examine the environment variables VIEWDIR, VIEWFILES, VIEW32DIR, and VIEW32FILES to determine if the requested view is present.

5111:ERROR

BAD Context shutdown caused at transaction associate

DESCRIPTION

An internal error has been detected, an error was returned by `gw_nw_AssociateTranByTCTXT`.

ACTION

Contact BEA Customer Support.

5112:ERROR

System full, can't create action, Enter shutdown

DESCRIPTION

Failed to create GWSNAX gateway internal scheduled event to handle failure ore disconnect.

ACTION

Either memory allocation failed or a system limit was reached. Contact BEA Customer Support.

5113:ERROR

Realloc buffer of size(%d) failed!

DESCRIPTION

An internal error has been detected, `gw_nw_Realloc` was unable to allocate memory needed.

ACTION

Contact BEA Customer Support.

5114:ERROR

Invalid network descriptor(%d)!

DESCRIPTION

An internal error has been detected by `gw_nw_acall`.

ACTION

Contact BEA Customer Support.

6000:ERROR

YOUR eLink SNA LICENSE IS EITHER INVALID OR EXPIRED

DESCRIPTION

The eLink for Mainframe SNA v3 license is missing from the lic.txt file in $TUXDIR/udataobj or it has expired.

ACTION

Look in the $TUXDIR/udataobj/lic.txt file for a section labeled eLink_SNA v3 (or CONNECT_SNA 3.x) and if present, check the expiration date.

6001:WARNING

YOUR eLink SNA LICENSE IS NOT ENABLED FOR SYNCLEVEL 2, FORCED TO SYNCLEVEL 1

DESCRIPTION

The eLink for Mainframe SNA v3 license does not include the license to run requests at synclevel 2 (transactional).

ACTION

MAXSYNCLVL has been specified as 2 in the DMCONFIG DM_SNALINKS section. This level requires an additional license. Look in the `$TUXDIR/udataobj/lic.txt` file for a section labeled eLink_SNA_TX v3 (or CONNECT_SNA_TX 3.x) and if present, check the expiration date.

9001:ERROR

<taskname> timed out with failCode <failcode>

DESCRIPTION

A conversation has timed out in the SNACRM with the stack return code of `<failcode>`. A timer event set to watch a conversation has expired.

`<taskname>` may appear as:

OB-Conversation #nn (`<linkref>`) tx #m `<tranname>`, or

IB-Conversation #nn (`<linkref>`) tx #m `<tranname>`

where:

nn is an internal APPC conversation number.

m is the transaction context where -1 signifies non-transactional.

ACTION

Examine `stderr` and the ULOG for additional information concerning the failure.

9002:ERROR

Server (<stackref>) Creation Failed

DESCRIPTION

SNACRM was unable to instantiate the stack object due to an error.

ACTION

Check for additional messages in stderr. Could be that the shared library for the stack or the stack interface could not be loaded due to an incorrect library path.

9003:ERROR

Server Failed (<stackref>), Code = <returncode>

DESCRIPTION

SNACRM received a bad return code from the stack start-up.

ACTION

The <returncode> is the value returned by the SNA Stack software. Check the status of the stack and the configuration of the stack and the DMCONFIG.

Note: Unless you started the SNACRM as a TUXEDO server, you must manually kill the SNACRM process.

9004:ERROR

Configuration change on link <linkref> requires cold start

DESCRIPTION

Attempting to do a warm start after changing the domain configuration.

ACTION

Change start type to "COLD" and restart.

9005:WARNING

Unrecovered transaction, ID=<tctxt>, blob dropped. Transaction presumed forgotten.

DESCRIPTION

An attempt was make by TUXEDO to recover the specified transaction which was unknown by the SNACRM. It is presumed that it was already committed or aborted prior to the recovery attempt.

ACTION

None. This message for information only.

9006:ERROR

Unable to start the recovery task for link <linkref>

DESCRIPTION

An error occurred during the warm start of TUXEDO.

ACTION

Cold start the TUXEDO application.

9008:WARNING

Unknown tranid dropped, id=<tctxt>

DESCRIPTION

Recovery was requested by TUXEDO on a transaction that was already forgotten by the SNACRM.

ACTION

None. This message for information only.

9009:ERROR

No blob with recovery request. Transaction dropped, id=<tctxt>

DESCRIPTION

Attempting to warm start after the SNACRM's BLOBLOG has been modified.

ACTION

Change start type to "COLD" and restart.

9010:ERROR

<taskname> failed with failCode <failcode>

DESCRIPTION

A conversation has failed with the stack return code of <failcode>.

`<taskname>` may appear as:

OB-Conversation #nn (`<linkref>`) tx #m `<tranname>`, or

IB-Conversation #nn (`<linkref>`) tx #m `<tranname>`

where:

nn is an internal APPC conversation number.

m is the transaction context where -1 signifies non-transactional.

Possible values for the <failcode> are:

1. Communications - unable to create the APPCserver object.

2. MemoryAllocation - internal error allocating memory.

3. InvalidObject - a SNACRM object could not be created or has been made invalid by some previous error.

4. InputOutput - error occurred during file I/O or an unexpected APPC return code was received.

5. Registration - internal task cannot be registered.

ACTION

Examine stderr and the ULOG for additional information concerning the failure. For failcode InputOutput, verify that the user starting the SNACRM process has the proper file permissions for the BLOBLOG and RSTRTLOG. If no apparent error is found, contact BEA Customer Support.

9011:ERROR

Attempt to connect as second master refused!

DESCRIPTION

A second GWSNAX is attempting to connect to the SNACRM as a master gateway. Only one master gateway is allowed.

ACTION

Ensure that multiple TUXEDO configurations do not use the same SNACRM address.

9012:ERROR

Attempt to connect as master in autonomous mode refused!

DESCRIPTION

An attempt to connect to the SNACRM as a master gateway was made when the SNACRM was running in autonomous mode.

ACTION

Ensure that multiple TUXEDO configurations do not use the same SNACRM address.

9013:ERROR

Attempt to connect with incorrect group name (<groupname>) refused!

DESCRIPTION

The group name in the DMCONFIG file does not match the group name specified in the SNACRM command line.

ACTION

Correct the group name that is in error and restart.

9014:ERROR

INTERNAL ERROR: memory allocation failed [for new context|data buffer]

DESCRIPTION

Internal error allocating memory.

ACTION

Contact BEA Customer Support.

9015:ERROR

INTERNAL ERROR: server registration failed

DESCRIPTION

Internal error registering the APPC server.

ACTION

Contact BEA Customer Support.

9016:ERROR

Link refers to undefined APPC stack (<stackref>)!

DESCRIPTION

The stackref in the link configuration is incorrect.

ACTION

Correct the stackref that is in error, run dmloadcf, and restart.

9017:ERROR

INTERNAL ERROR: link registration failed

DESCRIPTION

Internal error registering the link.

ACTION

Contact BEA Customer Support.

9018:ERROR

Invalid Transition <additional information>

DESCRIPTION

An internal state table failure has occurred. The `<additional information>` will be one of the following:

1. From `<oldstate>` to `<newstate>` for `<dir>`-bound transaction #`<tid>`

2. To `<newstate>` for in-bound transaction #`<tid>`

3. To `<newstate>` for out-bound transaction #`<tid>`

ACTION

Contact BEA Customer Support.

9019:ERROR

Unknown Service Correlator = <correlator>, message dropped

DESCRIPTION

Internal error assigning service correlator values.

ACTION

Contact BEA Customer Support.

9020:ERROR

Duplicate Service Correlator = <correlator>

DESCRIPTION

Internal error assigning service correlator values.

ACTION

Contact BEA Customer Support.

9021:ERROR

Invalid Remote Link Name <linkref>

DESCRIPTION

The remote link name in a request does not match any defined link name.

ACTION

Correct the DMCONFIG and restart.

9022:ERROR

Invalid transaction context = <tctxt>

DESCRIPTION

Internal error assigning transaction context values.

ACTION

Contact BEA Customer Support.

9023:ERROR

Unknown Service Correlator = <correlator>, message dropped

DESCRIPTION

Internal error assigning service correlator values.

ACTION

Contact BEA Customer Support.

9024:ERROR

Invalid initial syncpoint received from subordinate, tx#<tid>

DESCRIPTION

Syncpoint processing protocol violation. Subordinate member of conversation attempted to initiate a syncpoint.

ACTION

Contact BEA Customer Support.

9025:ERROR

Invalid Input Message Discarded

DESCRIPTION

Internal error, bad message sent between GWSNAX and SNACRM.

ACTION

Contact BEA Customer Support.

9026:ERROR

CNOS Notification Received for unknown partner <partnerLU>

DESCRIPTION

Multiple instances of the SNACRM may be using the same local LU.

ACTION

Ensure that multiple TUXEDO configurations do not use the same local LU.

9027:WARNING

Remote Stop Received for <linkref>

DESCRIPTION

The remote host has issued a stop for the specified link.

ACTION

None. This message for information only.

9028:WARNING

Remote Start Received for <linkref>

DESCRIPTION

The remote host has issued a start for the specified link.

ACTION

None. This message for information only.

9029:ERROR

Undefined Remote LU on link <linkref>

DESCRIPTION

The remote LU does not exist as defined.

ACTION

Check the DMCONFIG file and the stack configuration and correct the mis-match.

9030:ERROR

Unable to start session on link <linkref>. Reason=<reason>

DESCRIPTION

Link activation failure due to SNA error.

ACTION

<reason> is the description of the stack return code. Determine the cause and correct.

9031:ERROR

Unable to initialize link <linkref>. Reason=<reason>

DESCRIPTION

Link initialization failure due to SNA error.

ACTION

<reason> is the description of the stack return code. Determine the cause and correct.

9032:ERROR

No Available Session on link <linkref> for context <correlator>

DESCRIPTION

Max sessions has been exceeded.

ACTION

Check session limits in DMCONFIG, stack configuration, CICS or VTAM. Increase if necessary.

9033:ERROR

Requested Synclevel not supported by link <linkref> for context <correlator> (synclevel <level>)

DESCRIPTION

Attempted to issues a request at sync level <level> on a link that does not support that level.

ACTION

Correct application or DMCONFIG.

9034:ERROR

Service Request at SyncLevel=2 Rejected on PENDING link <linkref> for context <correlator>

DESCRIPTION

An attempt to start a new sync level 2 request has been received and the Link is currently processing recovery information.

ACTION

Wait until recovery is complete to request sync level 2 services.

9035:ERROR

Inbound Request Transform Failed (<status>) for context <correlator>

DESCRIPTION

An error has occurred while processing the CICS transform for an inbound DPL request. This normally occurs when the API entry in the DMCONFIG for the local service specifies CICS instead of ATMI.

ACTION

Check DMCONFIG for incorrect specification of local service API entry.

9036:ERROR

Inbound Response Transform Failed (<status>) for context <correlator>

DESCRIPTION

An error has occurred while processing the CICS transform for an inbound DPL response. This normally occurs when the API entry in the DMCONFIG for the local service specifies CICS instead of ATMI.

ACTION

Check DMCONFIG for incorrect specification of local service API entry.

9037:ERROR

Outbound Request Transform Failed (<status>) for context <correlator>

DESCRIPTION

An error has occurred while processing the CICS transform for an outbound DPL request. This normally occurs when the API entry in the DMCONFIG for the remote service specifies CICS instead of ATMI.

ACTION

Check DMCONFIG for incorrect specification of local service API entry.

9038:ERROR

Outbound Response Transform Failed (<status>) for context <correlator>

DESCRIPTION

An error has occurred while processing the CICS transform for an outbound DPL response. This normally occurs when the API entry in the DMCONFIG for the remote service specifies CICS instead of ATMI.

ACTION

Check DMCONFIG for incorrect specification of local service API entry.

9039:ERROR

Conversation terminated without confirm for context <correlator>

DESCRIPTION

Sync level 2 conversation was terminated with out confirm.

ACTION

Check application program and correct.

9040:ERROR

Inbound Confirm not supported

DESCRIPTION

Host application is requesting an inbound confirm. This is not supported.

ACTION

Check host application program and correct.

9041:ERROR

Inbound Confirm for multi-ISRT not supported

DESCRIPTION

Host IMS application is requesting an inbound confirm and using multiple ISRT commands. This is not supported.

ACTION

Check host application program and correct.

9043:ERROR

Missing send last from host (ATMI request/response) for context <correlator>

DESCRIPTION

Host application did not issue send last during an out-bound request/response service. The host application may have abended.

ACTION

Check application program and correct.

9044:INFO

DPL program abended with CICS code <abendcode>, program=<progname>

DESCRIPTION

The specified host DPL program has abended with the code specified.

ACTION

None. This message is for information only.

9045:INFO

DPL program failed with CICS rcode <eibrcode>, program=<progname>

DESCRIPTION

The specified host DPL program has failed with the eibrcode specified.

ACTION

None. This message is for information only.

9046:ERROR

Invalid combination for Service Context <correlator>, <combination>

DESCRIPTION

The specified `<combination>` is invalid. It will be one of the following:

1. Sync-Level, function, and API

2. Function and API

ACTION

Examine the DMCONFIG and make corrections.

9047:ERROR

Sequence number error for Service Context <correlator>, seqno <seqno>

DESCRIPTION

There has been a sequence number failure for the specified context.

ACTION

Contact BEA Customer Support.

9048:ERROR

Invalid conversation task for Service Context <correlator>, task=<task>

DESCRIPTION

The conversation has already been terminated.

ACTION

Contact BEA Customer Support.

9049:ERROR

Invalid task switch for Service Context <correlator>, from <task1> to <task2>

DESCRIPTION

An internal protocol violation has occurred.

ACTION

Contact BEA Customer Support.

9050:ERROR

Transformer creation failed for in-bound transaction <trancode>

DESCRIPTION

An internal error has occurred.

ACTION

Contact BEA Customer Support.

9051:ERROR

Transformer failed for in-bound transaction <trancode>

DESCRIPTION

An internal error has occurred. Resource name is not present.

ACTION

Contact BEA Customer Support.

9052:WARNING

Inter-task Message dropped (<verbname>), parm=<parm> From: <task1> to <task2>

DESCRIPTION

An internal message between two tasks has been dropped.

ACTION

None. This message is for information only.

9053:ERROR

Attempt to send <nnnnn> bytes (> 32767)

DESCRIPTION

The length of a send request exceeded 32767 (including overhead).

ACTION

Check application program and correct.

9054:ERROR

Allocation Failure for <trancode> on <remotesysid>: <error>

DESCRIPTION

An Allocation error occurred.

ACTION

The reason for the failure is described by <error>. Correct problem with configuration or application.

9055:ERROR

Invalid Exchange Logs GDS variable received from <remotesysid>

DESCRIPTION

The log files for the SNACRM have been incorrectly modified.

ACTION

Run CRMLOGS to examine the SNACRM log file. Cold start the TUXEDO application.

9056:ERROR

Invalid cold start received from <remotesysid>. Unrecovered local transactions are pending.

DESCRIPTION

Attempting to cold start host while warm starting TUXEDO.

ACTION

Run CRMLOGS to examine the SNACRM log file. Cold start the TUXEDO application.

9057:ERROR

Invalid warm start received from <remotesysid>. Unknown log name.

DESCRIPTION

The log files for the SNACRM have been incorrectly modified.

ACTION

Run CRMLOGS to examine the SNACRM log file. Cold start the TUXEDO application.

9058:ERROR

Invalid Compare States GDS variable received from <remotesysid>

DESCRIPTION

The log files for the SNACRM have been incorrectly modified.

ACTION

Run CRMLOGS to examine the SNACRM log file. Cold start the TUXEDO application.

9059:ERROR

Mixed Heuristic on link <linkref> for <unitofwork> Correlator [<correlator>]

DESCRIPTION

One side has reported committed while the other side has reported aborted.

ACTION

Check the ULOG for any additional messages.

9060:WARNING

Inbound Exchange Logs Rejected for <remotesysid>

DESCRIPTION

Link not configured for sync level 2.

ACTION

None. This message is for information only.

9061:WARNING

Link <linkref> not configured for synclevel 2

DESCRIPTION

Link specified by <linkref> is not configured for sync level 2.

ACTION

None. This message is for information only.

9062:ERROR

Exchange Logs Rejected for <remotesysid>, Restart Type or Log Name Mismatch

DESCRIPTION

The log files for the SNACRM have been incorrectly modified.

ACTION

Run CRMLOGS to examine the SNACRM log file. Cold start the TUXEDO application.

9063:ERROR

Exchange Logs failed with <linkref>

DESCRIPTION

An error occurred during the exchange logs process.

ACTION

Run CRMLOGS to examine the SNACRM log file. Cold start the TUXEDO application.

9064:ERROR

Invalid initial syncpoint received from subordinate, %s

DESCRIPTION

An internal error has occurred during the commit process.

ACTION

Contact BEA Customer Support

Copyright © 1999 BEA Systems, Inc. All Rights Reserved.
Required browser version: Netscape Communicator version 4.0 or higher, or Microsoft Internet Explorer version 4.0 or higher.
Last update: October 1, 1999.