[Top] [Prev] [Next] [Bottom]

# Chapter 1. Introducing BEA Connect SNA

## Features

BEA Connect SNA provides a bidirectional link enabling BEA TUXEDO and IBM mainframe applications to interact as either a client or server, using a Customer Information Control System/Extended System Architecture (CICS/ESA) Distributed Program Link (DPL), Information Management System (IMS) implicit LU6.2, or any IBM-supported Application Program-to-Program Communication (APPC) or Customer Information Control System/Extended System Architecture (CICS/ESA) interface.

BEA Connect SNA version 2.0 offers significant enhancements to prior versions. In summary, these include:

- New Process Architecture incorporating SNA Communication Resource Manager (SNACRM) for InterSystem Communications (ISC) connectivity along with a Process Initialization Server

- Sync-level 2 support enabling transactions between TUXEDO and a mainframe

- Added support for CICS/ESA ISC DPL

- Additional logging and trace files

## Functions

BEA Connect SNA performs the following functions:

- It supports the Application-Transaction Monitor Interface (ATMI) request/response model. Applications running in local TUXEDO System /T domains can request services in a remote domain. The remote domain is a MVS/CICS region. Applications in the remote domain can request services in a local TUXEDO System domain.

- It also supports the ATMI conversational model. Applications can establish a conversation between clients and servers in a TUXEDO System /T domain and an MVS/CICS region defined as a remote domain. Either side can initiate the conversation.

- It performs administration and configuration of a BEA Connect SNA gateway through the DMADM server and DMCONFIG server for a /SNA Domains instantiation.

- It supports the following typed buffers: FML, FML32, VIEW, VIEW32, X_COMMON, STRING, C_ARRAY, and X_OCTET. All buffer types except C_ARRAY and X_OCTET are converted automatically to and from EBCDIC between TUXEDO and CICS; C_ARRAY and X_OCTET are not converted.

- It maintains connectivity to multiple System Network Architecture (SNA) networks from the local TUXEDO System /T domain.

- It performs conversion between ASCII and EBCDIC encoding.

## Supported Platforms

Table 1-1 lists each UNIX-based platform and corresponding SNA protocol Stack on which BEA Connect SNA 2.0 is supported.

> Table 1-1 Supported Platforms

Operating System Version | Stack Version | TUXEDO Version
--- | --- | ---
HP-UX 10.20 | SNAplus2 5.1 | 6.4
HP-UX 10.20 | SNAplus2 6.0 | 6.4
HP-UX 11.00 | SNAplus2 6.0 | 6.4
AIX 4.2.1 | IBM Comm Server 5.0 | 6.4
Solaris 2.5.1 | DCL SNAP-IX 6.0 | 6.4
Solaris 2.5.1 | SUN Link 9.1 1 | 6.4
Solaris 2.5.1 | Brixton 4.0.1.8 1 | 6.4
Solaris 2.6 | SUN Link 9.1 1 | 6.4
Solaris 2.6 | Brixton 4.0.1.8 1 | 6.4

[Top] [Prev] [Next] [Bottom]