[Table of Contents] [Index] [Previous] [Next] Configuring TUXEDO

# Configuring TUXEDO

This chapter describes how to configure your BEA eLink Adapter for R/3 installation for TUXEDO. It includes the following sections:

- TUXEDO Initialization File

- Creating Queues for ALE

## TUXEDO Initialization File

BEA eLink Adapter for R/3 requires some configuration of the TUXEDO initilization file. For configuration instructions, see the BEA TUXEDO Administrator's Guide for your platform.

BEA eLink Adapter for R/3 provides a semi-configured TUXEDO initialization file, `cr3.ubb`, in the config sub-directory of the BEA eLink Adapter for R/3 installation directory. This `cr3.ubb` file is configured for the BEA eLink Adapter for R/3 servers and it requires further configuration for integration into the global TUXEDO environment. For example, in the GROUPS section of your UBB file, you must define the server group to which the ALE Inbound belongs, such as CR3. See Sample cr3.ubb File for a listing of this file.

Note: ALE Inbound and ALE Outbound use TUXEDO transactions. For these components, you need to create a transaction log (TLOG) using TUXEDO administrative tools. See the BEA TUXEDO Administrator's Guide for your platform.

## Creating Queues for ALE

If TUXEDO applications will be using the ALE Inbound or ALE Outbound features of BEA eLink Adapter for R/3, you will need to create one or more queues to handle IDOC packets. If you are not using these features, you do not need to create additional queues.

For more information about creating and managing queues, see your TUXEDO documentation.

[Table of Contents] [Index] [Previous] [Next]