# Index

## A

absolute OIDs

access to managed objects

through SMUX subagents

access, to MIB objects

specifying in NON_SMUX_PEER entries

actions

executing a command
in response to polling

actions, in polling

syntax of

Agent Integrator

capabilities of
commands
configuration file
configuring for access to agents
functionality of
how to use local polling feature of
re-initializing
setting up
stopping
supported MIB objects
types of agents supported

alarms from local threshold-checking

AND, use in defining polling thresholds

architecture of SNMP

asterisks

use in complex polling rules

## B

bea.asn1

default location of

BEA_PEER_MAX_TRIES

BEA_PEER_MAX_WAIT

BEA_SM_BEAMGR_CONF

BEA_SMUX_PASSWD

beaDfAvail

beaDfCapacity

beaDfFilesystem

beaDfHostname

beaDfIndex

beaDfKbytes

beaDfMounted

beaDfTable

beaDfUsed

beaIntAgtRuleAction

beaIntAgtRuleId

beaIntAgtScanIntvl

beaIntAgtStatus MIB object

beaIntAgtTable

role of

beaLclDfAvail

beaLclDfCapacity

beaLclDfFilesystem

beaLclDfKbytes

beaLclDfMountedon

beaLclDfTable

beaLclDfUsed

beamgr.conf

beamgr_snmpd.conf

beaMqCbytes

beaMqCgroup

beaMqCreator

beaMqCtime

beaMqGroup

beaMqId

beaMqKey

beaMqLrpid

beaMqLspid

beaMqMode

beaMqOwner

beaMqQbytes

beaMqQnum

beaMqRtime

beaMqStime

beaMqT

beaNTSysPerf MIB group

beaNTSysPerfAlignFix

beaNTSysPerfCacheBytes

beaNTSysPerfCacheRes

beaNTSysPerfCalls

beaNTSysPerfCodeRes

beaNTSysPerfCodeTotal

beaNTSysPerfDriverRes

beaNTSysPerfDriverTotal

beaNTSysPerfExptDisp

beaNTSysPerfFloatEmul

beaNTSysPerfPagePeak

beaNTSysPerfPageUsed

beaNTSysPerfPaging

beaNTSysPerfPgFaults

beaPsCmd

beaPsCpu

beaPsCpuTime

beaPsDate

beaPsHandleCount

beaPsMem

beaPsPid

beaPsRss

beaPsSize

beaPsStat

beaPsTable

beaPstatSwapAlloc

beaPstatSwapAvail

beaPstatSwapReser

beaPstatSwapUsed

beaPsThreadCount

beaPsTty

beaPsUser

beaSemCgroup

beaSemCtime

beaSemGroup

beaSemId

beaSemKey

beaSemMode

beaSemNsems

beaSemOtime

beaSemOwner

beaSemT

beaSemTable

beaShmAtime

beaShmCgroup

beaShmCpid

beaShmCreator

beaShmCtime

beaShmDtime

beaShmGroup

beaShmId

beaShmKey

beaShmLpid

beaShmMode

beaShmNattch

beaShmOwner

beaShmSegsz

beaShmT

beaSmgrAuxSize

beaSmgrCreationDate

beaSmgrCurrentShmEntries

beaSmgrHWMPctShmUsed

beaSmgrHWMShmUsed

beaSmgrIndex

beaSmgrIpcKey

beaSmgrLibVersion

beaSmgrMaxShmEntries

beaSmgrPctShmUsed

beaSmgrSemId

beaSmgrShmAllocated

beaSmgrShmId

beaSmgrSubsystem

beaSmgrTable

beaSmgrTotalShmSize

beaSmgrUsegSize

beaSysAgentVersion

beaSysContact

beaSysDescr

beaSysHasDisk

beaSysId

beaSysInstallTime

beaSysLocation

beaSysMachine

beaSysName

beaSysNodeName

beaSysPerf MIB group

beaSysPerfCntxt

beaSysPerfCntxtDelta

beaSysPerfCpu

beaSysPerfDisk

beaSysPerfDiskDelta

beaSysPerfIfCollisions

beaSysPerfIfCollisionsDelta

beaSysPerfIfDescr

beaSysPerfIfIndex

beaSysPerfIfInErrors

beaSysPerfIfInErrorsDelta

beaSysPerfIfInPackets

beaSysPerfIfNumber

beaSysPerfIfOperStatus

beaSysPerfIfOutErrors

beaSysPerfIfOutErrorsDelta

beaSysPerfIfOutPackets

beaSysPerfIfOutPacketsDelta

beaSysPerfIfPacketsDelta

beaSysPerfIfTable

beaSysPerfIntr

beaSysPerfIntrDelta

beaSysPerfLoad

beaSysPerfLoadDelta

beaSysPerfPage

beaSysPerfPageDelta

beaSysPerfSwap

beaSysPerfSwapDelta

beaSysRelease

beaSysServices

beaSysSysName

beaSystem MIB group

objects in

beaSysVersion

beaTrapDescr

beaTrapHost

beaTrapPort

beaUnix MIB group

## C

columnar object

what it is

COMMAND_ERR

COMMAND_OK

commands

as an action in polling
specifying more than one

community strings

configuring Agent Integrator to use with agents
specifying in passwords file

compilation

of MIB on management platform

condition

syntax for

conditions, complex

conditions, simple

configuration file

environment variable for
for Agent Integrator
for BEA Manager

configuring for access to agents

## D

data types

for polling conditions
in polling thresholds

disk accesses

monitoring on Windows NT systems

dot-dot notation

DPI

subagents

## E

em_snmpd

MIB groups supported by

em_snmpd, MIB groups supported by

enterprise OID

in traps generated by local polling

environment variables

summary of

ERR state of a polling rule

## F

file system attributes

as MIB table

file systems, local

as MIB objects

## H

host contact person

MIB object for

hostname

as MIB object

## I

instance

of a managed object

instance index

in an OID

INTEGRATOR_MAX_TIMEOUTS entry

INTEGRATOR_TIMEOUT

interfaces

features of that can be polled with beaSysPerf MIB group

IP address

specifying for remote agents
use by Integrator in managing remote agents
use for access to remote agents
use in polling thresholds

IP addresses

used by Agent Integrator

ISO

## L

location, of system

as MIB object

logical agent name

defining

## M

managed objects

configuring Agent Integrator access to
making accessible to Agent Integrator
what they are

managed resource

what it is

Management Information Base

See MIB

master agents

message queue table

as MIB table

MIB

for BEA Manager agents
role in system management
what it does

MIB file, for TUXEDO

default location of

MIB groups

in BEA Agent MIB
supported by subagents

MIB objects

directly supported by Agent Integrator

## N

network management platforms

role of

NON_SMUX PEER

configuring Agent Integrator for

NON_SMUX_PEER entries

in configuration file
role of

NON_SMUX_PEER entry

syntax of

NT, Windows

MIB objects specific to
polling for memory thrashing on
system performance attributes of as MIB objects

## O

object identifier

See OID

OID

expressing with textual names
format of in specifying objects to be polled
relative and absolute
use with Agent Integrator polling rules
what it is

OID tree

what it is
when agents overlap in

OID_CLASS entry

syntax of

OK state of a polling rule

## P

page faults

as MIB objects

password, of SMUX agents

environment variable for

passwords file

peer SNMP agents

use in polling

polling

a specific instance
activating or de-activating
availability of MIB objects for
data types in
how to de-activate
re-activating
relations for defining thresholds in
starting
use of deltas in
use of peer SNMP agents in

polling interval

as MIB object

polling rules

as MIB objects
creating through a manager
deleting or modifying
for Agent Integrator

polling, by Agent Integrator

how to use
of agents on remote nodes

port

specifying for peer agents

port 161

use of for peer SNMP agents

priority

of agent access to MIB objects
of SMUX subagents
setting
use in resolving overlap in agent OID registration

processes, attributes of

as objects in MIB process table

## R

read-write access to MIB objects

reinit_agents

relations

use of defining thresholds

relative OIDs

remote nodes

managing agents on

retries

environment variable for

RFC 1227

RULE_ACTION entry

syntax of

rules, for polling

## S

scalar object

what it is

semaphores

as MIB objects

SET

used to turn off polling

set up

of Agent Integrator

shared memory, attributes of

as MIB objects
as MIB table

Simple Network Management

See SNMP

SMUX

automatic registration of OID tree under
what it is

SMUX subagent passwords

specifying in passwords file

SMUX subagents

modifying management scope of
registration of managed objects with master

SNMP agents

more than one on a single host
on multiple nodes
use in Integrator polling

SNMP agents, managing

on remote nodes

SNMP architecture

SNMP trap notification

TRAP_HOST determines destination of

SNMP traps

SQL database, agents for

state, change of

in polling

states

of polling rules

status, of polling rules

as MIB object

stop_agents command

stopping agents

subagents

use in polling

support

customer
documentation

support, customer

support, documentation

swap space

attributes of as MIB objects

swap space statistics

as MIB objects

syntax

of actions when polling
of NON_SMUX_PEER entry
of OID_CLASS entry
of RULE_ACTION entry

SYS_CONTACT

SYS_DESCR

SYS_INSTALL

SYS_LOCATION

SYS_NAME

SYS_SERVICES

SYSOBJID

SYSSERVICES

system attributes

as MIB objects

system statistics

as MIB objects

## T

timeout

environment variable for
for replies to Agent Integrator from SNMP agents

TMAGENT entry

TMEVENT_FILTER entry

transition

of polling rules
what it is

trap destination

as MIB object

trap notification

what it is

TRAP_HOST entry

components making use of
more than one allowed

TRAPID_ERR

TRAPID_OK

traps

sending to multiple destinations

traps, enterprise-specific

use in polling

traps, polling

information passed in

TUXEDO event filters

TUXEDO system events

subscribing for

## U

unix_snmpd

configuration file keywords used by
MIB groups supported by

unsolicited messages from agents

## V

VAL, use of in defining thresholds

variable bindings

of trap generated by Agent Integrator

variable bindings, of Agent Integrator traps

information in

## W

wildcards

use in OIDs

Windows NT

see also NT, Windows