Overview | Package | Class | Use | Tree | Deprecated | Index | Help
|  | BEA Systems, Inc.
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I K L M N O P Q R S T U V W X

## P

parseHex(String) - Static method in class com.connecterra.ale.reader.access.DeviceTagReport
  Parses the hex string passed in as a raw binary EPC value, returning a DeviceTagReport with no opReports.
PASSWORD - Static variable in interface com.connecterra.ale.dynamicconfig.api.PluginParameterMeta.Type
  This is also a string parameter.
PasswordDeviceOpReport - Class in com.connecterra.ale.reader.access
  Report from issuing an access password to a tag.
PasswordDeviceOpReport(OpStatus) - Constructor for class com.connecterra.ale.reader.access.PasswordDeviceOpReport
  Creates a new `PasswordDeviceOpReport` instance
PasswordDeviceOpSpec - Class in com.connecterra.ale.reader.access
  Operate on a tag by transitioning into the "secured" state.
PCSPEC - Static variable in class com.bea.rfid.edge.toolkit.workflow.SimpleOneWayPortType
  Type that sends/receives objects of type `com.connecterra.alepc.api.PCSpec`.
PCWRITE_REPORT - Static variable in class com.bea.rfid.edge.toolkit.workflow.SimpleOneWayPortType
  Type that sends/receives objects of type `com.connecterra.alepc.api.PCWriteReport`.
PeriodicEvent - Class in com.connecterra.util.event
  Like `Event`, except used as the base class for periodically executed event handlers.
PeriodicEvent() - Constructor for class com.connecterra.util.event.PeriodicEvent
PhysicalDevice - Interface in com.connecterra.ale.reader
  All physical devices must implement this interface.
PluginConfig - Class in com.connecterra.ale.dynamicconfig.api
  Models plugin instance in the edge server.
PluginConfig() - Constructor for class com.connecterra.ale.dynamicconfig.api.PluginConfig
PluginConfigParameter - Class in com.connecterra.ale.dynamicconfig.api
  Models an individual parameter contained within a `PluginConfig`.
PluginConfigParameter() - Constructor for class com.connecterra.ale.dynamicconfig.api.PluginConfigParameter
PluginException - Exception in com.connecterra.ale.dynamicconfig.api
  Root exception type for all Dynamic Configuration API exceptions.
PluginException() - Constructor for exception com.connecterra.ale.dynamicconfig.api.PluginException
  Constructs a `PluginException` with no detail message or cause.
PluginException(String) - Constructor for exception com.connecterra.ale.dynamicconfig.api.PluginException
  Constructs a `PluginException` with the specified detail message.
PluginException(Throwable) - Constructor for exception com.connecterra.ale.dynamicconfig.api.PluginException
  Constructs a `PluginException` with the specified causing exception and a detail message from the causing exception.
PluginException(String, Throwable) - Constructor for exception com.connecterra.ale.dynamicconfig.api.PluginException
  Constructs a `PluginException` with the specified detail message.
PluginMeta - Interface in com.connecterra.ale.dynamicconfig.api
  Models a plugin type in the edge server.
PluginMeta.Role - Interface in com.connecterra.ale.dynamicconfig.api
  Plugin roles supported by the configuration framework.
PluginParameterConstraint - Interface in com.connecterra.ale.dynamicconfig.api
  Base interface for constraints on parameter values.
PluginParameterConstraintDynamicSet - Interface in com.connecterra.ale.dynamicconfig.api
  Used to specify a constraint that is a set of values that is dynamically computed.
PluginParameterConstraintEnum - Interface in com.connecterra.ale.dynamicconfig.api
  Constraint used to restrict a configuration parameter value to a predefined set of string values.
PluginParameterConstraintRangeNumeric - Interface in com.connecterra.ale.dynamicconfig.api
  Restricts a parameter value within a numeric range (inclusive).
PluginParameterMeta - Interface in com.connecterra.ale.dynamicconfig.api
  Describes a configuration parameter of a plugin.
PluginParameterMeta.Type - Interface in com.connecterra.ale.dynamicconfig.api
  Supported parameter types.
populateAbstractEPCISEvent(AbstractEPCISEvent) - Method in class com.bea.rfid.workflow.epcis.EventGenerator
  Populates common EPCIS event fields using the event field properties on this.
Port - Interface in com.bea.rfid.edge.api.workflow
  Represents an input or output port of a module.
PortImpl - Class in com.bea.rfid.edge.toolkit.workflow
  Simple implementation of `Port` interface.
PortImpl(String, String, PortType) - Constructor for class com.bea.rfid.edge.toolkit.workflow.PortImpl
  Constructor.
PortType - Interface in com.bea.rfid.edge.api.workflow
  Holds information about what type of messages a port may send or accept.
print(String) - Method in class com.bea.rfid.workflow.print.PrintTag
  Prints an EPC based on the input string.
print(PollingDeviceUnit, long[], Long, Long, Long, Long, Long, Map) - Method in class com.connecterra.ale.reader.AbstractPrinterPhysicalReader
  This method should print a tag.
PRINTER_ACCESS_PASSWORD - Static variable in class com.connecterra.ale.reader.DeviceCapabilities
  This capability indicates that an rfid printer is capable of using an access password to write to or kill a locked tag.
PRINTER_KILL_PASSWORD - Static variable in class com.connecterra.ale.reader.DeviceCapabilities
  This capability indicates that an rfid printer is capable of killing a tag.
PRINTER_LOCK_BITS - Static variable in class com.connecterra.ale.reader.DeviceCapabilities
  This capability indicates that an rfid printer is capable of locking a tag.
PrintObserver - Interface in com.bea.rfid.workflow.print
  Interface that must be implemented by classes that should process callbacks from `PrintTag`.
printSetup(String) - Method in class com.bea.rfid.workflow.print.PrintTag
  This method should be used to set up PCSpec for the input EPC class.
PrintTag - Class in com.bea.rfid.workflow.print
  Java class for programing tags for specified EPC class or with the specified EPC.
PrintTag(ALEPC, ALEPCFactory, Timer) - Constructor for class com.bea.rfid.workflow.print.PrintTag
  Constructor.
processECReports(ECReports) - Method in class com.bea.rfid.workflow.util.Directionality
  Looks in the input ECReports to find out which tags were seen or disappeared from each point to determine the directionality of tags.
processMessage(Object) - Method in class com.bea.rfid.edge.toolkit.workflow.AbstractWorkflowModulePlugin.OneWayInputPortImpl
  The method that does the actual work of processing the message.
processOpSpecs(AbstractPhysicalDevice.TagProcessor, List) - Method in class com.connecterra.ale.reader.AbstractPhysicalDevice
  Execute the opSpecs on a single TagProcessor.
PURCHASED_FROM_GLN_AI - Static variable in class com.bea.rfid.workflow.util.BarcodeDecoder

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| Documentation is available at ${DOCSWEBROOT} Copyright 2007 BEA Systems Inc.
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I K L M N O P Q R S T U V W X