Overview | Package | Class | Use | Tree | Deprecated | Index | Help
|  | BEA Systems, Inc.
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I K L M N O P Q R S T U V W X

## I

I18N_INPUT_PORTS_PARAM_GROUP - Static variable in class com.bea.rfid.edge.toolkit.workflow.AbstractWorkflowModulePlugin
  Internationalized name of the plugin configuration parameter that groups input ports.
I18N_OUTPUT_PORTS_PARAM_GROUP - Static variable in class com.bea.rfid.edge.toolkit.workflow.AbstractWorkflowModulePlugin
  Internationalized name of the plugin configuration parameter that groups output ports.
ID_OF_PHYSICAL_LOCATION_GLN_AI - Static variable in class com.bea.rfid.workflow.util.BarcodeDecoder
ID_PAT_URI_HEADER - Static variable in class com.bea.rfid.workflow.util.BarcodeDecoder
IDLE - Static variable in class com.bea.rfid.api.workflow.types.WorkflowModuleState
  A module that is not processing its inputs is in this state.
INACTIVE - Static variable in class com.connecterra.ale.reader.ChannelManager.State
  Communications with the device are offline.
INCOMPATIBLE_TAG_TYPE - Static variable in class com.connecterra.ale.reader.OpStatus
  The tag value to be written is not compatible with the tag type (or the reader type).
initialize(String, WorkflowManager) - Method in interface com.bea.rfid.edge.api.workflow.WorkflowModulePlugin
  This method should take care of any initializations that should happen in the module before it is configured or started up.
initialize(String, WorkflowManager) - Method in class com.bea.rfid.edge.toolkit.workflow.AbstractWorkflowModulePlugin
  Interface method implementation.
initialize(PluginConfig) - Method in class com.connecterra.ale.reader.AbstractPhysicalDevice
initialize() - Method in interface com.connecterra.ale.reader.ChannelManager.Proxy
  Called after the channels are all activated, this method should perform any necessary initialization, such as setting listeners, authenticating to a device, and setting up current application state on the device.
initializeSession() - Method in class com.connecterra.ale.reader.AbstractPhysicalDevice
initializeSession(AbstractPhysicalDevice.Requests) - Method in class com.connecterra.ale.reader.AbstractPhysicalDevice
INPUT_PORT - Static variable in class com.bea.rfid.api.workflow.config.DynamicSetConstants.DynamicSetID
  Dynamic set identifier for input ports of edge flow modules.
INPUT_PORTS_PARAM_GROUP - Static variable in class com.bea.rfid.edge.toolkit.workflow.AbstractWorkflowModulePlugin
  Name of the plugin configuration parameter that groups all input ports together.
INTEGER - Static variable in class com.bea.rfid.edge.toolkit.workflow.SimpleOneWayPortType
  Type that sends/receives objects of type `Integer`.
InvalidBarcodeException - Exception in com.bea.rfid.workflow.util
  Exception declaring problem with barcode decoding
InvalidBarcodeException() - Constructor for exception com.bea.rfid.workflow.util.InvalidBarcodeException
InvalidBarcodeException(String) - Constructor for exception com.bea.rfid.workflow.util.InvalidBarcodeException
InvalidBarcodeException(Throwable) - Constructor for exception com.bea.rfid.workflow.util.InvalidBarcodeException
InvalidBarcodeException(String, Throwable) - Constructor for exception com.bea.rfid.workflow.util.InvalidBarcodeException
inventoryTagsInField(Set) - Method in class com.connecterra.ale.reader.AbstractDispatchingPollingPhysicalDevice
  Inventory all the tags for the device units specified.
INVOICE_GLN_AI - Static variable in class com.bea.rfid.workflow.util.BarcodeDecoder
isActive() - Method in class com.bea.rfid.workflow.util.Accumulator
  Returns boolean indicating if this is active or not.
isAllowExtraChildren() - Method in class com.bea.rfid.workflow.epcis.AggregationReconciler
  Returns boolean value that indicates if extra children in input aggregation should result in matched children value of false.
isForceAFI() - Method in class com.connecterra.ale.reader.AbstractPhysicalDevice
isMatchEPCParent() - Method in class com.bea.rfid.workflow.epcis.AggregationReconciler
  Returns true if parent value in aggregation should be compared when the expected parent is an EPC value.
isMatchNonEPCParent() - Method in class com.bea.rfid.workflow.epcis.AggregationReconciler
  Returns true if parent value in aggregation should be compared when the expected parent is not an EPC value.
isNamedField(String) - Method in class com.connecterra.ale.uri.TagMemoryURI
  If this is a reference to a memory by symbolic name, returns true if `name` equals the symbolic name.
isNumericBank() - Method in class com.connecterra.ale.uri.TagMemoryURI
isProcessing() - Method in class com.bea.rfid.workflow.epcis.EventGenerator
  Returns boolean indicating if the event generator is in active state or not.
isReadAFI() - Method in class com.connecterra.ale.reader.AbstractPhysicalDevice
isRequired() - Method in interface com.connecterra.ale.dynamicconfig.api.PluginParameterMeta
  Returns true if this is a required parameter, false otherwise.
isRestrictSingleTag() - Method in class com.connecterra.ale.reader.DeviceUnitRequest
  If true, then the `DeviceUnitRequest` should fail if more than one tag would be operated on.
isRunning() - Method in class com.bea.rfid.workflow.util.Directionality
  Returns boolean indicating if this is in the state in which it processes inputs to determine directionality.
isStopOnError() - Method in class com.connecterra.ale.reader.DeviceUnitRequest
  If true, then the `DeviceUnitRequest` should stop immediately if one of the DeviceOpSpecs fails.
isStoppingCondition() - Method in class com.connecterra.ale.reader.OpStatus
  Tells whether this write cycle failure status is a "hard" failure, meaning that it is pointless to try to repeat the write cycle on the reporting logical reader.
isSymbolic() - Method in class com.connecterra.ale.uri.TagMemoryURI
isWirableFrom(PortType) - Method in interface com.bea.rfid.edge.api.workflow.PortType
  Determines whether it is valid to connect the given `PortType` to this.
isWirableFrom(PortType) - Method in class com.bea.rfid.edge.toolkit.workflow.AnyPortType
  Interface method implementation.
isWirableFrom(PortType) - Method in class com.bea.rfid.edge.toolkit.workflow.ListOneWayPortType
isWirableFrom(PortType) - Method in class com.bea.rfid.edge.toolkit.workflow.MultiTypeOneWayPortType
isWirableFrom(PortType) - Method in class com.bea.rfid.edge.toolkit.workflow.SimpleOneWayPortType
  Interface method implementation.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| Documentation is available at ${DOCSWEBROOT} Copyright 2007 BEA Systems Inc.
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I K L M N O P Q R S T U V W X