Overview | Package | Class | Use | Tree | Deprecated | Index | Help
|  | BEA Systems, Inc.
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I K L M N O P Q R S T U V W X

## W

waitForShutdown(long) - Method in class com.connecterra.ale.reader.AbstractPhysicalDevice
waitForShutdown(long) - Method in interface com.connecterra.util.Controllable
  Wait for the shutdown process initiated by `Controllable.shutdown()` to complete.
waitForTermination(long) - Method in class com.connecterra.ale.reader.AbstractPhysicalDevice
waitForTermination(long) - Method in interface com.connecterra.util.Controllable
  Wait for the termination process initiated by `Controllable.terminate()` to complete.
WORKFLOW_MODULE - Static variable in interface com.connecterra.ale.dynamicconfig.api.PluginMeta.Role
  Role for edge flow plugins.
WorkflowManager - Interface in com.bea.rfid.edge.api.workflow
  Edge flow manager interface used by the edge server to define, reconfigure or delete edge flow modules.
WorkflowModulePlugin - Interface in com.bea.rfid.edge.api.workflow
  Interface representing an edge flow plugin in the edge server.
WorkflowModuleState - Class in com.bea.rfid.api.workflow.types
  Enum class representing the different states of an edge flow module.
WorkflowNamingService - Interface in com.bea.rfid.edge.api.workflow
  Interface to get to workflow related objects like workflow modules and serializers and deserializers for the different types.
WORKING - Static variable in class com.bea.rfid.api.workflow.types.WorkflowModuleState
  A module that is actively processing inputs that it receives is in this state.
WriteDeviceOpReport - Class in com.connecterra.ale.reader.access
  Report from a tag write operation.
WriteDeviceOpReport(OpStatus, long[]) - Constructor for class com.connecterra.ale.reader.access.WriteDeviceOpReport
  Creates a new `WriteDeviceOpReport` instance.
WriteDeviceOpReport(OpStatus, long, long) - Constructor for class com.connecterra.ale.reader.access.WriteDeviceOpReport
  Creates a new `WriteDeviceOpReport` instance.
WriteDeviceOpReport(OpStatus) - Constructor for class com.connecterra.ale.reader.access.WriteDeviceOpReport
  Creates a new `WriteDeviceOpReport` instance.
WriteDeviceOpSpec - Class in com.connecterra.ale.reader.access
  Base class which represents write operations on tags
writeEPC(long[]) - Method in interface com.connecterra.ale.reader.AbstractPhysicalDevice.EPCglobalTagWriteProcessor
  Writes the provided EPC data to the associated tag.
WriteEPCCacheDeviceOpSpec - Class in com.connecterra.ale.reader.access
  Operate on a tag by writing to the EPC bank using a value from an EPC Cache.
WriteLiteralDeviceOpSpec - Class in com.connecterra.ale.reader.access
  Operate on a tag by writing a literal value to a given memory bank.
writeMemoryBank(String, int, int, long[]) - Method in interface com.connecterra.ale.reader.AbstractPhysicalDevice.BankWriteTagProcessor
WRITING - Static variable in class com.connecterra.ale.reader.DeviceUnitCapabilities
  This capability indicates that the device is capable of writing.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| Documentation is available at ${DOCSWEBROOT} Copyright 2007 BEA Systems Inc.
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I K L M N O P Q R S T U V W X