Overview | Package | Class | Use | Tree | Deprecated | Index | Help
|  | BEA Systems, Inc.
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD

## com.connecterra.ale.reader
Interface AbstractPhysicalDevice.EPCglobalTagWriteProcessor

All Known Subinterfaces:
  AbstractPhysicalDevice.EPCglobalClass1Gen2TagProcessor, AbstractPhysicalDevice.EPCglobalTagProcessor

Enclosing class:
  AbstractPhysicalDevice

    public static interface AbstractPhysicalDevice.EPCglobalTagWriteProcessor

`TagProcessors` should implement this interface if the device has the capability of modifying the associated tag's EPC value.

Method Summary
`WriteDeviceOpReport` | `writeEPC(long[] writeData)` Writes the provided EPC data to the associated tag.

Method Detail

### writeEPC

    WriteDeviceOpReport writeEPC(long[] writeData)
                                 throws IOException,
                                        AbstractPhysicalDevice.TagResultException

  Writes the provided EPC data to the associated tag.

  Parameters:
    `writeData` - a long[2] that contains the EPC data to be written to the associated tag. This value is either 64, 96, or 128 bits long, stored "right-justified", i.e. prefaced with 0 bits, within the array. When writing a 64-bit tag value, writeData[0] equals 0L.
  Returns:
    the WriteDeviceOpReport that contains the results of the operation
  Throws:
    `IOException` - if there is an IO error attempting to communicate with the device
    `AbstractPhysicalDevice.TagResultException` - if there is an error writing the value to the tag. See `AbstractPhysicalDevice.TagResultException`.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| Documentation is available at ${DOCSWEBROOT} Copyright 2007 BEA Systems Inc.
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD