Overview | Package | Class | Use | Tree | Deprecated | Index | Help
|  | BEA Systems, Inc.
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I K L M N O P Q R S T U V W X

## M

m_addReportsPointA - Variable in class com.bea.rfid.workflow.util.Directionality
m_addReportsPointB - Variable in class com.bea.rfid.workflow.util.Directionality
m_channelManager - Variable in class com.connecterra.ale.reader.AbstractPhysicalDevice
m_deleteReportsPointA - Variable in class com.bea.rfid.workflow.util.Directionality
m_deleteReportsPointB - Variable in class com.bea.rfid.workflow.util.Directionality
m_deviceUnit - Variable in class com.connecterra.ale.reader.AbstractPhysicalDevice.TagData
m_filters - Variable in class com.connecterra.ale.reader.DefaultLogicalReader
m_logicalReaderName - Variable in class com.connecterra.ale.reader.DefaultLogicalReader
m_physicalDevice - Variable in class com.connecterra.ale.reader.DefaultLogicalReader
m_readCycleCount - Variable in class com.connecterra.ale.reader.DefaultLogicalReader
m_readCyclesTelemetryID - Variable in class com.connecterra.ale.reader.DefaultLogicalReader
m_tagsInFieldGauge - Variable in class com.connecterra.ale.reader.DefaultLogicalReader
m_tagsInFieldTelemetryID - Variable in class com.connecterra.ale.reader.DefaultLogicalReader
m_telemetryDeviceName - Variable in class com.connecterra.ale.reader.DefaultLogicalReader
m_writeCycleCount - Variable in class com.connecterra.ale.reader.DefaultLogicalReader
m_writeCyclesTelemetryID - Variable in class com.connecterra.ale.reader.DefaultLogicalReader
Manifest - Interface in com.bea.rfid.api.workflow.types
  Interface representing the manifest (parent and children identifiers expected) for an aggregation.
MANIFEST - Static variable in class com.bea.rfid.edge.toolkit.workflow.SimpleOneWayPortType
  Type that sends/receives objects of type `Manifest`.
markUsed() - Method in class com.connecterra.ale.reader.DeviceChannel
  This method must be invoked by the channel whenever data is received on the channel.
MessageDeserializer - Interface in com.bea.rfid.api.workflow.encoding
  Interface that must be implemented by edge flow message deserializers for messages should be automatically deserialized by the framework.
MessageSerializer - Interface in com.bea.rfid.api.workflow.encoding
  Interface that must be implemented by edge flow message serializers for messages should be automatically serialized by the framework.
MODULE_STATE - Static variable in class com.bea.rfid.edge.toolkit.workflow.SimpleOneWayPortType
  Type that sends/receives objects of type `WorkflowModuleState`.
ModuleDescriptor - Interface in com.bea.rfid.edge.api.workflow
  Contains information about about a module's input and output ports.
ModuleDescriptorImpl - Class in com.bea.rfid.edge.toolkit.workflow
  A simple implementation of `ModuleDescriptor`.
ModuleDescriptorImpl(List, List) - Constructor for class com.bea.rfid.edge.toolkit.workflow.ModuleDescriptorImpl
  Constructor.
MULTIPLE_IN_FIELD - Static variable in class com.connecterra.ale.reader.OpStatus
  No write was attempted because there were multiple tags in the field.
MultiTypeOneWayPortType - Class in com.bea.rfid.edge.toolkit.workflow
  Represents the type of a one-way `Port` that accepts/sends multiple types of input.
MultiTypeOneWayPortType(PortType[], String) - Constructor for class com.bea.rfid.edge.toolkit.workflow.MultiTypeOneWayPortType
  Constructor.
MultiTypeOneWayPortType(Set, String) - Constructor for class com.bea.rfid.edge.toolkit.workflow.MultiTypeOneWayPortType
  Constructor.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| Documentation is available at ${DOCSWEBROOT} Copyright 2007 BEA Systems Inc.
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I K L M N O P Q R S T U V W X