Overview | Package | Class | Use | Tree | Deprecated | Index | Help
|  | BEA Systems, Inc.
PREV NEXT | FRAMES NO FRAMES

## Uses of Class
com.connecterra.ale.reader.OpStatus

Packages that use OpStatus
com.connecterra.ale.reader |
com.connecterra.ale.reader.access |

Uses of OpStatus in com.connecterra.ale.reader

Fields in com.connecterra.ale.reader declared as OpStatus
`static OpStatus` | `OpStatus.ANTENNA_FAILURE` Write operation failed because the specified antenna was not present.
`static OpStatus` | `OpStatus.BUSY` The reader could not be write-subscribed because it is already subscribed for a write operation.
`static OpStatus` | `OpStatus.CACHE_EMPTY` Write operation failed because the cache was empty.
`static OpStatus` | `OpStatus.COMMUNICATION_FAILURE` Value indicating error establishing or maintaining communications with the reader.
`static OpStatus` | `OpStatus.DRIVER_INCAPABLE` Write operation failed because the specified antenna could not perform the requested operation.
`static OpStatus` | `OpStatus.FAILED` Value indicating that a logical reader is non-functional.
`static OpStatus` | `OpStatus.INCOMPATIBLE_TAG_TYPE` The tag value to be written is not compatible with the tag type (or the reader type).
`static OpStatus` | `OpStatus.LOCKED` No write was attempted because the tag is locked.
`static OpStatus` | `OpStatus.MULTIPLE_IN_FIELD` No write was attempted because there were multiple tags in the field.
`static OpStatus` | `OpStatus.NONE_IN_FIELD` The reader did not find any tag in the field.
`static OpStatus` | `OpStatus.NOT_WRITTEN` There was a single tag in the field, but its value was not altered by the write operation.
`static OpStatus` | `OpStatus.OK` Value indicating that the write cycle was successful.
`static OpStatus` | `OpStatus.READ_ONLY` No write was attempted because the tag is not a programmable type.
`static OpStatus` | `OpStatus.STOPPED` The write operation was stopped by program action prior to completion.
`static OpStatus` | `OpStatus.UNKNOWN` sentinel used within ProgrammingCycle logic to indicate that no status report or cycle completion report has been received from a reader
`static OpStatus` | `OpStatus.VERIFY_ERROR` After the write operation, the tag in field reads back with an invalid value (CRC problem) or a value different than the value that was written to it.

Methods in com.connecterra.ale.reader that return OpStatus
`OpStatus` | `AbstractPhysicalDevice.TagResultException.getOpStatus()`

Constructors in com.connecterra.ale.reader with parameters of type OpStatus
`AbstractPhysicalDevice.TagResultException(OpStatus opStatus, String failureInfo)`

Uses of OpStatus in com.connecterra.ale.reader.access

Methods in com.connecterra.ale.reader.access that return OpStatus
`OpStatus` | `DeviceTagReport.getOpStatus()`

Methods in com.connecterra.ale.reader.access with parameters of type OpStatus
`static com.connecterra.alepc.api.PCStatus` | `DeviceOpReport.opStatusToPCStatus(OpStatus opstat)` Helper method to convert driver-level `OpStatus` to an API-level `PCStatus`.
`void` | `DeviceTagReport.setDeviceOpReports(List deviceOpReports, OpStatus opStatus, String failureInfo)` Set the List of DeviceOpReports.

Constructors in com.connecterra.ale.reader.access with parameters of type OpStatus
`KillDeviceOpReport(OpStatus status)` Creates a new `KillDeviceOpReport` instance
`LockDeviceOpReport(OpStatus status)` Creates a new `LockDeviceOpReport` instance
`PasswordDeviceOpReport(OpStatus status)` Creates a new `PasswordDeviceOpReport` instance
`ReadDeviceOpReport(OpStatus status)` Creates a new `ReadDeviceOpReport` instance.
`ReadDeviceOpReport(OpStatus status, long[] data)` Creates a new `ReadDeviceOpReport` instance.
`ReadDeviceOpReport(OpStatus status, long[] data, int afi, int dataLength)`
`ReadDeviceOpReport(OpStatus status, long msWord, long lsWord)` Creates a new `ReadDeviceOpReport` instance.
`ReadDeviceOpReport(OpStatus status, URI field, long[] data, int afi, int dataLength)`
`WriteDeviceOpReport(OpStatus status)` Creates a new `WriteDeviceOpReport` instance.
`WriteDeviceOpReport(OpStatus status, long[] data)` Creates a new `WriteDeviceOpReport` instance.
`WriteDeviceOpReport(OpStatus status, long msWord, long lsWord)` Creates a new `WriteDeviceOpReport` instance.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| Documentation is available at ${DOCSWEBROOT} Copyright 2007 BEA Systems Inc.
PREV NEXT | FRAMES NO FRAMES