Overview | Package | Class | Use | Tree | Deprecated | Index | Help
|  | BEA Systems, Inc.
PREV NEXT | FRAMES NO FRAMES

## Uses of Interface
com.connecterra.ale.dynamicconfig.api.DynamicConfigFactory

Packages that use DynamicConfigFactory
com.bea.rfid.edge.toolkit.workflow | This class contains abstract classes and helper classes for writing edge flow modules.
com.connecterra.ale.dynamicconfig.bean |
com.connecterra.ale.reader |

Uses of DynamicConfigFactory in com.bea.rfid.edge.toolkit.workflow

Methods in com.bea.rfid.edge.toolkit.workflow with parameters of type DynamicConfigFactory
`static PluginParameterMeta` | `AbstractWorkflowModulePlugin.createInputPortsSubConfig(DynamicConfigFactory factory, List ports)` Utility method to create input ports sub-configuration parameter meta.
`protected static PluginParameterMeta` | `AbstractWorkflowModulePlugin.createOutputPortsSubConfig(DynamicConfigFactory factory, List ports)` Utility method to create output ports sub-configuration parameter meta.

Uses of DynamicConfigFactory in com.connecterra.ale.dynamicconfig.bean

Classes in com.connecterra.ale.dynamicconfig.bean that implement DynamicConfigFactory
`class` | `AbstractDynamicConfigFactory` Abstract class that defines the convenience methods in the factory interface using the other required methods in the factory.
`class` | `DynamicConfigBeanFactory` An implementation of `DynamicConfigFactory`.

Uses of DynamicConfigFactory in com.connecterra.ale.reader

Methods in com.connecterra.ale.reader with parameters of type DynamicConfigFactory
`static void` | `AbstractPhysicalDevice.addAFIParametersToPluginMeta(DynamicConfigFactory factory, PluginMeta pm)` Adds the `"Read Tag AFI"` and `"Forced AFI value"` parameters to the PluginMeta.
`static void` | `AbstractPhysicalDevice.addForceAFIParameterToPluginMeta(DynamicConfigFactory factory, PluginMeta pm)` Adds the "Forced AFI value" parameter to the PluginMeta.
`static void` | `AbstractPhysicalDevice.addReadAFIParameterToPluginMeta(DynamicConfigFactory factory, PluginMeta pm)` Adds the "Read Tag AFI" parameter to the PluginMeta.
`static void` | `AbstractPhysicalDevice.addToPluginMeta(DynamicConfigFactory factory, PluginMeta pm)` Adds appropriate PluginParameterMeta objects to the PluginMeta as needed by the framework.
`static void` | `AbstractPrinterPhysicalReader.addToPluginMeta(DynamicConfigFactory factory, PluginMeta pm)`
`static void` | `DeviceUnit.addToPluginMeta(DynamicConfigFactory factory, PluginMeta pluginMeta, String deviceUnitKeyNamePrefix, MessageFormat deviceUnitParameterPattern, int deviceUnitNumber, DeviceUnitCapabilities caps)`
`static void` | `DeviceUnit.addToPluginMeta(DynamicConfigFactory factory, PluginMeta pluginMeta, String deviceUnitKeyNamePrefix, MessageFormat deviceUnitParameterPattern, int deviceUnitNumber, DeviceUnitCapabilities caps, boolean isRequired)` Adds appropriate PluginParameterMeta objects to the PluginMeta as needed by the framework.
`static void` | `SocketAcceptorDeviceChannel.addToPluginMeta(DynamicConfigFactory factory, PluginMeta pm, String portKeyName, String portDisplayName, String defaultPort)` Adds `PluginParameterMeta` to the specified `PluginMeta` for each parameter read by the channel.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| Documentation is available at ${DOCSWEBROOT} Copyright 2007 BEA Systems Inc.
PREV NEXT | FRAMES NO FRAMES