Overview | Package | Class | Use | Tree | Deprecated | Index | Help
|  | BEA Systems, Inc.
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I K L M N O P Q R S T U V W X

## T

TAG_LIST - Static variable in class com.bea.rfid.edge.toolkit.workflow.ListOneWayPortType
  Type that sends or receives Lists containing `com.connecterra.ale.api.ECReportGroupListMember`.
tagAccumulationCompleted(List) - Method in interface com.bea.rfid.workflow.util.AccumulationObserver
  Called by Accumulator to report the completion of an accumulation.
TagListBuilder - Class in com.bea.rfid.workflow.util
  Plain java class that may be used to extract Tags (`com.connecterra.ale.api.ECReportGroupListMember`) from `ECReports` or `PCWriteReport`.
TagListBuilder() - Constructor for class com.bea.rfid.workflow.util.TagListBuilder
  No argument constructor.
TagListBuilder(Set) - Constructor for class com.bea.rfid.workflow.util.TagListBuilder
  Constructor.
TagMemoryURI - Class in com.connecterra.ale.uri
  Parsed representation of a tag memory URI, as used in an ECSpec included memory, or a PCSpec OpRequest.
terminate() - Method in class com.connecterra.ale.reader.AbstractPhysicalDevice
terminate() - Method in class com.connecterra.ale.reader.ChannelManager
  Makes a best-effort attempt to close all the channels.
terminate() - Method in class com.connecterra.ale.reader.DeviceChannel.AbstractOpenChannel
  Makes a best-effort attempt to drop resources in use by the channel.
terminate() - Method in interface com.connecterra.util.Controllable
  Initiate whatever process is necessary to forcibly shut down the subsystem.
TERMINATED - Static variable in class com.connecterra.ale.reader.ChannelManager.State
  The manager enters this state when the system is being shut down.
THROW - Static variable in class com.connecterra.util.event.EventReceiver
toString() - Method in class com.connecterra.ale.reader.AbstractPhysicalDevice
toString() - Method in class com.connecterra.ale.reader.access.DeviceTagReport
toString() - Method in interface com.connecterra.ale.reader.ChannelManager.Proxy
  The ChannelManager uses the toString() method to get a printable name which is used in log messages issued when the channel changes state.
toString() - Method in class com.connecterra.ale.reader.DefaultLogicalReader
toString() - Method in class com.connecterra.ale.reader.DeviceUnit
toString() - Method in class com.connecterra.ale.reader.OpStatus
toString() - Method in class com.connecterra.ale.uri.TagMemoryURI
toString() - Method in class com.connecterra.util.event.EventReceiver
TRIGGER - Static variable in class com.bea.rfid.edge.toolkit.workflow.SimpleOneWayPortType
  Type that sends/receives objects of type `TriggerOutput`.
TRIGGER - Static variable in interface com.connecterra.ale.dynamicconfig.api.PluginMeta.Role
  Role for trigger driver plugins in the edge server.
TriggerOutput - Interface in com.bea.rfid.api.workflow.types
  Represents trigger output generated by trigger receiver modules.
TriggerOutputImpl - Class in com.bea.rfid.edge.toolkit.workflow.types
  An implementation of `TriggerOutput`.
TriggerOutputImpl() - Constructor for class com.bea.rfid.edge.toolkit.workflow.types.TriggerOutputImpl

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| Documentation is available at ${DOCSWEBROOT} Copyright 2007 BEA Systems Inc.
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I K L M N O P Q R S T U V W X