Overview | Package | Class | Use | Tree | Deprecated | Index | Help
|  | BEA Systems, Inc.
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I K L M N O P Q R S T U V W X

## A

AbstractDispatchingPollingPhysicalDevice - Class in com.connecterra.ale.reader
  Adds to AbstractPhysicalDevice support for sequenced polling for inventorying and automatic calls to `AbstractPhysicalDevice.TagProcessor` methods for each method returned from the inventory method.
AbstractDispatchingPollingPhysicalDevice() - Constructor for class com.connecterra.ale.reader.AbstractDispatchingPollingPhysicalDevice
AbstractDynamicConfigFactory - Class in com.connecterra.ale.dynamicconfig.bean
  Abstract class that defines the convenience methods in the factory interface using the other required methods in the factory.
AbstractDynamicConfigFactory() - Constructor for class com.connecterra.ale.dynamicconfig.bean.AbstractDynamicConfigFactory
AbstractEventProcessor - Class in com.connecterra.util.event
  This class encapsulates a common pattern of use of `EventReceiver` and `EventProcessor`.
AbstractEventProcessor.PeriodicEventHandle - Class in com.connecterra.util.event
  This class contains the state for a periodic event.
AbstractEventProcessor.PeriodicEventHandle() - Constructor for class com.connecterra.util.event.AbstractEventProcessor.PeriodicEventHandle
AbstractPhysicalDevice - Class in com.connecterra.ale.reader
  This is the base class for the device driver framework.
AbstractPhysicalDevice() - Constructor for class com.connecterra.ale.reader.AbstractPhysicalDevice
  Creates a new `AbstractPhysicalDevice` instance.
AbstractPhysicalDevice.AFIReadingTagProcessor - Interface in com.connecterra.ale.reader
  A `AbstractPhysicalDevice.TagProcessor` should implement this interface if the device provides special support for efficiently reading the AFI value of a tag that has already been inventoried.
AbstractPhysicalDevice.BankReadTagProcessor - Interface in com.connecterra.ale.reader
  `TagProcessors` should implement this interface if the device can read data from memory banks on the associated tag.
AbstractPhysicalDevice.BankTagProcessor - Interface in com.connecterra.ale.reader
  A convenience interface that combines `AbstractPhysicalDevice.BankReadTagProcessor` and `AbstractPhysicalDevice.BankWriteTagProcessor`
AbstractPhysicalDevice.BankWriteTagProcessor - Interface in com.connecterra.ale.reader
  `TagProcessors` should implement this interface if the device can write data to memory banks on the associated tag.
AbstractPhysicalDevice.EPCglobalClass1Gen2TagProcessor - Interface in com.connecterra.ale.reader
  `TagProcessors` should implement this interface if the device supports full EPCglobal Class 1 Gen 2 tag functionality.
AbstractPhysicalDevice.EPCglobalTagProcessor - Interface in com.connecterra.ale.reader
  A convenience interface that combines `AbstractPhysicalDevice.EPCglobalTagReadProcessor` and `AbstractPhysicalDevice.EPCglobalTagWriteProcessor`
AbstractPhysicalDevice.EPCglobalTagReadProcessor - Interface in com.connecterra.ale.reader
  `TagProcessors` should implement this interface if the object in question is identified by an EPC or otherwise contains an EPC value.
AbstractPhysicalDevice.EPCglobalTagWriteProcessor - Interface in com.connecterra.ale.reader
  `TagProcessors` should implement this interface if the device has the capability of modifying the associated tag's EPC value.
AbstractPhysicalDevice.EPCTagData - Class in com.connecterra.ale.reader
  Base class for TagProcessors that are associated with a DeviceUnit, and which contain DeviceTagReports that always store EPC data as the tag identity.
AbstractPhysicalDevice.EPCTagData(DeviceUnit, DeviceTagReport) - Constructor for class com.connecterra.ale.reader.AbstractPhysicalDevice.EPCTagData
AbstractPhysicalDevice.Requests - Class in com.connecterra.ale.reader
  Represents all of the subscribed `DeviceUnitRequests` on a device, and all the tags which have been reported for any of those DeviceUnitRequests.
AbstractPhysicalDevice.Requests() - Constructor for class com.connecterra.ale.reader.AbstractPhysicalDevice.Requests
AbstractPhysicalDevice.TagData - Class in com.connecterra.ale.reader
  Base class for TagProcessors that are associated with a DeviceUnit
AbstractPhysicalDevice.TagData(DeviceUnit, DeviceTagReport) - Constructor for class com.connecterra.ale.reader.AbstractPhysicalDevice.TagData
AbstractPhysicalDevice.TagProcessor - Class in com.connecterra.ale.reader
  The base class of objects which can be passed to `AbstractPhysicalDevice.processOpSpecs(com.connecterra.ale.reader.AbstractPhysicalDevice.TagProcessor, java.util.List)`.
AbstractPhysicalDevice.TagProcessor() - Constructor for class com.connecterra.ale.reader.AbstractPhysicalDevice.TagProcessor
AbstractPhysicalDevice.TagResultException - Exception in com.connecterra.ale.reader
  This exception should be thrown from a TagProcessor exception with an appropriate OpStatus, and failure info String if the OpStatus is not OK.
AbstractPhysicalDevice.TagResultException(OpStatus, String) - Constructor for exception com.connecterra.ale.reader.AbstractPhysicalDevice.TagResultException
AbstractPollingPhysicalDevice - Class in com.connecterra.ale.reader
  Adds support for sequenced polling to the AbstractPhysicalDevice.
AbstractPollingPhysicalDevice() - Constructor for class com.connecterra.ale.reader.AbstractPollingPhysicalDevice
AbstractPrinterPhysicalReader - Class in com.connecterra.ale.reader
  Base class for rfid printers.
AbstractPrinterPhysicalReader() - Constructor for class com.connecterra.ale.reader.AbstractPrinterPhysicalReader
AbstractWorkflowModulePlugin - Class in com.bea.rfid.edge.toolkit.workflow
  Abstract base class for edge flow modules.
AbstractWorkflowModulePlugin() - Constructor for class com.bea.rfid.edge.toolkit.workflow.AbstractWorkflowModulePlugin
AbstractWorkflowModulePlugin.OneWayInputPortImpl - Class in com.bea.rfid.edge.toolkit.workflow
  Inner class implementation of `OneWayInputPort`.
AbstractWorkflowModulePlugin.OneWayInputPortImpl(String, String, PortType) - Constructor for class com.bea.rfid.edge.toolkit.workflow.AbstractWorkflowModulePlugin.OneWayInputPortImpl
  Constructor.
AbstractWorkflowModulePlugin.OneWayInputPortImpl(Port) - Constructor for class com.bea.rfid.edge.toolkit.workflow.AbstractWorkflowModulePlugin.OneWayInputPortImpl
  Constructor that just takes in a `Port` and constructs OneWayInputPort using it.
acceptorError(SocketAcceptorDeviceChannel, IOException) - Method in interface com.connecterra.ale.reader.SocketAcceptorDeviceChannel.SocketAcceptorListener
  This callback is invoked when the accept throws an IOException.
AccumulationObserver - Interface in com.bea.rfid.workflow.util
  Interface for observers of `Accumulator`.
Accumulator - Class in com.bea.rfid.workflow.util
  Plain java class for accumulating tags.
Accumulator(long, int, Timer) - Constructor for class com.bea.rfid.workflow.util.Accumulator
  Constructor.
ACTIVATING - Static variable in class com.connecterra.ale.reader.ChannelManager.State
  The manager is in the process of activating the channels and initializing the proxy.
ACTIVE - Static variable in class com.connecterra.ale.reader.ChannelManager.State
  Communications with the device are online, that is, the channels are active and proxy initialization has completed.
add(List) - Method in class com.bea.rfid.workflow.util.Accumulator
  Add unique tags from the list of `ECReportGroupListMember` to current accumulated tags list, if this accumulator is in active state.
add(long, EventReceiver, Object) - Method in class com.connecterra.util.event.AlarmClock
  Schedules an event for delivery at a specified time from now to a specified event receiver.
addAFIParametersToPluginMeta(DynamicConfigFactory, PluginMeta) - Static method in class com.connecterra.ale.reader.AbstractPhysicalDevice
  Adds the `"Read Tag AFI"` and `"Forced AFI value"` parameters to the PluginMeta.
addBusinessTransaction(URI, URI) - Method in class com.bea.rfid.workflow.epcis.EventGenerator
  Creates a business transaction for the given type and ID and adds it to the list of business transactions to be used on the generated event.
addBusinessTransaction(BusinessTransaction) - Method in class com.bea.rfid.workflow.epcis.EventGenerator
  Adds a business transaction entry to list of business transactions to be used on the generated event.
addChannel(DeviceChannel) - Method in class com.connecterra.ale.reader.ChannelManager
  Adds a DeviceChannel to the manager.
addChildParameter(PluginConfigParameter) - Method in class com.connecterra.ale.dynamicconfig.api.PluginConfigParameter
  Specifies the value on one child parameter.
addChildParameterMeta(PluginParameterMeta) - Method in interface com.connecterra.ale.dynamicconfig.api.PluginParameterMeta
  Adds a parameter to this parameter's child parameter list.
addDeviceChannel(DeviceChannel) - Method in class com.connecterra.ale.reader.AbstractPhysicalDevice
  Add a new DeviceChannel to the device.
addDeviceUnit(DeviceUnit) - Method in class com.connecterra.ale.reader.AbstractPhysicalDevice
  Add a new DeviceUnit to the physical device.
addEventExtension(String, String, String) - Method in class com.bea.rfid.workflow.epcis.EventGenerator
  Creates an EPCIS event extension for the given namespace, name and values and adds it to the list of event extensions to be used on the generated event.
addForceAFIParameterToPluginMeta(DynamicConfigFactory, PluginMeta) - Static method in class com.connecterra.ale.reader.AbstractPhysicalDevice
  Adds the "Forced AFI value" parameter to the PluginMeta.
additionAtPointA(List) - Method in class com.bea.rfid.workflow.util.Directionality
  Accepts a list of tags seen at Point A and updates the state of the tags.
additionAtPointB(List) - Method in class com.bea.rfid.workflow.util.Directionality
  Accepts a list of tags seen at Point B and updates the state of the tags.
addParameter(PluginConfigParameter) - Method in class com.connecterra.ale.dynamicconfig.api.PluginConfig
  Adds a `PluginConfigParameter` representing a configuration parameter value of the plugin.
addParameterMeta(PluginParameterMeta) - Method in interface com.connecterra.ale.dynamicconfig.api.PluginMeta
  Adds a configuration parameter description to the list of supported by this plugin type.
addReadAFIParameterToPluginMeta(DynamicConfigFactory, PluginMeta) - Static method in class com.connecterra.ale.reader.AbstractPhysicalDevice
  Adds the "Read Tag AFI" parameter to the PluginMeta.
addReaderThread(Thread) - Method in class com.connecterra.ale.reader.AbstractPhysicalDevice
  Inform the framework about a thread created by the device driver.
addReportNames(Collection) - Method in class com.bea.rfid.workflow.util.TagListBuilder
  Adds the given report names to the set of filter report names for `ECReports` inputs.
addTagData(AbstractPhysicalDevice.TagData) - Method in class com.connecterra.ale.reader.AbstractPhysicalDevice
addToPluginMeta(DynamicConfigFactory, PluginMeta) - Static method in class com.connecterra.ale.reader.AbstractPhysicalDevice
  Adds appropriate PluginParameterMeta objects to the PluginMeta as needed by the framework.
addToPluginMeta(DynamicConfigFactory, PluginMeta) - Static method in class com.connecterra.ale.reader.AbstractPrinterPhysicalReader
addToPluginMeta(DynamicConfigFactory, PluginMeta, String, MessageFormat, int, DeviceUnitCapabilities, boolean) - Static method in class com.connecterra.ale.reader.DeviceUnit
  Adds appropriate PluginParameterMeta objects to the PluginMeta as needed by the framework.
addToPluginMeta(DynamicConfigFactory, PluginMeta, String, MessageFormat, int, DeviceUnitCapabilities) - Static method in class com.connecterra.ale.reader.DeviceUnit
addToPluginMeta(DynamicConfigFactory, PluginMeta, String, String, String) - Static method in class com.connecterra.ale.reader.SocketAcceptorDeviceChannel
  Adds `PluginParameterMeta` to the specified `PluginMeta` for each parameter read by the channel.
AggregationEventGenerator - Class in com.bea.rfid.workflow.epcis
  Java class to generate EPCIS Aggregation Events for input tags.
AggregationEventGenerator() - Constructor for class com.bea.rfid.workflow.epcis.AggregationEventGenerator
AggregationReconciler - Class in com.bea.rfid.workflow.epcis
  Compares an aggregation with its manifest (expected elements in an aggregation).
AggregationReconciler(double, boolean, boolean, boolean) - Constructor for class com.bea.rfid.workflow.epcis.AggregationReconciler
  Constructor.
AlarmClock - Class in com.connecterra.util.event
  The alarm clock sends events at specified times in the future.
AlarmClock() - Constructor for class com.connecterra.util.event.AlarmClock
ALWAYS_QUEUE - Static variable in class com.connecterra.util.event.EventReceiver
ANTENNA - Static variable in interface com.connecterra.ale.dynamicconfig.api.PluginParameterMeta.Type
  Type representing antennae of devices.
ANTENNA_FAILURE - Static variable in class com.connecterra.ale.reader.OpStatus
  Write operation failed because the specified antenna was not present.
ANY_OBJECT - Static variable in class com.bea.rfid.edge.toolkit.workflow.SimpleOneWayPortType
  Type that sends/receives objects of type `Object`.
AnyPortType - Class in com.bea.rfid.edge.toolkit.workflow
  Represents the type of a `Port` that sends or receives messages of any type.
AnyPortType() - Constructor for class com.bea.rfid.edge.toolkit.workflow.AnyPortType

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| Documentation is available at ${DOCSWEBROOT} Copyright 2007 BEA Systems Inc.
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I K L M N O P Q R S T U V W X