### Tuxedo Configuration

Tuxedo Configuration allows you to view and refresh Tuxedo domain configuration information. If TSAM is running, Tuxedo configuration information is received from the LMS at boot time.

Note: | If TSAM is not running at boot time, or when there are Tuxedo-side configuration changes, you must manually retrieve the configuration information.

Table 1-12 lists the Tuxedo Configuration page properties.

Table 1-12 Tuxedo Configuration Page
Name | Description
--- | ---
Domains | Lists of Tuxedo domains in the following format: `<DOMAINID>:<master machine name>:<IPCKEY>`. `<DOMAINID>` and `<IPCKEY>` are configured in the UBBCONFIG `*RESOURCE` section; <master machine name> is configured in the UBBCONFIG `*MACHINE` section.
View | Displays a visible representation of the domain.
Refresh | Manually retrieves the selected domain configuration information
Expand Tree | Displays the following detailed Tuxedo domain information: Domain ID (DOMAINID), Logical Machine ID (LMID), Group name and group number (GRPNO), Server name, server ID (SRVID)
Show service | Lists the services provided by a given server.

#### View Tuxedo Domain Configuration

To view domain configuration information, do the following steps:

1. Select a domain from the Domains list

Note: | Press and hold the CTRL key to select multiple domains

Note: | Some servers (including TMS, BRIDGE) that are not configured in UBBCONFIG may be displayed.

2. Click the View button;
3. Click the Expand Tree to display detailed domain information
4. Click the Show Service check box to display service information

#### Refresh Tuxedo Domain Configuration

To refresh a domain configuration, do the following steps:

1. Select a domain from the Domains list

Note: | Press and hold the CTRL key to select multiple domains.

Note: | Some servers (including TMS, BRIDGE) that are not configured in UBBCONFIG may be displayed.

2. Click the Refresh button

Any of the following possible results are displayed:

- Successful: The configuration information is retrieved successfully, and the configuration tree is updated.
- Failed: The "refresh" failed. Configuration information was not retrieved.
- Timed out: Configuration information was not retrieved within a given time frame.

The default timeout is 30 seconds and is configured using the "tsam.config.timeoutwithtuxedo"parameter in the TSAM `web.xml` file.