This figure is used to install an SSL key/certificate on the system. You are advised that the key must contain a PKCS #12 structure, or both a key and matching certificate in PEM or DER encoding. The Key field is available (together with a Browse facility) to specify the name and location of the required file. If the key is encrypted, the Passphrase field allows you specify it. If the key is encrypted, two additional fields (Password and Confirm password), are available to specify it. You are advised that you need to manually specify the key activation password after each system re-start.