This figure shows four supported configurations: a single server setup, and three split server setups. The single server setup shows a single system with a Collector and Reporter instance. The first split server setup shows two systems: a Collector system connects to a TAP/copy port, and is itself connected to a second system with a Reporter instance (the Collector instance is disabled). The second split server setup shows two systems: a Collector system connects to a TAP/copy port, and is itself connected to a second system with a Reporter instance (the Collector instance is enabled). This system is also connected to a TAP/copy port. The final split server setup shows three systems. Two of these systems connect to separate data lines, and are both connected to a third system with a Reporter instance (the Collector instance is disabled).