Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| Sun Adapter for SNA LU62 API
PREV NEXT | FRAMES NO FRAMES

## Uses of Class
com.stc.connector.snalu62.exception.SNAApplicationException

Packages that use SNAApplicationException
com.stc.connector.snalu62.api |
com.stc.connector.snalu62.inbound |
com.stc.connector.snalu62.outbound |

Uses of SNAApplicationException in com.stc.connector.snalu62.api

Methods in com.stc.connector.snalu62.api that throw SNAApplicationException
`void` | `SNACPICCalls.cmaccp()` The Accept_Conversation (cmaccp) call accepts an incoming conversation.
`void` | `SNACPICCalls.cmallc()` A program uses the Allocate (cmallc) call to establish a basic or mapped conversation (depending on the conversation_type characteristic) with its partner program.
`void` | `SNACPICCalls.cmcanc()` A program uses Cancel_Conversation (cmcanc) to end a conversation immediately.
`void` | `SNACPICCalls.cmcfm()` The Confirm (cmcfm) call is used by a local program to send a confirmation request to the remote program and then wait for a reply.
`void` | `SNACPICCalls.cmcfmd()` A program uses the Confirmed (cmcfmd) call to send a confirmation reply to the remote program.
`void` | `SNACPICCalls.cmdeal()` A program uses the Deallocate (cmdeal) call to end a conversation.
`void` | `SNACPICCalls.cmecs()` A program uses the Extract_Conversation_State (cmecs) call to extract the conversation state for a given conversation.
`void` | `SNACPICCalls.cmecsu()` The Extract_Conversation_Security_User_ID (cmecsu) call returns the user identifier being used in a specified conversation.
`void` | `SNACPICCalls.cmect()` A program uses the Extract_Conversation_Type (cmect) call to extract the conversation_type characteristic's value for a given conversation.
`void` | `SNACPICCalls.cmemn()` A program uses the Extract_Mode_Name (cmemn) call to extract the mode_name characteristic's value for a given conversation.
`void` | `SNACPICCalls.cmepln()` A program uses the Extract_Partner_LU_Name (cmepln) call to extract the partner_LU_name characteristic's value for a given conversation.
`void` | `SNACPICCalls.cmesl()` A program uses the Extract_Sync_Level (cmesl) call to extract the sync_level characteristic's value for a given conversation.
`void` | `SNACPICCalls.cmetpn()` A program uses the Extract_TP_Name (cmetpn) call to extract the TP_name characteristic's value for a given conversation.
`void` | `SNACPICCalls.cmflus()` A program uses the Flush (cmflus) call to empty the local system's send buffer for a given conversation.
`void` | `SNACPICCalls.cminit()` A program uses the Initialize_Conversation (cminit) call to initialize values for various conversation characteristics before the conversation is allocated (with a call to Allocate).
`void` | `SNACPICCalls.cmptr()` Programs use the Prepare_To_Receive (cmptr) call to transfer control of the conversation to the remote program without waiting for the remote program to send data; that is, waiting for a Receive to complete.
`void` | `SNACPICCalls.cmrcv()` A program uses the Receive (cmrcv) call to receive information from a given conversation.
`void` | `SNACPICCalls.cmrts()` The local program uses the Request_To_Send (cmrts) call to notify the remote program that the local program would like to enter Send state for a given conversation.
`void` | `SNACPICCalls.cmscsp()` Set_Conversation_Security_Password (cmscsp) is used by a program to set the security_password and security_password_length characteristics for a conversation.
`void` | `SNACPICCalls.cmscst()` Set_Conversation_Security_Type (cmscst) is used by a program to set the conversation_security_type characteristic for a conversation.
`void` | `SNACPICCalls.cmscsu()` Set_Conversation_Security_User_ID (cmscsu) is used by a program to set the security_user_ID and security_user_ID_length characteristics for a conversation.
`void` | `SNACPICCalls.cmsct()` Set_Conversation_Type (cmsct) is used by a program to set the conversation_type characteristic for a given conversation.
`void` | `SNACPICCalls.cmsdt()` Set_Deallocate_Type (cmsdt) is used by a program to set the deallocate_type characteristic for a given conversation.
`void` | `SNACPICCalls.cmsed()` Set_Error_Direction (cmsed) is used by a program to set the error_direction characteristic for a given conversation.
`void` | `SNACPICCalls.cmsend()` A program uses the Send_Data (cmsend) call to send data to the remote program.
`void` | `SNACPICCalls.cmserr()` Send_Error (cmserr) is used by a program to inform the remote program that the local program detected an error during a conversation.
`void` | `SNACPICCalls.cmsf()` Set_Fill (cmsf) is used by a program to set the fill characteristic for a given conversation.
`void` | `SNACPICCalls.cmsld()` Set_Log_Data (cmsld) is used by a program to set the log_data and log_data_length characteristics for a given conversation.
`void` | `SNACPICCalls.cmsltp()` A program uses the Specify_Local_TP_Name (cmsltp) call to associate a name with itself, thus notifying CPI Communications that it can accept conversations destined for the name.
`void` | `SNACPICCalls.cmsmn()` Set_Mode_Name (cmsmn) is used by a program to set the mode_name and mode_name_length characteristics for a conversation.
`void` | `SNACPICCalls.cmspln()` Set_Partner_LU_Name (cmspln) is used by a program to set the partner_LU_name and partner_LU_name_length characteristics for a conversation.
`void` | `SNACPICCalls.cmspm()` A program uses the Set_Processing_Mode (cmspm) call to set the processing_mode characteristic of a conversation.
`void` | `SNACPICCalls.cmsptr()` Set_Prepare_To_Receive_Type (cmsptr) is used by a program to set the prepare_to_receive_type characteristic for a conversation.
`void` | `SNACPICCalls.cmsrc()` Set_Return_Control (cmsrc) is used to set the return_control characteristic for a given conversation.
`void` | `SNACPICCalls.cmsrt()` Set_Receive_Type (cmsrt) is used by a program to set the receive_type characteristic for a conversation.
`void` | `SNACPICCalls.cmssl()` Set_Sync_Level (cmssl) is used by a program to set the sync_level characteristic for a given conversation.
`void` | `SNACPICCalls.cmsst()` Set_Send_Type (cmsst) is used by a program to set the send_type characteristic for a conversation.
`void` | `SNACPICCalls.cmstpn()` Set_TP_Name (cmstpn) is used by a program that initiates a conversation, using the Initialize_Conversation call, to set the TP_name and TP_name_length characteristics for a given conversation.
`void` | `SNACPICCalls.cmtrts()` Test_Request_To_Send_Received (cmtrts) is used by a program to determine whether a request-to-send or allocate-confirmed notification has been received from the remote program for the specified conversation.
`void` | `SNACPICCalls.cmwait()` A program must use the Wait_For_Conversation (cmwait) call to wait for the completion of an outstanding operation on a conversation using conversation-level non-blocking.
`void` | `SNAConversationAttributes.setConvType(int convType)` Setter of conversation_type ([OTD].[CPICCalls].[ConversationAttributes].[ConvType]).
`void` | `SNAConversationAttributes.setDataOut(byte[] dataOut)` Setter of DataOut ([OTD].[CPICCalls].[ConversationAttributes].[DataOut]).
`void` | `SNAConversationAttributes.setDeallocType(int deallocType)` Setter of deallocate_type ([OTD].[CPICCalls].[ConversationAttributes].[DeallocType]).
`void` | `SNAConversationAttributes.setErrorDirection(int errorDirection)` Setter of error_direction ([OTD].[CPICCalls].[ConversationAttributes].[ErrorDirection]).
`void` | `SNAConversationAttributes.setFillType(int fillType)` Setter of fill (fill_type) ([OTD].[CPICCalls].[ConversationAttributes].[FillType]).
`void` | `SNAConversationAttributes.setLocalTPName(java.lang.String localTPName)` Setter of local_TP_Name ([OTD].[CPICCalls].[ConversationAttributes].[LocalTPName]).
`void` | `SNAConversationAttributes.setLogData(byte[] logData)` Setter of log data ([OTD].[CPICCalls].[ConversationAttributes].[LogData]).
`void` | `SNAConversationAttributes.setModeName(java.lang.String modeName)` Setter of mode_name ([OTD].[CPICCalls].[ConversationAttributes].[ModeName])
`void` | `SNAConversationAttributes.setPartnerLUName(java.lang.String partnerLUName)` Setter of Partner LU Name ([OTD].[CPICCalls].[ConversationAttributes].[PartnerLUName]).
`void` | `SNAConversationAttributes.setPrepareToReceiveType(int prepareToReceiveType)` Setter of prepare_to_receive_type ([OTD].[CPICCalls].[ConversationAttributes].[PrepareToReceiveType]).
`void` | `SNAConversationAttributes.setProcessingMode(int processingMode)` Setter of processing_mode ([OTD].[CPICCalls].[ConversationAttributes].[ProcessingMode]).
`void` | `SNAConversationAttributes.setReceiveType(int receiveType)` Setter of receive_type ([OTD].[CPICCalls].[ConversationAttributes].[ReceiveType]).
`void` | `SNAConversationAttributes.setRequestedLength(int requestedLength)` Setter of requested_length ([OTD].[CPICCalls].[ConversationAttributes].[RequestedLength]) which is the PacketSize of data the local program is to receive.
`void` | `SNAConversationAttributes.setReturnControl(int returnControl)` Setter of return_control ([OTD].[CPICCalls].[ConversationAttributes].[ReturnControl]).
`void` | `SNAConversationAttributes.setSecurityPassword(java.lang.String securityPassword)` Setter of security_password ([OTD].[CPICCalls].[ConversationAttributes].[SecurityPassword]).
`void` | `SNAConversationAttributes.setSecurityType(int securityType)` Setter of conversation_security_type ([OTD].[CPICCalls].[ConversationAttributes].[SecurityType]).
`void` | `SNAConversationAttributes.setSecurityUserID(java.lang.String securityUserID)` Setter of security_user_ID ([OTD].[CPICCalls].[ConversationAttributes].[SecurityUserID]).
`void` | `SNAConversationAttributes.setSendType(int sendType)` Setter of send_type ([OTD].[CPICCalls].[ConversationAttributes].[SendType]).
`void` | `SNAConversationAttributes.setSymDestName(java.lang.String symDestName)` Setter of sym_dest_name ([OTD].[CPICCalls].[ConversationAttributes].[SymDestName]).
`void` | `SNAConversationAttributes.setSyncLevel(int syncLevel)` Setter of sync_level ([OTD].[CPICCalls].[ConversationAttributes].[SyncLevel]).
`void` | `SNACustomerHandshake.startConversation(SNACPICCalls cpic)` Starts the SNA conversation in whatever way the user decides.

Uses of SNAApplicationException in com.stc.connector.snalu62.inbound

Methods in com.stc.connector.snalu62.inbound that throw SNAApplicationException
`void` | `SNAInboundApplication.changeState(java.lang.String state)` Changes conversation state.
`void` | `SNAInboundApplication.changeState(java.lang.String state, boolean confirm)` Changes conversation state with confirmation flag, if the flag is `true`, a CPIC cmcfm will be callled afterwards.
`void` | `SNAInboundApplication.confirm()` Flushes local LU's send buffer and sends a confirmation request to the partner TP and waits for confirmation.
`void` | `SNAInboundApplication.confirmed()` Replies to a confirmation request from the partner TP.
`java.lang.String` | `SNAInboundApplication.getPersistentData()` Retrieves the data from the persistent file.
`void` | `SNAInboundApplication.recv()` Receives any data that is currently available from the partner TP into incoming payload (buffer) represented as `DataIn` in the OTD from the partner TP.
`void` | `SNAInboundApplication.recv(boolean confirm)` Receives any data that is currently available from the partner TP into incoming payload (buffer) represented as `DataIn` in the OTD from the partner TP with confirmation flag, if the flag is `true`, a CPIC cmcfmd will be callled after the data is received.
`void` | `SNAInboundApplication.send()` Sends the outgoing payload (buffer) represented in the OTD as node `DataOut` into the local LU's send buffer for transmission to the partner TP.
`void` | `SNAInboundApplication.send(boolean confirm)` Sends the outgoing payload (buffer) represented in the OTD as node `DataOut` into the local LU's send buffer for transmission to the partner TP with confirmation flag.
`void` | `SNAInboundConfiguration.SNAInboundListenerSchedule.setAtFixedRate(boolean atFixedRate)` Sets AtFixedRate
`void` | `SNAInboundConfiguration.SNAInboundServiceSchedule.setAtFixedRate(boolean atFixedRate)` Sets AtFixedRate
`void` | `SNAInboundConfiguration.SNAInboundConnectionManagement.setConnectionPoolSize(long aConnectionPoolSize)` Sets ConnectionPoolSize
`void` | `SNAInboundConfiguration.SNAInboundSettings.setCustomerHandshakeClassName(java.lang.String aCustomerHandshakeClassName)` Sets the customerHandshakeClassName.
`void` | `SNAInboundApplication.setDataOut(byte[] data)` Sets the content for outgoing payload (buffer) which is represented in the OTD as node `DataOut`.
`void` | `SNAInboundConfiguration.SNAInboundSettings.setDeallocationType(int aDeallocationType)` Sets DeallocationType
`void` | `SNAInboundConfiguration.SNAInboundListenerSchedule.setDelay(long aDelay)` Sets Delay
`void` | `SNAInboundConfiguration.SNAInboundServiceSchedule.setDelay(long aDelay)` Sets Delay
`void` | `SNAInboundConfiguration.SNAInboundSettings.setHostName(java.lang.String aHostName)` Sets the HostName where the lu62 Server runs, only needed for Brixton LU62 server.
`void` | `SNAInboundConfiguration.SNAInboundSettings.setInitializeConversation(boolean initializeConversation)` Sets InitializeConversation
`void` | `SNAInboundConfiguration.SNAInboundSettings.setLocalLUName(java.lang.String aLocalLUName)` Sets LocalLUName
`void` | `SNAInboundConfiguration.SNAInboundSettings.setLocalTPName(java.lang.String aLocalTPName)` Sets LocalTPName
`void` | `SNAInboundConfiguration.SNAInboundConnectionEstablish.setMaxConnectionRetries(int aMaxConnectionRetries)` Sets MaxConnectionRetries
`void` | `SNAInboundConfiguration.SNAInboundSettings.setPacketSize(int aPacketSize)` Sets PacketSize which is requested_length of data the local program is to receive.
`void` | `SNAInboundConfiguration.SNAInboundListenerSchedule.setPeriod(long aPeriod)` Sets Period
`void` | `SNAInboundConfiguration.SNAInboundServiceSchedule.setPeriod(long aPeriod)` Sets Period
`void` | `SNAInboundApplication.setPersistentData(java.lang.String data)` Stores the data into the persistent file.
`void` | `SNAInboundConfiguration.SNAInboundGeneralSettings.setPersistentStorageLocation(java.lang.String dirName)` Sets Persistent Storage Location
`void` | `SNAInboundConfiguration.SNAInboundConnectionEstablish.setRetryConnectionInterval(long aRetryConnectionInterval)` Sets RetryConnectionInterval
`void` | `SNAInboundConfiguration.SNAInboundListenerSchedule.setScheduler(java.lang.String aScheduler)` Sets Scheduler
`void` | `SNAInboundConfiguration.SNAInboundServiceSchedule.setScheduler(java.lang.String aScheduler)` Sets Scheduler
`void` | `SNAInboundConfiguration.SNAInboundListenerSchedule.setScheduleType(java.lang.String aScheduleType)` Sets ScheduleType
`void` | `SNAInboundConfiguration.SNAInboundServiceSchedule.setScheduleType(java.lang.String aScheduleType)` Sets ScheduleType
`void` | `SNAInboundConfiguration.SNAInboundConnectionManagement.setScopeOfConnection(java.lang.String aScopeOfConnection)` Sets ScopeOfConnection
`void` | `SNAInboundConfiguration.SNAInboundGeneralSettings.setScopeOfState(java.lang.String aScope)` Sets Scope Of State
`void` | `SNAInboundApplication.setState(java.lang.String stateValue)` Sets the State.
`void` | `SNAInboundConfiguration.SNAInboundSettings.setSymbolicDestName(java.lang.String aSymbolicDestName)` Sets SymbolicDestName
`void` | `SNAInboundConfiguration.SNAInboundSettings.setSynchronizationLevel(int aSynchronizationLevel)` Sets SynchronizationLevel
`void` | `SNAInboundConfiguration.SNAInboundSettings.setTimeout(int aTimeout)` Sets Timeout
`void` | `SNAInboundConfiguration.validate()` Validates inbound configuration
`void` | `SNAInboundConfiguration.SNAInboundGeneralSettings.validate()` Validates GeneralSettings section
`void` | `SNAInboundConfiguration.SNAInboundSettings.validate()` Validates SNASettings section
`void` | `SNAInboundConfiguration.SNAInboundConnectionEstablish.validate()` Validates inbound ConnectionEstablish section
`void` | `SNAInboundConfiguration.SNAInboundSchedules.validate()` Validates inbound Schedules section
`void` | `SNAInboundConfiguration.SNAInboundConnectionManagement.validate()` Validates inbound ConnectionManagement section
`void` | `SNAInboundConfiguration.SNAInboundListenerSchedule.validate()` Validates inbound ListenerSchedule section
`void` | `SNAInboundConfiguration.SNAInboundServiceSchedule.validate()` Validates inbound ServiceSchedule section

Uses of SNAApplicationException in com.stc.connector.snalu62.outbound

Methods in com.stc.connector.snalu62.outbound that throw SNAApplicationException
`void` | `SNAOutboundApplication.changeState(java.lang.String state)` Changes conversation state.
`void` | `SNAOutboundApplication.changeState(java.lang.String state, boolean confirm)` Changes conversation state with confirmation flag, if the flag is `true`, a CPIC cmcfm will be callled afterwards.
`void` | `SNAOutboundApplication.confirm()` Flushes local LU's send buffer and sends a confirmation request to the partner TP and waits for confirmation.
`void` | `SNAOutboundApplication.confirmed()` Replies to a confirmation request from the partner TP.
`void` | `SNAOutboundApplication.endConversation()` Ends the conversation manually.
`java.lang.String` | `SNAOutboundApplication.getPersistentData()` Retrieves the data from the persistent file.
`void` | `SNAOutboundApplication.recv()` Receives any data that is currently available from the partner TP into incoming payload (buffer) represented as `DataIn` in the OTD from the partner TP.
`void` | `SNAOutboundApplication.recv(boolean confirm)` Receives any data that is currently available from the partner TP into incoming payload (buffer) represented as `DataIn` in the OTD from the partner TP with confirmation flag, if the flag is `true`, a CPIC cmcfmd will be callled after the data is received.
`void` | `SNAOutboundApplication.send()` Sends the outgoing payload (buffer) represented in the OTD as node `DataOut` into the local LU's send buffer for transmission to the partner TP.
`void` | `SNAOutboundApplication.send(boolean confirm)` Sends the outgoing payload (buffer) represented in the OTD as node `DataOut` into the local LU's send buffer for transmission to the partner TP with confirmation flag.
`void` | `SNAOutboundConfiguration.SNAOutboundConnectionEstablish.setAlwaysCreateNewConnection(boolean alwaysCreateNewConnection)` Sets AlwaysCreateNewConnection
`void` | `SNAOutboundConfiguration.SNAOutboundConnectionEstablish.setAutoDisconnectConnection(boolean autoDisconnectConnection)` Sets AutoDisconnectConnection
`void` | `SNAOutboundConfiguration.SNAOutboundConnectionEstablish.setAutoReconnectUponMatchingFailure(boolean autoReconnectUponMatchingFailure)` Sets AutoReconnectUponMatchingFailure
`void` | `SNAOutboundConfiguration.SNAOutboundSettings.setCustomerHandshakeClassName(java.lang.String aCustomerHandshakeClassName)` Sets the customerHandshakeClassName.
`void` | `SNAOutboundApplication.setDataOut(byte[] data)` Sets the content for outgoing payload (buffer), which is represented in the OTD as node `DataOut`.
`void` | `SNAOutboundConfiguration.SNAOutboundSettings.setDeallocationType(int aDeallocationType)` Sets DeallocationType
`void` | `SNAOutboundConfiguration.SNAOutboundSettings.setHostName(java.lang.String aHostName)` Sets the HostName where the lu62 Server runs, only needed for Brixton LU62 server.
`void` | `SNAOutboundConfiguration.SNAOutboundSettings.setInitializeConversation(boolean initializeConversation)` Sets InitializeConversation
`void` | `SNAOutboundConfiguration.SNAOutboundSettings.setLocalLUName(java.lang.String aLocalLUName)` Sets LocalLUName
`void` | `SNAOutboundConfiguration.SNAOutboundSettings.setLocalTPName(java.lang.String aLocalTPName)` Sets LocalTPName
`void` | `SNAOutboundConfiguration.SNAOutboundConnectionEstablish.setMaxConnectionRetries(int aMaxConnectionRetries)` Sets MaxConnectionRetries
`void` | `SNAOutboundConfiguration.SNAOutboundSettings.setPacketSize(int aPacketSize)` Sets PacketSize which is requested_length of data the local program is to receive.
`void` | `SNAOutboundApplication.setPersistentData(java.lang.String data)` Stores the data into the persistent file.
`void` | `SNAOutboundConfiguration.SNAOutboundGeneralSettings.setPersistentStorageLocation(java.lang.String dirName)` Sets the Persistent Storage Location
`void` | `SNAOutboundConfiguration.SNAOutboundConnectionEstablish.setRetryConnectionInterval(long aRetryConnectionInterval)` Sets RetryConnectionInterval
`void` | `SNAOutboundConfiguration.SNAOutboundGeneralSettings.setScopeOfState(java.lang.String aScope)` Sets Scope Of State
`void` | `SNAOutboundApplication.setState(java.lang.String stateValue)` Sets the State.
`void` | `SNAOutboundConfiguration.SNAOutboundSettings.setSymbolicDestName(java.lang.String aSymbolicDestName)` Sets SymbolicDestName
`void` | `SNAOutboundConfiguration.SNAOutboundSettings.setSynchronizationLevel(int aSynchronizationLevel)` Sets SynchronizationLevel
`void` | `SNAOutboundConfiguration.SNAOutboundSettings.setTimeout(int aTimeout)` Sets Timeout
`void` | `SNAOutboundApplication.startConversation()` Starts the conversation manually.
`void` | `SNAOutboundConfiguration.validate()` Validates the outbound configuration
`void` | `SNAOutboundConfiguration.SNAOutboundGeneralSettings.validate()` Validates outbound GeneralSettings section
`void` | `SNAOutboundConfiguration.SNAOutboundSettings.validate()` Validates outbound SNASettings section
`void` | `SNAOutboundConfiguration.SNAOutboundConnectionEstablish.validate()` Validates outbound ConnectionEstablish section

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| Sun Adapter for SNA LU62 API
PREV NEXT | FRAMES NO FRAMES

Copyright © 2008 Sun Microsystems, Inc. All rights reserved.