Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A C D E F G I L M P R S T V W _

## _

_ConvReturnCode - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The SNA conversation return code set by the JNI code as a result of the last CPIC function call which generated a conversation return code.
_ConvType - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The SNA conversation type.
_ConversationID - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  SNA Conversation ID which gets set by the JNI code when a conversation is established.
_ConversationSecurityID - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The SNA conversation security ID set by the JNI code as a result of retrieving the SNA conversation security ID.
_ConversationSecurityIDLen - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The length of the SNA conversation security ID set by the JNI code as a result of retrieving the SNA conversation security ID.
_ConversationSecurityPass - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The SNA conversation security password used set by the JNI code for setting the SNA conversation security password.
_ConversationSecurityPassLen - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  Deprecated.
_ConversationSecurityType - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The SNA conversation security type used by the JNI code to set the SNA conversation security type.
_DataIn - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  Data which gets set by the JNI code when data is received from the partner in the SNA conversation.
_DataOut - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  Data which is passed to the JNI code for sending data to the partner in the SNA conversation.
_DataReceivedType - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The SNA data receive type set by the JNI code as a result of the last CPIC function call which generated a data receive type.
_DeallocType - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The SNA dealloc type.
_ErrorDirection - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The SNA error direction used by the JNI code for setting the SNA error direction.
_FillType - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The SNA fill type.
_HaveConversation - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  If a conversation is established with the SNA partner, this flag will be set to true otherwise it is set to false by the JNI code.
_IsInbound - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  Deprecated.
_LocalLUName - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The Local Logical Unit Name of the SNA partner which is accepting conversations from the initiating SNA partner.
_LocalTPName - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The Local TP (Transaction Program) Name
_LogData - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The SNA log data which is used by the JNI code for sending the log data.
_ModeName - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The SNA mode name.
_PacketSize - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The size of the data packets used by the JNI code when receiving data from the partner in the SNA conversation.
_PartnerLUName - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The partner LU (Logical Unit) name.
_PrepareToReceiveType - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The SNA prepare to receive type.
_ProcessingMode - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The SNA processing mode.
_ReceiveType - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The SNA receive type.
_Req2SendReceived - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The SNA request to send received code set by the JNI code as a result of the last CPIC function call which generated a request to send received code.
_ReturnCode - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  Return code which gets set by the JNI code and is the return code returned by the last major CPIC function call.
_ReturnControl - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The SNA return control.
_SNALastError - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  Deprecated.
_SNALastState - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The SNA state set by the JNI code.
_SNALastStatus - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The SNA status code set by the JNI code as a result of the last CPIC function call which generated an SNA status code.
_SendType - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The SNA send type.
_StatusReceived - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The SNA status received set by the JNI code as a result of the last CPIC function call which generated a status received.
_SymDestName - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The Symbolic Destination Name of the SNA partner to which the initiating SNA partner will establish an SNA conversation.
_SyncLevel - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  The SNA synch level.
_Timeout - Variable in class com.stc.connector.snalu62.jni.SNAInterface
  Timeout in milliseconds used by the JNI code when waiting for a conversation or when receiving data.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A C D E F G I L M P R S T V W _