Index

### Numerics

1000BASE-T, 1, 2

100BASE-TX, 1, 2, 3

10BASE-T, 1, 2, 3

6U, 1

### A

ACT, LED, 1

Advanced Telecom Computing Architecture (ATCA), 1

Airflow requirements, 1

AMC modules

installation, 1

antistatic wrist strap, 1

Application extension commands, 1

applications, terminating, 1

ATCA shelf (chassis), 1

### B

backplane connectors for Zone 3, 1

back-to-back slots, 1

Blade Management Controller (BMC), 1

blue LED, 1

board removal, 1

### C

changing the OOS LED color, 1

compatible node boards, 1

compliance, EMI, 1

connectors, 1

### D

data corruption, 1

description of connectors, 1

### E

electrical requirements, 1

electromagnetic interference (EMI, 1

electronic keying (e-Keying), 1, 2

electrostatic discharge (ESD), 1

EMI, electromagnetic interference, 1

empty chassis, installing boards, 1

Emulex IOC3532 controller, 1, 2

energy hazards, 1

environmental specifications and compliance, 1

ESD precautions, 1

Ethernet, 1

Ethernet management port, 1

event commands, 1

### F

features, Netra CP32x0 ARTM-FC, 1

fibre channel

network access, 1

SFP connector, 1

SFP connector pin assignments, 1

file corruption, 1

front- and rear-board installations, 1

front panel, 1

FRU device commands, 1

FRU information, 1

full-duplex mode, 1

### G

GbE

connections, 1

controllers, 1

RJ45 connector pin assignments, 1, 2

RJ45 copper connector, 1

SFP connector pin assignments, 1

SPF connector, 1

Gigabit Ethernet (GbE), 1, 2

Gigabit Ethernet Controllers, 1

### H

half-duplex mode, 1

Hardware Platform Management (HPM), 1

headers, 1

host boards, compatible, 1

hot-swap, 1

communication, 1

insertion, 1

HPM.1 extension commands, 1

HS, LED, 1

### I

I/O connectors, 1

ID 15, 1

identifying the ARTM, 1

illustration of Netra CP32x0 ARTM-FC, 1

inlet air temperature, 1

input/output (I/O), 1

installing, 1

Intel 82571EB controllers, 1

Intelligent Platform Management Interface (IPMI), 1

IPM device global commands, 1

IPMBL address, 1

IPMI 2.0 requests supported, 1

IPMI FRU PROM, 1

### L

LAN, 1

LEDs

ACT, 1

blue, 1

green, 1

HS, 1

LNK, 1

OK, 1

OOS, 1

software control, 1

LNK, LED, 1

### M

media access control (MAC), 1

midplane, 1

Module Management Controller (MMC), 1

### N

node boards, compatible, 1

### O

OEM Extension Commands, 1

OK, LED, 1

OOS, LEDs, 1

Out-of-service (OOS), 1

### P

packing list and material, 1

PCI-E cable connector, 1

PCI-E cable connector pin assignment, 1

PCI-Express (PCI-E), 1

physical dimensions, 1

PINs

bent or damaged, 1

common, 1

port commands, compliance, 1

ports, 1

power requirements, 1, 2

powering down, 1

### R

rear I/O access, 1

removing the ARTM, 1

RTM pressure drop, 1

### S

sensor device commands, 1

serial management, 1

serial port, 1

shelf manager, 1

shut down, 1

signals, 1

slot usage, 1

slot, compatible host, 1

software support information, 1

switches, 1

switches and headers, factory-use only, 1

### T

terminating applications, 1

thermal requirements, 1

threshold values

temperature sensors, 1

voltage sensors, 1

Transmission Control Protocol (TCP), 1

### U

UL60950-1, compliance, 1

### V

voltage monitoring, 1

### Z

Zone 3

backplane connectors, 1

connector complex, 1

connectors, 1

P32 pin assignments, 1

Copyright © 2009 Sun Microsystems, Inc. All rights reserved.