A P P E N D I X C

Connector Pinouts

This chapter shows the pin signal assignments (pinouts) for the three-connector cable dongle (FIGURE C-1).

FIGURE C-1 Three-Connector Cable Dongle (UCP-3)

Note - The older four-connector cable dongle (UCP-4) can also be used on the Sun Netra T6340 server module, with some restrictions. The Sun Netra T6340 does not support use of the UCP-4 dongle’s RJ-45 connector.

##

C.1 RJ-45 Serial Connector

FIGURE C-2 RJ-45 Serial Connector on the Cable Dongle

TABLE C-1 RJ-45 Connector Pin Assignments
Pin Number | Signal | Pin Number on Universal Connector
--- | --- | ---
7 | DSR | 21
6 | RxD | 22
1 | RTS | 23
3 | TxD | 24
8 | CTS | 25
2 | DTR | 26
7 | DCD | 27
4, 5 | GND | 29

##

C.2 USB Connectors

FIGURE C-3 Dual USB 2.0 Connector Pin Assignments

TABLE C-2 USB 2.0 Connector Pinout
Pin Number | Signal | Pin Number on Universal Connector
--- | --- | ---
1 | USB1 VCC Red | 14, 15
2 | USB1 DN white | 12
3 | USB1 DP Green | 13
4 | USB1 GND Black | 11
5 | USB2 VCC Orange | 16, 17
6 | USB2 DN Yellow | 18
7 | USB2 DP Blue | 19
8 | USB2 GND Brown | 20

##

C.3 HD15 Video Output Connector

FIGURE C-4 and TABLE C-3 show the XVR-50 graphics accelerator HD15 connector and pinout signals.

The console video output port connects to the 15-pin connector on the cable dongle. The HD15 video connector supports DDC2 monitor support and Display Power Management Signaling (DPMS).

FIGURE C-4 XVR-50 Graphics Accelerator HD15 Connector Pin Assignments

TABLE C-3 XVR-50 Graphics Accelerator HD15 Connector Pinout
Pin Number | Signal | Pin Number on Universal Connector
--- | --- | ---
1 | Red analog video | 2
2 | Green analog video | 3
3 | Blue analog video | 4
4 | No Connect | -
5 | Ground | shell
6 | Ground |
7 | Ground | shell
8 | Ground |
9 | +5V Supply, black | 1
10 | Ground |
11 | No Connect | shell
12 | Monitor ID1 (DAT, white) |
13 | Horizontal Sync, orange |
14 | Vertical Sync, yellow |
15 | Monitor ID2, red | 11

##

C.4 Using the Cable Dongle

| Caution - The cable dongle is for temporary connections only. The cable dongle has not been evaluated for electromagnetic compatibility (EMC). The cable dongle or server module connectors could be damaged by closing rack doors or other impacts. Remove the cable dongle during normal system operation.

Copyright © 2010, Oracle and/or its affiliates. All rights reserved.