Exit Print View
#### Sun Integrated Lights Out Manager (ILOM) 3.0 Supplement for the Sun Netra T6340 Server Module |

| Event Messages Available Through the ALOM Compatibility Shell |

### Host Monitoring Event Messages

The following table displays host monitoring event messages from the service processor (system controller).

###### Host Monitoring Event Messages

Severity | Message | Description
--- | --- | ---
Critical | `SP detected fault at time time component disabled` | ALOM compatibility shell sends this message when a component has been disabled, either automatically by POST discovering a fault or by a user typing the `disablecomponent` command. component is the disabled component, which will be an entry from the platform showcomponent command.This fault event message appears in the output of the ALOM compatibility shell showfaults command.
Minor | `SP detected fault cleared at component reenabled` | ALOM compatibility shell sends this message when a component is enabled. A component can be enabled by a user typing the enablecomponent command or by FRU replacement if the component itself is a FRU (such as a DIMM). component is the name of the component shown in the output of the platform `showcomponent` command.
Major | `Host detected fault, MSGID: SUNW-MSG-ID` | ALOM compatibility shell sends this message when the Solaris PSH software diagnoses a fault. The SUNW-MSG-ID of the fault is an ASCII identifier that can be entered at http://www.sun.com/msg for more information about the nature of the fault and the steps to repair.This fault event message appears in the output of the ALOM compatibility shell `showfaults` command.
Major | `Location has been replaced;faults cleared.` | ALOM compatibility shell sends this message after the replacement of a FRU that contained a host-detected fault. Location is the location and name of the FRU that was replaced. This event can be received at SC boot or after FRUs have been swapped and the chassis cover is closed.
Major | `Existing faults detected in FRU_PROM at location.` | ALOM compatibility shell sends this message to indicate that the SC has detected a new FRU with pre-existing faults logged into its FRU PROM. This event can occur when either a FRU or the SC card is moved from one system to another. The location is the name of the SEEPROM on the replaced FRU, such as `MB/SEEPROM`.The most recent existing fault will be imported from the FRU PROM onto the `showfaults` list. The entry on the `showfaults` list is the fault imported, not this message.

Legal Copyright 1994-2010 Oracle and/or its affiliates. |