Exit Print View
#### Sun Integrated Lights Out Manager (ILOM) 3.0 Supplement for the Sun Netra T6340 Server Module |

| ALOM CMT Compatibility Shell > Comparing ILOM and ALOM CMT Commands |

#### ALOM CMT Shell Status and Control Commands

ALOM CMT Command | Summary | Comparable ILOM Command
--- | --- | ---
`showenvironment` | Displays the environmental status of the host server. This information includes system temperatures, power supply status, front panel LED status, hard disk drive status, fan status, voltage, and current sensor status. | `show –o table –level all /SYS`
`showpower [–v]` | Displays power metrics for the host server. | `show /SP/powermgmt`
`shownetwork [–v]` | Displays the current network configuration information. The `–v` option shows additional information about your network, including information about your DHCP server. | `show /SP/network`
`console [–f]` | Connects to the host system console. The `–f` option forces the console write lock from one user to another. In ILOM, the `–force` option terminates the console, permitting you to start a new console. | `start [–force] /SP/console`
`break` `[–D][–c]` | Drops the host server from running the Solaris OS software into OpenBoot PROM or `kmdb` depending upon the mode in which the Solaris software was booted. | `set /HOST send_break_action=[break|dumpcore]` `[start /SP/console]`
`bootmode [normal] [reset_nvram] [config=`configname`][bootscript =`string] | Controls the host server OpenBoot PROM firmware method of booting. | `set /HOST/bootmode` property`=`value `(`where property is `state,` `config,` or `script)`
`flashupdate –s` IPaddr `–f` pathname [`–v`] [`-y`] [`-c`] | Downloads and updates system firmware (both host firmware and ALOM CMT firmware). For ILOM, ipaddr must be a TFTP server. If you use DHCP, you can replace ipaddr with the name of the TFTP host. The `-y` option enables you to skip the confirmation question. The `-c` option enables you to update system firmware on your server without preserving configuration information. After configuration information has been deleted (by having used the `-c` option or the `set /SP reset_to_defaults=factory` command), you must use the `-c` option when replacing system firmware that includes ILOM 3.0 with firmware that includes ILOM 2.0. If you omit the `-c` option, the `flashupdate` command attempts to restore preserved configuration information, halting the firmware downgrade because that configuration information is absent. | `load –source tftp://`ipaddr`/`pathname
`reset [–y] [–f] [–c]` `` `reset –d [–n] [–y] [–f] [–c]` | Generates a hardware reset on the host server. The `–y` option enables you to skip the confirmation question. The `–f` option forces a hardware reset.The `–c` option starts the console. The `–d` option gracefully resets the control domain.The `–n` option sets the `auto-boot` variable to disable (lasts for one reset).The `–y` option enables you to skip the confirmation question.The `–f` option forces a hardware reset.The `–c` option starts the console. | `reset [-script][–force] /SYS` [`start /SP/console`] `` `[set /HOST/domain/control auto-boot=disable`] `reset [–script] [–force] /HOST/domain/control` [`start /SP/console`] ``
`powercycle [–y] [–f]` | `poweroff` followed by `poweron`. The `–f` option forces an immediate `poweroff`, otherwise the command attempts a graceful shutdown. | `stop [–script] [–force] /SYS` `start [`–script] [–force] /SYS
`poweroff` [`–y`][`–f`] | Removes the main power from the host server. The `–y` option enables you to skip the confirmation question. ALOM CMT attempts to shut the server down gracefully. The `–f` option forces an immediate shutdown. | `stop [–script][–force] /SYS`
`poweron` | Applies the main power to the host server or FRU. | `start /SYS`
`setlocator [on/off`] | Turns the Locator LED on the server on or off. | `set /SYS/LOCATE value=`value
`showfaults [–v]` | Displays current valid system faults. | `show /SP/faultmgmt`
`clearfault` UUID | Manually repairs system faults. | `set /SYS/`component `clear_fault_action=true`
`showlocator` | Displays the current state of the Locator LED as either `on` or `off`. | `show /SYS/LOCATE`
`removeblade [-y]` | Pauses the service processor tasks and illuminates the blue OK to Remove LED, indicating that it is safe to remove the blade. The `-y` option enables you to skip the confirmation question. | `set /SYS prepare_to_remove_action=true`
`unremoveblade` | Turns off the OK to Remove LED and restores the service processor state. | `set /SYS return_to_service_action=true`

Legal Copyright 1994-2010 Oracle and/or its affiliates. |