Exit Print View
#### Sun Integrated Lights Out Manager (ILOM) 3.0 Supplement for the Sun Netra T6340 Server Module |

| Managing the Service Processor > Managing Network Access |

### Display the DHCP Server’s IP Address (CLI)

To display the IP address of the DHCP server that provided the dynamic IP address requested by the service processor, view the `dhcp_server_ip` property. To see the `dhcp_server_ip` property, use the following procedure.

- Type:

      -> show /SP/network

        /SP/network
           Targets:

           Properties:
               commitpending = (Cannot show property)
               dhcp_server_ip = 10.8.31.5
               ipaddress = 10.8.31.188
               ipdiscovery = dhcp
               ipgateway = 10.8.31.248
               ipnetmask = 255.255.252.0
               macaddress = 00:14:4F:7E:83:4F
               pendingipaddress = 10.8.31.188
               pendingipdiscovery = dhcp
               pendingipgateway = 10.8.31.248
               pendingipnetmask = 255.255.252.0
               state = enabled

           Commands:
               cd
               set
               show

Legal Copyright 1994-2010 Oracle and/or its affiliates. |