Exit Print View
#### Sun Integrated Lights Out Manager (ILOM) 3.0 Supplement for the Sun Netra T6340 Server Module |

| Managing Devices > Managing Virtual Keyswitch Settings |

### Specify Host Behavior (CLI)

Use the `/SYS keyswitch_state` property to control the position of the virtual keyswitch.

- At the `->` prompt, type:

      -> set /SYS keyswitch_state=value

  where value can be:

  - `normal` – The system can power itself on and start the boot process (the default).

  - `standby` – The system cannot power itself on.

  - `diag` – The system can power itself on using preset values of diagnostic properties `(/HOST/diag level=max, /HOST/diag mode=max, /HOST/diag verbosity=max)` to provide thorough fault coverage. This option overrides the values of diagnostic properties that you might have set.

  - `locked` – The system can power itself on, however you are prohibited from updating any of the flash devices or setting `/HOST send_break_action=break`.

Legal Copyright 1994-2010 Oracle and/or its affiliates. |