Index

### A

advanced ECC technology, 1

Advanced Lights Out Management (ALOM) CMT

POST, and, 1

Advanced Lights Out Management (ALOM) CMT and POST, 1

ALOM and ILOM, switching between, 1

ALOM CMT commands, 1

antistatic mat, 1

antistatic wrist strap, 1

architecture designation, 1

ASR blacklist, 1

asrkeys, 1

`asrkeys`, 1

Automatic System Recovery (ASR), 1

### B

battery, service processor

replacing, 1

blacklist, ASR, 1

`bootmode` command, 1

`break` command, 1

button

Locator, 1

Power, 1

### C

`cfgadm` command, 1, 2

chassis

reinstalling server, 1

chipkill, 1

`clear_fault` command, 1

`clear_fault_action`, ILOM command, 1

`clearasrdb` command, 1

`clearfault` command, 1

`clearfault`, ALOM-CMT command, 1

clearing POST detected faults, 1

clearing PSH detected faults, 1

clock settings, 1

common procedures for parts replacement, 1

component, replaceable, 1

`component_state=enabled`, ILOM command, 1

components, disabled, 1

components, displaying the state of, 1

connector pinouts, cable dongle, 1

console, 1

`console` command, 1

console, switching with ALOM, 1

`consolehistory` command, 1

cooling, 1

cores, 1

cover, removing, 1

cover, replacing, 1

### D

defaults, resetting, 1 - 2

device configuration, checking

`-prconf`, 1

`-propt`, 1

`diag_level` parameter, 1, 2, 3

`diag_mode` parameter, 1, 2, 3

`diag_trigger` parameter, 1, 2, 3

`diag_verbosity` parameter, 1, 2, 3

diagnostics

about, 1

flowchart, 1

low level, 1

running remotely, 1

SunVTS, 1

DIMM configuration, 1

DIMMs

example POST error output, 1

replacing, 1

troubleshooting, 1

disabling components with ILOM, 1

disk configuration

RAID, 1

striping, 1

disk drives See hard drives

displaying FRU status, 1

`dmesg` command, 1

Drive Ready to Remove LED, 1

dynamic FRU and ALOM, 1

### E

EEPROM, system configuration, 1

electrostatic discharge (ESD) prevention, 1

`enablecomponent` command, 1, 2

enabling components with ILOM, 1

environmental faults, 1, 2, 3

Ethernet ports

LEDs, 1

specifications, 1

event log, checking the PSH, 1

### F

factory defaults, 1 - 2

fan status, displaying, 1

fault manager daemon, `fmd(1M)`, 1

fault message ID, 1

fault records, 1

faults

clearing with PSH, 1

environmental, 1

ILOM handling, 1

POST detected, 1

recovery, 1

repair, 1

`fbconfig`, 1

`-list`, 1

man page, 1, 2

`-prconf`, 1

`-propt`, 1

FB-DIMMs, fully-buffered DIMMs, 1

features, server module, 1

field-replaceable units (FRUs) See FRUs, 4-1

`fmadm` command, 1

`fmadm faulty` command, 1

`fmadm faulty` command, 1

`fmdump` command, 1

front panel

LED status, displaying, 1

LEDs, 1

FRU

replacement, common procedures, 1

status, displaying, 1

FRU ID PROMs, 1

FRUs

hot-swapping, 1

### G

graphics accelerator specifications, 1

### H

hard drives

hot-plugging, 1

identification, 1, 2

latch release button, 1

mirroring, 1

replacing, 1

replacing or installing, 1

specifications, 1

status, displaying, 1

HD15 video connector pinouts, 1

`help` command, 1

host console, switching to ILOM console, 1

host, ALOM and ILOM, switching between, 1

hot-plugging hard drives, 1

hot-swapping FRUs, 1

### I

I/O port, front panel, 1

identifying the chassis, 1

ILOM and ALOM, switching between, 1

ILOMSee Integrated Lights Out Management

Integrated Lights Out Management, 1

### K

knowledge database, PSH, 1, 2

### L

latch release button, hard drive, 1

LEDs

descriptions, 1, 2

Ethernet port (chassis), 1

OK, 1

system, interpreting, 1

locating the server for maintenance, 1

locating the server module, 1

Locator LED, 1

log files, viewing, 1

### M

MAC address label, 1

man pages, 1

`fbconfig`, 1

`SUNWpfb_config`, 1

memory

configuration, 1

fault handling, 1

overview, 1

message ID, 1, 2

`messages` file, 1

mirrored disk, 1

MSG-ID, online, 1, 2

### N

NVRAM, system controller PROM, 1

### O

OK LED, 1, 2

operating state, determining, 1

### P

parts, replaceable, 1

parts, replacement See FRUs

password

root, 1 - 2

PCI EM, adding, 1

PCI ExpressModules, adding, 1

pinouts, cable dongle, 1

platform name, 1

POST

detected faults, 1

reasons to run, 1

POST detected faults, 1

See also POSTpower-on self-test (POST), 2-27

Power button, 1

power supply, 1

power supply status, displaying, 1

`powercycle` command, 1

powering off the system, 1

`poweroff` command, 1

`poweron` command, 1

power-on self-test (POST), 1

about, 1

ALOM CMT commands, 1, 2

configuration flowchart, 1, 2

error message example, 1

error messages, 1

fault clearing, 1

faulty components detected by, 1

memory faults and, 1

parameters, changing, 1

reasons to run, 1

troubleshooting with, 1

power-on, standby, 1

`-prconf`, 1

Predictive Self-Healing (PSH)

about, 1

clearing faults, 1, 2

knowledge database, 1, 2

memory faults and, 1

Sun URL, 1

procedures for finishing up, 1

procedures for parts replacement, 1

processor, 1

processor description, 1

PROM, system configuration, 1

`-propt`, 1

PSH detected faults, 1

See also PSHPredictive Self-Healing (PSH), 2-39

### R

RAID (redundant array of independent disks)

storage configurations, 1

RAID expansion module replacement, 1

REM replacement, 1

remote management, 1

Remote Power Control in ILOM, 1

`removeblade` command, 1

`reset /SYS` command, 1

reset button, 1

`reset` command, 1

`resetsc` command, 1

resolutions, 1

RJ45 connector pinouts, 1

### S

safety information, 1

safety symbols, 1

screen resolutions, 1

serial number

finding, 1

server module, 1

server module

locating, 1

serial number, 1

Service Action Required LED, 1, 2, 3

service information resources, 1

service mode, 1

service processor

battery, 1

description, 1

service processor and ILOM, 1

service resources, 1

`set /SP/clock datetime` command and POST, 1

`set /SYS/`component component_state=disabled command, 1

`set /SYS/`component component_state=enabled command, 1

`set /SYS/LOCATE` command, 1

`set /SYS/PS0 prepare_to_remove_action=true` command, 1

`set component_state=enabled` command, 1

`setkeyswitch` parameter, 1, 2, 3

`setlocator` command, 1

`show /SP/faultmgmt` command, 1, 2, 3

troubleshooting with, 1

`show /SYS` command, 1

`show /SYS/MB` command, 1

`showcomponent` command, 1

`showenvironment` command, 1, 2

`showfaults` command

syntax, 1

`showfru` command, 1, 2, 3

`showkeyswitch` command, 1

`showlocator` command, 1

`showlogs` command, 1

`shownetwork` command, 1

`showplatform` command, 1, 2

shutting down the system, 1

signal, cable dongle pinouts, 1

Solaris log files, 1

Solaris OS, collecting diagnostic information from, 1

Solaris Predictive Self-Healing (PSH) detected faults, 1

specifications, 1

standby power, 1

state of server module, 1

`stop /SYS` command, 1

striping disks, 1

striping support, 1

Sun XVR-50 graphics accelerator

man pages, 1

video formats, HD15, 1

SunSolve online, 1

SunVTS, 1

running, 1

tests, 1

user interfaces, 1, 2, 3

SUNW-MSG-ID, online, 1, 2

`SUNWpfb_config`, 1

`syslogd` command, 1

`syslogd` daemon, 1

system configuration PROM, 1

system console, switching to, 1, 2

system console, switching to ILOM console, 1

system controller card

removing, 1, 2, 3, 4

replacing, 1, 2

See

system status LEDs

interpreting, 1

system temperatures, displaying, 1

### T

tools required, 1

troubleshooting

actions, 1

DIMMs, 1

### U

UltraSPARC T2 Plus processor

and PSH, 1

universal connector port features, 1

Universal Unique Identifier (UUID), 1, 2

`unremoveblade` command, 1

USB connector pinouts, 1

### V

video connector pinouts, 1

video formats, HD15, 1

video, Sun XVR-50, 1

voltage and current sensor status, displaying, 1

### W

web interface and ILOM, 1

Copyright © 2010, Oracle and/or its affiliates. All rights reserved.