A P P E N D I X A

Device Tree for the Sun Netra T6340 Server Module

The table shows the Solaris Operating System device tree for some server module devices.

Device Location on Server Module | Device Name in OpenBoot PROM | Solaris OS Device Tree
--- | --- | ---
On-board graphics chip. Output to external monitor via HD15 connector on dongle cable |
    screen
    /pci@500/pci@0/pci@2/pci@0/display@1
Remote mouse (rM) from JavaRConsole |
    mouse
    /pci@500/pci@0/pci@2/pci@0/usb@0/device@2/mouse@1
On-board graphics chip, output to remote screen (rV) on JavaRConsole |
    rscreen
    /pci@500/pci@0/pci@2/pci@0/display@1:r1024x768x75
Remote keyboard (rK) from JavaRConsole |
    rkeyboard
    /pci@500/pci@0/pci@2/pci@0/usb@0/device@2/keyboard@0
On-board graphics chip |
    display
    /pci@500/pci@0/pci@2/pci@0/display@1
On-board 1-Gbit ethernet port 1, routes to NEM 1 |
    net1
    /pci@400/pci@0/pci@2/network@0,1
On-board 1-Gbit ethernet port 0, routes to NEM 0 |
    net0
    /pci@400/pci@0/pci@2/network@0
On-board 1-Gbit ethernet port 0, routes to NEM 0, same as net0. |
    net
    /pci@400/pci@0/pci@2/network@0
Remote storage from JavaRConsole (rS) |
    cdrom
    /pci@500/pci@0/pci@2/pci@0/usb@0,2/storage@1/disk@0:f
HDD1, on-board disk1 |
    disk1
    /pci@500/pci@0/pci@9/@0/disk@1
HDD0, on-board disk0 |
    disk0
    /pci@500/pci@0/pci@9/@0/disk@0
On-board disk0, same as disk0 above |
    disk
    /pci@500/pci@0/pci@9/@0/disk@0
On-board SAS/SATA RAID 0/1 controller, the REM |
    scsi
    /pci@500/pci@0/pci@9/@0
Serial console port via RJ-45 connector on the dongle cable |
    virtual-console
    /vritual-devices/console@1
Fabric Expansion Module (FEM) |
    /pci@400/pci@0/pci@9
On-board USB 2.0 controller |
    None
    /pci@500/pci@0/pci@2/pci@0/usb@0,2
On-board USB 1.x controller |
    None
    /pci@500/pci@0/pci@2/pci@0/usb@0,1
On-board USB 1.x controller |
    None
    /pci@500/pci@0/pci@2/pci@0/usb@0

Copyright © 2010, Oracle and/or its affiliates. All rights reserved.