Exit Print View
#### Sun Integrated Lights Out Manager (ILOM) 3.0 Supplement for the Sun Netra T6340 Server Module |

| IPMI Sensor Reference |

### Sensors on the Sun Netra T6340 Server Module

IPMI Name | Full Path | Description
--- | --- | ---
`/SYS/SLOTID` | `/SYS/SLOTID` | Identifier of the slot where the blade is installed
`/MB/V_+V3_STBY` | `/SYS/MB/V_+V3_STBY` | 3.3V standby voltage threshold sensor
`/MB/V+1VO` | `/SYS/MB/V+1VO` | MB voltage sensor
`/MB/V+1V2` | `/SYS/MB/V+1V2` | MB voltage sensor
`/MB/V+1V5IO` | `/SYS/MB/V+5IO` | MB voltage sensor
`/MB/V+1V8` | `/SYS/MB/V+1V8` | MB voltage sensor
`/MB/V+3V3` | `/SYS/MB/V+3V3` | MB voltage sensor
`/MB/V+5V` | `/SYS/MB/V+5V` | MB voltage sensor
`/MB/V+12V` | `/SYS/MB/V+12V` | MB voltage sensor
`/MB/I+12V` | `/SYSS/MB/I+12V` | MB 12V current sensor, in Amps
`/SP/V_BAT` | `/SYS/SP/V_BAT` | Battery voltage threshold sensor
`/SYS/VPS` | `/SYS/VPS` | Real-time blade power consumption, in Watts
`/MB/V_VDDIO` | `/SYS/MB/V_DDIO` | I/O voltage threshold sensor
`/MB/CMPn/V_+1V1` | `/SYS/MB/CMPn/V_+1V1` | CMP (0-1) CPU core voltage sensor
`/MB/CMPn/V_+1V5` | `/SYS/MB/CMPn/V_+1V5` | CMP (0-1) CPU core voltage sensor
`/MB/CMPn/V_+1V8` | `/SYS/MB/CMPn/V_+1V8` | CMP (0-1) CPU core voltage sensor
`/MB/CMPn/I_+1V1` | `/SYS/MB/CMPn/I_+1V1` | CMP (0-1) CPU current draw sensor, in Amps
`/MB/CMPn/I_+1V5` | `/SYS/MB/CMPn/I_+1V5` | CMP (0-1) CPU current draw sensor, in Amps
`/MB/CMPn/I_+1V8` | `/SYS/MB/CMPn/I_+1V8` | CMP (0-1) CPU current draw sensor, in Amps
`/MB/CMPn/T_+1V1` | `/SYS/MB/CMPn/T_+1V1` | CMP (0-1) temperature sensor for voltage regulators, in degrees Celsius.
`/MB/CMPn/T_+1V5` | `/SYS/MB/CMPn/T_+1V8` | CMP (0-1) temperature sensor for voltage regulators, in degrees Celsius.
`/MB/CMPn/T_+1V8` | `/SYS/MB/CMPn/T_+1V8` | CMP (0-1) temperature sensor for voltage regulators, in degrees Celsius.
`/Pn/BRn/CHn/Dn/P` | `/SYS/MB/Pn/BRn/CHn/Dn/P` | CMP (0-1) DIMM presence sensors defined by branch BRn (where n= 0 or 1), channel CHn (where n= 0 or 1), and DIMM Dn (where n is an integer 0-3).
`/MB/Pn/CBUS_BTn` | `/SYS/MB/Pn/CBUS_BTn` | CMP (0-1) CPU corner bus test point, for point CBUS_BTn, where n is an integer 0-11.
`/MB/CMPn/T_IN` | `/SYS/MB/CMPn/T_IN` | CMP (0-1) temperature leading into the CPU, in degrees Celsius.
`/MB/CMPn/T_TCORE` | `/SYS/MB/CMPn/T_TCORE` | CMP (0-1) CPU temperature sensor at the top of the chip, in degrees Celsius.
`/MB/CMPn/T_BCORE` | `/SYS/MB/CMPn/T_BCORE` | CMP (0-1) CPU temperature sensor at the bottom of the chip, in degrees Celsius.
`/Pn/BRn/CHn/Dn/T_AMB` | `/SYS/MB/Pn/BRn/CHn/Dn/T_AMB` | CMP (0-1) temperature sensor (in degrees Celsius) defined by branch BRn (where n= 0 or 1), channel CHn (where n= 0 or 1), and DIMM Dn (where n is an integer 0-3).
`/HDDn/PRSNT` | `/SYS/HDDn/PRSNT` | Hard disk drive (0-1) presence sensors
`/NEMn/PRSNT` | `/SYS/NEMn/PRSNT` | Network Express Module (NEM) disk (0-1) presence sensors.
`/PSn/PRSNT` | `/SYS/PSn/PRSNT` | PS (0-1) chassis component sensors.
`/FMn/PRSNT` | `/SYS/FMn/PRSNT` | FM (0-5) chassis component sensors.
`/FMn/Fn/TACH` | `/SYS/FMn/Fn/TACH` | FM (0-5) tachometer (in RPM) for Fn, where n = 0 or 1.
`/FMn/SERVICE` | `/SYS/FMn/SERVICE` | FM (0-5) service sensor.
`/PSn/VINOKn` | `/SYS/PSn/VINOKn` | PS (0-1) sensor for `VINOKn`, where n = 0 or 1.
`/PSn/PWROKn` | `/SYS//PSn/PWROKn` | PS (0-1) sensor for `PWROKn`, where n = 0 or 1.
`/PSn/FANOK` | `/SYS/PSn/FANOK` | PS (0-1) fan OK sensor
`/PSn/TEMPOK` | `/SYS/PSn/TEMPOK` | PS (0-1) temperature OK sensor
`/PSn/V12VOK` n | `/SYS``/PSn/V12VOKn` | PS (0-1) OK sensor for `IV12VOKn`, where n = 0 or 1.
`/PSn/I12VOKn` | `/PSn/I12VOKn` | PS (0-1) OK sensor for `V12VOKn`, where n = 0 or 1.
`/MB/FEM/PRSNT` | `/SYS/MB/FEM/PRSNT` | FEM presence sensor.
`/MB/FEM/PRSNT` | `/SYS/MB/FEM/PRSNT` | REM presence sensor

Legal Copyright 1994-2010 Oracle and/or its affiliates. |