Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Use the ILOM Command-Line Interface to View the Sensor Readings

Before You Begin

To view sensor readings, you need the Read Only (o) role enabled.

1. Log in to the ILOM CLI.
2. Type the following commands to navigate to the sensor target and then to view the sensor properties:

   ->`cd target`

   ->`show`

   For example, on some server platforms, you can specify the following path to view a temperature reading of a server's ambient air intake:

   ->`cd /SYS/MB/T_AMB0`

   ->`show`

   The properties that describes the sensor target appear. For example:

       type = Temperature
               ipmi_name = MB/T_AMB0
               class = Threshold Sensor
               value = 39.000 degree C
               upper_nonrecov_threshold = 100.000 degree C
               upper_critical_threshold = 90.000 degree C
               upper_noncritical_threshold = 80.000 degree C
               lower_noncritical_threshold = N/A
               lower_critical_threshold = N/A
               lower_nonrecov_threshold = N/A
               alarm_status = cleared

3. To view a discrete sensor reading, type the following commands:

   ->`cd target`

   ->`show`

   The properties that describe the discrete sensor target appear.

   For example:

   - `Type = Entity Presence`

   - `Class = Discrete Indicator`

   - `Value = Present`

   For specific details about the type of discrete or threshold sensor targets you can access, as well as the paths to access them, see Sun ILOM 3.0 Supplement for the Sun Fire X4640 Server.

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |