Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Service Manual Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Install the Fan Tray

1. Prepare the server for service. See How to Prepare the Server for Service.
2. Align the fan tray with the bay in the chassis.

   The connector at the bottom of the fan tray should be on the left (as you face the server front) to align with the connector on the motherboard.

3. Lower the fan tray into the bay until it comes into contact with the connector on the motherboard.
4. Push down gently until the connector is fully engaged and the plastic securing buttons snap into place.
5. Prepare the server for operation. See How to Prepare the Server for Operation.

See Also

- Fan Tray Designations

- How to Remove the Fan Tray

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |