Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Diagnostics Guide Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

### Viewing the ILOM Sensor Readings

There are three ambient temperature sensors that are monitored. Each CPU board has two temperature sensors. Ambient temperature sensors and core temperature sensors on CPU boards are fed to IPMI stack to adjust fan speed. View the sensor information in Sun ILOM 3.0 Supplement for the Sun Fire X4640 Server for more information about the sensors.

This section contains the following procedures:

- How to Use the ILOM Web Interface to View the Sensor Readings

- How to Use the ILOM Command-Line Interface to View the Sensor Readings

Copyright © 2009, 2010, Oracle and/or its affiliates. All rights reserved. Legal Notices |