Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

##### Tools and Staff Required

| Caution - To avoid serious personal injury and equipment damage, always use all four chassis handles to support the product weight when handling or moving the product.

| Caution - The server weighs about 88 pounds (40 kg) when fully loaded with components. To reduce the risk of serious personal injury or equipment damage, use a mechanical lift to install the server into the rack. If a lift is not available, remove components as described in How to Remove Components to Reduce Weight. This reduces the weight of the server to 35 pounds (16 kg).

| Caution - Always load equipment into a rack from the bottom up so that it does not become top-heavy and tip over. Deploy your rack’s anti-tilt bar to prevent the rack from tipping during equipment installation.

Before installing the server into a rack, gather the tools, equipment, and staff required.

Tools, Equipment, and Staffing Required | Notes
--- | ---
Two trained staff | Two people are needed to install the server and operate the lift.
#2 10–inch Phillips screwdriver (magnetic tip recommended) | Optional. Required if you are hardmounting the server.
Mechanical lift | Strongly recommended. If not available, reduce the weight of the server. See How to Remove Components to Reduce Weight.
Compatible rack | See Compatible Racks.
Slide rails | Optional. See Slide Rail Kit.
Cable management arm | Optional. See Installing the Cable Management Arm (CMA).

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |