Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Service Manual Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Remove DIMMs

1. Prepare the server for service. See How to Prepare the Server for Service.
2. Remove the CPU module that contains the DIMM you want to remove. See How to Remove a CPU Module or Filler Card.
3. Set the CPU module on an anti-static surface.

   Tip - Use an antistatic mat. See How to Use an Antistatic Mat.

4. Use the CPU module's DIMM diagnostics to locate the DIMM that you want to remove from the CPU module.
5. To remove the DIMM, rotate both DIMM slot locking handles outward as far as they will go.

   This action partially ejects the DIMM from the socket.

6. Carefully lift the DIMM straight up to remove it from the socket.

See Also

- How to Install DIMMs

- CPU Module Features and Components

- DIMM Population Rules

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |