Skip Navigation Links
Exit Print View
| Sun Installation Assistant 2.2 User's Guide for the Sun Fire X4640 Server Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## To Establish Connection Using a VNC Viewer

Follow these steps to establish a connection using a VNC viewer.

1. Set a password as shown in Set Up Passwords for Root and Virtual Access.
2. Press the Esc key shortly after the SIA splash screen appears.

   Console messages appear. After the VNC server has started, a message appears providing the IP address to connect using VNC.

3. Connect to the VNC viewer using the IP address displayed in Step 2.

   For example:

   `# vncviewer IP_address:1.0`

4. When prompted, enter the password that you set in Step 1 and VNC starts.

   The installer interface appears when performing a manual installation. The screens automatically move forward as the installation progresses. The VNC screens are active for input and you will disrupt the installation if you do anything in the VNC window.

Copyright © 2009, 2010, Oracle and/or its affiliates. All rights reserved. Legal Notices |