Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Replace the Battery

If you are clearing the battery-backed CMOS-based BIOS settings, remove the battery for approximately 30 seconds and then install the battery.

Before You Begin

- Battery type: CR2032

1. Prepare the server for service. See How to Prepare the Server for Service.
2. Remove the battery by gently pulling the spring-clip away from the battery face and lifting the battery straight up.
3. To install the new battery, align the battery with the holder on the motherboard so that the positive (+) side of the battery is facing toward the center of the chassis.
4. Press the battery down fully into the holder until the spring clip snaps around the battery.
5. Prepare the server for operation. See How to Prepare the Server for Operation.

Next Steps

Access the system BIOS to customize the server settings. See Configuring the System Using the BIOS Setup Utilities.

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |