Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Notes Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

### Mixing DIMMs Impacts Memory Performance

For optimum performance, all DIMMs controlled by a given CPU should be the same capacity and all single-rank or dual-rank. Mixed configurations are supported, but could result in lower memory performance. Note that all supported 4 GB and 8 GB DIMMs are dual-rank.

Copyright © 2009, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |