Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

##### Identifying Correctable DIMM Errors (CEs)

CEs rarely occur, therefore during a short POST, the BIOS might not be able to catch a CE to log it in the server's IPMI SEL (system event logs). Memory Correctable Errors are usually reported and handled by the supporting operating systems. See the following procedures for more information:

- How to Identify CEs on a Solaris Server

- How to Identify CEs on a Linux Server

- How to Identify CEs on a Windows Server

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |