Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Service Manual Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Remove the Service Processor Board

Before You Begin

- If you are replacing an SP board that is not dead, obtain the ILOM version and download the system software release package (combined BIOS/ILOM) that incorporates that version. A system software release package can be downloaded from: http://support.oracle.com.

- If you are replacing a dead SP board, obtain the BIOS version and download the system software release package (combined BIOS/ILOM) that incorporates that version. A system software release package can be downloaded from: http://support.oracle.com.

1. Prepare the server for service. See How to Prepare the Server for Service.
2. Pinch the tabs on the white plastic standoff post that is closest to the back panel of the server and simultaneously lift the rear edge the of service processor (SP) board to free it from that rear standoff post and the connector on the motherboard.
3. With the rear edge free, pivot the SP board so that it clears the plastic retainer that is attached to the motherboard handle.
4. Pinch the tabs on the white plastic standoff post that is closest to the front panel of the server, and simultaneously lift the front edge the of SP board to free it from that front standoff post.

   Note - Do not bend the SP board while removing it or installing it.

See Also

- How to Install the Service Processor Board

- Identifying Components

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |