Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Service Manual Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Install the Fan Tray Carriage

Before You Begin

- You need a torque screwdriver to tighten the screws to correct specification.

1. Lower the fan tray carriage into the chassis until it is seated firmly against the motherboard and the top of the chassis.

   There are two alignment pins on the motherboard that match the holes on the bottom of the fan tray carriage.

2. Tighten the seven captive screws that secure the fan tray carriage to the chassis and the motherboard.

   Torque the screws to 7 inch-pounds.

3. Secure the fan tray carriage to the top of the chassis using the nine screws.

   Torque the screws to 7 inch-pounds.

4. Install the fan trays. See How to Install the Fan Tray.

See Also

- How to Remove the Fan Tray Carriage

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |