Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Update the LSI Firmware Using the Remote Console Method

1. Connect to the ILOM Remote Console, according to the instructions in How to Connect Remotely Using the ILOM Web Interface.
2. In the remote console window, select Devices.
3. At the pop-up screen, select the CD-ROM Image.

   A check mark is displayed on the drop-down menu selection.

4. Browse to the LSI firmware update image .iso file, and select the correct .iso image file.
5. Select Remote Control -> Remote Power Control in the ILOM GUI.
6. Select Reset from the drop-down menu.
7. When the system reboots, select 1 (Perform the Update) from the remote console window.

   The update proceeds.

   When complete, the console responds with a new prompt.

8. In the remote console window, select Devices -> CDROM Image to detach the LSI firmware update .iso file.
9. Select Keyboard -> Control Alt Delete.

   The system boots, and the new LSI firmware version is displayed in the boot messages.

   You will notice the new LSI firmware version.

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |