Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Update the LSI Firmware Using the Local Method

1. Download the LSI firmware .iso file from the Sun Fire X64 servers web site and burn it to a bootable CD.

   Note - The bootable CD appear blanks when viewed using the operating system. This is expected behavior.

2. Insert the bootable CD and reboot the server.

   The firmware is upgraded.

3. Reboot the system.

   The new LSI firmware version is displayed in the boot messages.

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |