Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Install a PCI Card

1. Prepare the server for service. See How to Prepare the Server for Service.
2. Working from the rear of the chassis, pivot the PCI card latch to the open position.
3. Insert the PCI card into the PCI card slot. Ensure that the PCI card’s rear connector panel engages the tab in the chassis rear panel.
4. Pivot the PCI card latch to the closed position until it locks.
5. Prepare the server for operation. See How to Prepare the Server for Operation.

See Also

- How to Remove a PCI Card

- Identifying Components

- Boot Device Detection and Priority

- PCI Slot Designations

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |