Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

##### Error Messages Are Displayed With Solaris 10 5/09 and Sun Dual 10GbE XFP 2 SR PCI Express Card (6804557)

The following message might be displayed when doing a stress test on Sun Dual 10GbE XFP 2 SR PCI Express card (X1107A-Z) on a system running Solaris 10 5/09:

    fmd: [ID 441519 daemon.error] SUNW-MSG-ID: SUNOS-8000-FU, TYPE: Defect, VER: 1, SEVERITY: Major
    EVENT-TIME: Thu Aug 20 14:30:18 PDT 2009
    PLATFORM: Sun Fire X4640   , CSN: 002555               , HOSTNAME: nsgbj-phoenix01
    SOURCE: eft, REV: 1.16
    EVENT-ID: b94dd051-aecb-c0d3-ed0f-aec3fe312222
    DESC: The diagnosis engine encountered telemetry for which it was unable to perform a diagnosis.
    Refer to http://sun.com/msg/SUNOS-8000-FU for more information.
    AUTO-RESPONSE: Error reports have been logged for examination by Sun.
    IMPACT: Automated diagnosis and response for these events will not occur.
    REC-ACTION: Ensure that the latest Solaris Kernel and Predictive Self-Healing (PSH) patches are installed.

These messages can be safely ignored.

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |